IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 7ba92475-4af4-4fbf-b376-f387dcf6b5d7, NumberOfSaves: 1]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates]"
File name: "084_CQC"
Time stamp: "2023-11-07T16:26:38+01:00"
Preprocessor: "ODA SDAI 24.3"
Originating system: "Autodesk Revit 24.1.0.66 (ENG) - IFC 24.2.0.49"
Application: "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)"

People and organizations
  Person "meray.nassimos" of Organization (no name given)
  Owner history of Person "meray.nassimos" of Organization (no name given) | application "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)" | change NOCHANGE | created 1692282453 (2023-08-17T14:27:33Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "084_CQC" | long name "DOCKin - QUAI CHARLEROI" | phase "Permis d'urbanisme"
  IFCSITE "Default" | latitude 48° 52′ 0″ | longitude 2° 20′ 0″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Quai Arthur Rimbaud, 66000 Charleroi", "Défini par l'utilisateur"
      IFCBUILDINGSTOREY "FFL-B1" | long name "FFL-B1" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation -368.
        contains 232 elements
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:2407560", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3228145", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6874283" (+21 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:2408949" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/111 - Panneau 211/103" | object type "RA325_001:GO 215/111 - Panneau 211/103" | names: "RA325_001:GO 215/111 - Panneau 211/103:2409035" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:2409059", "RA325_001:GO 215/91 - Panneau 211/83:6874719" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:2409165", "RA325_001:GO 215/101 - Panneau 211/93 - EI30:3276467", "RA325_001:GO 215/101 - Panneau 211/93 - EI30:3499513" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm:2409566", "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm:7493488" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:2409628", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:2409688", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:2409777" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:2410264", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:2410422", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:2410491" (+13 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          10 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:2410896", "RA325_081_Menuiserie:Panneau 211/73:3227903", "RA325_081_Menuiserie:Panneau 211/73:3227911" (+7 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:2448277", "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4229582" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          8 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:2712335", "RA325_081_Menuiserie:Panneau 211/73:3228067", "RA325_081_Menuiserie:Panneau 211/73:3228075" (+5 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:3061454" | parts: 2 IFCRAILING, 2 IFCSLAB, 2 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_101:GO 215/195 - Panneau 211/2x113 - EI30" | object type "RA325_101:GO 215/195 - Panneau 211/2x113 - EI30" | names: "RA325_101:GO 215/195 - Panneau 211/2x113 - EI30:3143287" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:3228196" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:3395845" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | HALF_TURN_STAIR | names: "Precast Stair:Stair:4014679" | parts: 2 IFCSTAIRFLIGHT, 1 IFCRAILING, 1 IFCSLAB | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4014754", "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4025127" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30:4024486" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4230325" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241753", "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241755" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241756" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sous-sol 2 - 140mm" | object type "Floor:RA239_Finition - Sous-sol 2 - 140mm" | FLOOR | names: "Floor:RA239_Finition - Sous-sol 2 - 140mm:4264940", "Floor:RA239_Finition - Sous-sol 2 - 140mm:6865569" | material: layers "Floor:RA239_Finition - Sous-sol 2 - 140mm" ("M-430_01 - Sol Finition Gén Type 2" 1.5, "M-431_01 - Chape Type 1" 9.5, "M-239_01 - Isolation Sol Int - Type 1" 3., "M-431_01 - Natte drainante - Type 1" 3.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm:4344133", "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm:4344167", "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm:4344186" (+3 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-219_610 - Isolation résistant à l'humidité - 60mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:5867940", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5868010", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5868101" (+25 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/113 - EI30 2" | object type "RA325_001:GO 215/101 - Panneau 211/113 - EI30 2" | names: "RA325_001:GO 215/101 - Panneau 211/113 - EI30 2:6334040" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm:6861984" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-219_610 - Isolation résistant à l'humidité - 60mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sous-sol - 110mm" | object type "Floor:RA239_Finition - Sous-sol - 110mm" | FLOOR | names: "Floor:RA239_Finition - Sous-sol - 110mm:6864109" | material: materials ("M-431_01 - Chape Type 1", "M-431_01 - Natte drainante - Type 1") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:6874632" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7194085" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7194087", "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7494290", "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7494310" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194089" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7216074" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/63" | object type "RA325_081_Menuiserie:Panneau 211/63" | names: "RA325_081_Menuiserie:Panneau 211/63:7494362" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2:7515173", "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2:7515505", "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2:7515550" (+1 more) | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2" ("M-353_03 - Faux-Plafond - Type 3" 9.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCGRID | names: "Default Grid"
          1 x IFCWALL | type IFCWALLTYPE "Walls 3:Walls 3" | object type "Walls 3:Walls 3" | names: "Walls 3:Walls 3:2787081" | material: "M-000_Béton, coulé sur place" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Windows 1:Windows 1" | object type "Windows 1:Windows 1" | names: "Windows 1:Windows 1:7130245" | material: "A-000_Poche" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:2217558", "Basic Wall:RA2xx_ isolant - Mitoyen:2803641", "Basic Wall:RA2xx_ isolant - Mitoyen:3777469" (+3 more) | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462105" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462154" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462205" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462254" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462311" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2462362" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2614671" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2614741" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:2691492", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3007406", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3217322" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:2772768", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3217165", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3828842" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871115" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871130" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871149" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871164" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871280" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871295" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871310" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871327" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871342" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871359" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871376" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:350 x 700mm" | object type "RA232_Stru - Colonne rectangulaire:350 x 700mm" | names: "RA232_Stru - Colonne rectangulaire:350 x 700mm:2871460" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871541" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:350 x 700mm" | object type "RA232_Stru - Colonne rectangulaire:350 x 700mm" | names: "RA232_Stru - Colonne rectangulaire:350 x 700mm:2871556" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:2871571" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          3 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3008688", "Floor:RA232_Stru - Béton générique - 200mm:3133709", "Floor:RA232_Stru - Béton générique - 200mm:6300458" | material: "M-280_02 - Beton Arme"; layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | object type "RA232_Stru - Colonne carrée:700 x 700mm" | names: "RA232_Stru - Colonne carrée:700 x 700mm:3011503" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | object type "RA232_Stru - Colonne carrée:600 x 600mm" | names: "RA232_Stru - Colonne carrée:600 x 600mm:3011509" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:3039679" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:3039768" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | object type "RA232_Stru - Colonne carrée:350 x 350mm" | names: "RA232_Stru - Colonne carrée:350 x 350mm:3039890" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:700 x 700mm" | object type "RA232_Stru - Poutre rectangulaire:700 x 700mm" | names: "RA232_Stru - Poutre rectangulaire:700 x 700mm:3040539" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:3040541" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:3227339", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:3441198", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:7115392" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" ("M-220_01 - Maconnerie interieure - Type 1" 19.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:3227340", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:6230069", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm:6301251" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" ("M-220_01 - Maconnerie interieure - Type 1" 19.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:3395172", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7192569" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3439275" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" | object type "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" | names: "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm:3909044" | material: layers "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" ("M-280_02 - Beton Arme" 10., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:4233932", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:4251698", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:4251928" (+4 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:4234152" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:4256838" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:5972839", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7032668", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7035817" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Beton Arme - 200mm" | object type "Basic Wall:RA280 - Stru - Beton Arme - 200mm" | names: "Basic Wall:RA280 - Stru - Beton Arme - 200mm:6307132" | material: layers "Basic Wall:RA280 - Stru - Beton Arme - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 660mm" | object type "Floor:RA232_Stru - Béton générique - 660mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 660mm:7052803", "Floor:RA232_Stru - Béton générique - 660mm:7062193" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:7061500" | material: layers "Floor:RA232_Stru - Béton générique - 260 mm" ("M-280_02 - Beton Arme" 26.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 800mm" | object type "Floor:RA232_Stru - Béton générique - 800mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 800mm:7096438" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 500mm" | object type "Floor:RA232_Stru - Béton générique - 500mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 500mm:7096722", "Floor:RA232_Stru - Béton générique - 500mm:7256866" | material: "M-280_02 - Beton Arme"; layers "Floor:RA232_Stru - Béton générique - 500mm" ("M-280_02 - Beton Arme" 50.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm:7113749" | material: layers "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm" ("M-220_11 - Maconnerie interieure Portante - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7113934" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 860mm" | object type "Floor:RA232_Stru - Béton générique - 860mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 860mm:7129776" | material: layers "Floor:RA232_Stru - Béton générique - 860mm" ("M-280_02 - Beton Arme" 86.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 350mm" | object type "Floor:RA232_Stru - Béton générique - 350mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 350mm:7263865" | material: layers "Floor:RA232_Stru - Béton générique - 350mm" ("M-280_02 - Beton Arme" 35.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 250mm" | object type "Floor:RA232_Stru - Béton générique - 250mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 250mm:7264157", "Floor:RA232_Stru - Béton générique - 250mm:7615715" | material: layers "Floor:RA232_Stru - Béton générique - 250mm" ("M-280_02 - Beton Arme" 25.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7265979", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459941", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7707918" (+3 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 140mm" | object type "Floor:RA232_Stru - Béton générique - 140mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 140mm:7290546" | material: layers "Floor:RA232_Stru - Béton générique - 140mm" ("M-280_02 - Beton Arme" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1200mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1200mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1200mm:7703514" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 820mm" | object type "Floor:RA232_Stru - Béton générique - 820mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 820mm:7716958" | material: layers "Floor:RA232_Stru - Béton générique - 820mm" ("M-280_02 - Beton Arme" 82.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
        IFCSPACE "01-023" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5859148" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7449595" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "01-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "01-012" | long name "WC/DOUCHE PMR" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5859140" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "01-018" | long name "-" | INTERNAL
        IFCSPACE "01-003" | long name "CABINE HT" | INTERNAL
        IFCSPACE "01-006" | long name "ESC. 1" | INTERNAL
        IFCSPACE "01-028" | long name "T1" | INTERNAL
        IFCSPACE "01-019" | long name "-" | INTERNAL
        IFCSPACE "01-020" | long name "-" | INTERNAL
        IFCSPACE "01-011" | long name "LOCAL VELOS 2" | INTERNAL
        IFCSPACE "01-029" | long name "T2" | INTERNAL
        IFCSPACE "01-026" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5859130" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7449544" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "01-009" | long name "LOCAL TECHNIQUE" | INTERNAL
          contains 4 elements
            4 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Heracklith" | object type "Compound Ceiling:Heracklith" | CEILING | names: "Compound Ceiling:Heracklith:7514653", "Compound Ceiling:Heracklith:7514860", "Compound Ceiling:Heracklith:7514976" (+1 more) | material: layers "Compound Ceiling:Heracklith" ("M-353_03 - Faux-Plafond - Type 3" 9.5) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "01-025" | long name "DOUCHES FEMMES" | INTERNAL
          contains 6 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6882798" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            4 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "F 83_005b1:F 83_005b 2" | object type "F 83_005b1:F 83_005b 2" | names: "F 83_005b1:F 83_005b 2:7446467", "F 83_005b1:F 83_005b 2:7446520", "F 83_005b1:F 83_005b 2:7446536" (+1 more) | material: "Matériau du rendu 255-255-255" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7449465" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "01-004" | long name "CITERNE" | INTERNAL
        IFCSPACE "01-010" | long name "LOCAL VELOS 1" | INTERNAL
        IFCSPACE "01-005" | long name "CUISINE DE RECHAUFFE" | INTERNAL
        IFCSPACE "01-014" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "01-015" | long name "LOCAL TECHNIQUE" | INTERNAL
        IFCSPACE "01-016" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "01-017" | long name "LOCKERS" | INTERNAL
        IFCSPACE "01-013" | long name "RACK DATA" | INTERNAL
        IFCSPACE "01-007" | long name "ESC. 1" | INTERNAL
        IFCSPACE "01-021" | long name "-" | INTERNAL
        IFCSPACE "01-022" | long name "T3" | INTERNAL
        IFCSPACE "01-027" | long name "STOCKAGE MATERIEL" | INTERNAL
        IFCSPACE "01-024" | long name "DOUCHES HOMMES" | INTERNAL
          contains 6 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6882535" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            4 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "F 83_005b1:F 83_005b 2" | object type "F 83_005b1:F 83_005b 2" | names: "F 83_005b1:F 83_005b 2:7446277", "F 83_005b1:F 83_005b 2:7446519", "F 83_005b1:F 83_005b 2:7446535" (+1 more) | material: "Matériau du rendu 255-255-255" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7448511" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "01-001" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6882477" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-036" | long name "LOCAL TECHNIQUE 1" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Heracklith" | object type "Compound Ceiling:Heracklith" | CEILING | names: "Compound Ceiling:Heracklith:7514180", "Compound Ceiling:Heracklith:7514442" | material: layers "Compound Ceiling:Heracklith" ("M-353_03 - Faux-Plafond - Type 3" 9.5) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "FFL-GN" | long name "FFL-GN" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 10.
        contains 403 elements
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" | object type "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" | names: "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm:2217368", "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm:3145223" | material: layers "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" ("M-280_02 - Beton Arme" 10., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm" | object type "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm" | names: "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm:2218863", "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm:2219871", "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm:2490771" (+1 more) | parts: 194 IFCMEMBER, 14 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 300mm" | object type "Floor:RA232_Stru - Béton générique - 300mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 300mm:2224850", "Floor:RA232_Stru - Béton générique - 300mm:6864501" | material: layers "Floor:RA232_Stru - Béton générique - 300mm" ("M-280_02 - Beton Arme" 30.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          6 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Standard" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Standard" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Standard:2396854", "Curtain Wall:RA213 - CW_Cloison vitrée - Standard:2764738", "Curtain Wall:RA213 - CW_Cloison vitrée - Standard:3142131" (+3 more) | parts: 23 IFCMEMBER, 5 IFCPLATE, 1 IFCCURTAINWALL | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          9 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:171_CW_Secant Piled Wall 530mm" | object type "Curtain Wall:171_CW_Secant Piled Wall 530mm" | names: "Curtain Wall:171_CW_Secant Piled Wall 530mm:2406872", "Curtain Wall:171_CW_Secant Piled Wall 530mm:2406876", "Curtain Wall:171_CW_Secant Piled Wall 530mm:2656404" (+6 more) | parts: 304 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" | object type "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" | names: "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:2408599", "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:2485614", "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:2879406" (+3 more) | material: layers "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" ("M-220_11 - Maconnerie interieure Portante - Type 1" 19.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:2418414" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:2447830", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3746073", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7114246" (+1 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" | object type "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" | names: "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:2485802", "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:3945340", "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm:3945794" (+1 more) | material: layers "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" ("M-220_11 - Maconnerie interieure Portante - Type 1" 19.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          19 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:2553186", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:3007407", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:3217257" (+16 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:2553776" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          51 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:2556322", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:2680948", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3035220" (+48 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Cast-In-Place Stair:A-245_Escalier_Int - Béton_Escalier monobloc" | object type "Cast-In-Place Stair:A-245_Escalier_Int - Béton_Escalier monobloc" | STRAIGHT_RUN_STAIR | names: "Cast-In-Place Stair:Stair:2695834" | parts: 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:2708542", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:2772775", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:2772776" (+9 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Beton Arme - 250mm" | object type "Basic Wall:RA280 - Stru - Beton Arme - 250mm" | names: "Basic Wall:RA280 - Stru - Beton Arme - 250mm:2768064", "Basic Wall:RA280 - Stru - Beton Arme - 250mm:2768171", "Basic Wall:RA280 - Stru - Beton Arme - 250mm:2768243" (+8 more) | material: layers "Basic Wall:RA280 - Stru - Beton Arme - 250mm" ("M-280_02 - Beton Arme" 25.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm:2885176", "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm:2885222", "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm:2885414" (+1 more) | material: layers "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm" ("M-280_02 - Beton Arme" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | object type "RA232_Stru - Colonne carrée:700 x 700mm" | names: "RA232_Stru - Colonne carrée:700 x 700mm:3012719" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3035214", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7705575" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:3060269" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:3060421", "Precast Stair:Stair:6329951" | parts: 7 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3217809", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:4240583", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632060" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:3217811" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | object type "RA232_Stru - Colonne carrée:600 x 600mm" | names: "RA232_Stru - Colonne carrée:600 x 600mm:3276483" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:3360771", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:5845274" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_101:GO 205/155 - Panneau 201/2x83 - EI30" | object type "RA325_101:GO 205/155 - Panneau 201/2x83 - EI30" | names: "RA325_101:GO 205/155 - Panneau 201/2x83 - EI30:3360772" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:3395173" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:3439274" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3456848", "RA319_Glass Ext:Type 1:3999254" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:M-419_01 - Couvre-murs - Type 1" | object type "Basic Wall:M-419_01 - Couvre-murs - Type 1" | names: "Basic Wall:M-419_01 - Couvre-murs - Type 1:3674508" | material: layers "Basic Wall:M-419_01 - Couvre-murs - Type 1" ("M-419_01 - Couvre-murs - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:M-340_Railing - Teinte gris clair" | object type "Basic Wall:M-340_Railing - Teinte gris clair" | names: "Basic Wall:M-340_Railing - Teinte gris clair:3675635" | material: layers "Basic Wall:M-340_Railing - Teinte gris clair" ("M-340_Railing - Teinte gris clair" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:M-214_01 - Mur rideau - Type 1" | object type "Basic Wall:M-214_01 - Mur rideau - Type 1" | names: "Basic Wall:M-214_01 - Mur rideau - Type 1:3675741" | material: layers "Basic Wall:M-214_01 - Mur rideau - Type 1" ("M-214_01 - Mur rideau - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_001:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_001:GO 215/131 - Panneau 211/123 - EI30:4018414" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:4019852" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | object type "Floor:RA239_Finition - Sol Rez - 200 mm" | FLOOR | names: "Floor:RA239_Finition - Sol Rez - 200 mm:4233273" | parts: 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sol Rez - 200 mm" | object type "Floor:RA239_Finition - Sol Rez - 200 mm" | FLOOR | names: "Floor:RA239_Finition - Sol Rez - 200 mm:4271742", "Floor:RA239_Finition - Sol Rez - 200 mm:5879002", "Floor:RA239_Finition - Sol Rez - 200 mm:6310713" (+1 more) | material: layers "Floor:RA239_Finition - Sol Rez - 200 mm" ("M-431_01 - Chape Type 2 - 8cm" 8., "M-431_01 - Insulit BI+9 - Type 1" 1., "M-431_01 - Chape Type 1 - 6cm" 6., "M-239_01 - Isolation Sol Int - Type 1" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033562" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033700" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:7090900" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7095618" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 600mm" | object type "Floor:RA232_Stru - Béton générique - 600mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 600mm:7112269" | material: layers "Floor:RA232_Stru - Béton générique - 600mm" ("M-280_02 - Beton Arme" 60.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 500mm" | object type "Floor:RA232_Stru - Béton générique - 500mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 500mm:7129243" | material: layers "Floor:RA232_Stru - Béton générique - 500mm" ("M-280_02 - Beton Arme" 50.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 1000mm" | object type "Floor:RA232_Stru - Béton générique - 1000mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 1000mm:7129719" | material: layers "Floor:RA232_Stru - Béton générique - 1000mm" ("M-280_02 - Beton Arme" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192092" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192265" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7194086" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7207360" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 430mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 430mm:7459653" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7506234" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7506556" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7506648" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7506746" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7506850" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | object type "M_Footing-Rectangular:1000 x 1000 x 600mm" | names: "M_Footing-Rectangular:1000 x 1000 x 600mm:7507120" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          2 x IFCFOOTING | type IFCTYPEPRODUCT "Foundation Slab:Radier 1000mm" | object type "Foundation Slab:Radier 1000mm" | names: "Foundation Slab:Radier 1000mm:7507134", "Foundation Slab:Radier 1000mm:7508416" | material: layers "Foundation Slab:Radier 1000mm" ("M-280_02 - Beton Arme" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          2 x IFCFOOTING | type IFCTYPEPRODUCT "Foundation Slab:Radier 1590mm" | object type "Foundation Slab:Radier 1590mm" | names: "Foundation Slab:Radier 1590mm:7507783", "Foundation Slab:Radier 1590mm:7508492" | material: layers "Foundation Slab:Radier 1590mm" ("M-280_02 - Beton Arme" 159.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "Foundation Slab:Radier 1500mm" | object type "Foundation Slab:Radier 1500mm" | names: "Foundation Slab:Radier 1500mm:7507861" | material: layers "Foundation Slab:Radier 1500mm" ("M-280_02 - Beton Arme" 150.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:500mm Diameter" | object type "M_Pile-Steel Pipe:500mm Diameter" | names: "M_Pile-Steel Pipe:500mm Diameter:7509547" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7509869" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7509918" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7509959" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7509987" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7509996" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510013" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510082" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510102" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510119" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510136" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510153" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510174" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510204" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510240" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510257" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510274" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510291" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510308" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510333" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510343" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510352" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510362" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510371" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510382" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510391" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510408" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510425" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510442" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510461" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510478" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510495" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510522" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510539" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510556" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510571" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510597" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510614" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510631" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510648" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510665" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510690" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510733" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510750" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | names: "M_Pile-Steel Pipe:600mm Diameter:7510767" | material: "Steel, 45-345" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          3 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Empierrement - 300mm" | object type "Floor:RA232_Stru - Empierrement - 300mm" | FLOOR | names: "Floor:RA232_Stru - Empierrement - 300mm:7513435", "Floor:RA232_Stru - Empierrement - 300mm:7513435:2", "Floor:RA232_Stru - Empierrement - 300mm:7513562" | material: layers "Floor:RA232_Stru - Empierrement - 300mm" ("M-940 - Site - Empierrement" 30.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7536490", "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7538404", "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7540273" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | object type "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | names: "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7552905" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | object type "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | names: "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7553261" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          38 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7572881", "RA319_Glass Ext:Type 1:7572883", "RA319_Glass Ext:Type 1:7572884" (+35 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7572893" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7572899" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7574304", "RA319_Glass Ext:Type 1:7579077", "RA319_Glass Ext:Type 1:7582206" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7574310" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7578011", "RA319_Glass Ext:Type 1:7578018" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7578088" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7578094" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7578100" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7578385", "RA319_Glass Ext:Type 1:7578386" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:7581968", "Curtain Wall:RA313 - Window_Gris Clair:7589051", "Curtain Wall:RA313 - Window_Gris Clair:7639391" | parts: 5 IFCMEMBER, 2 IFCDOOR, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7581970", "RA319_Glass Ext:Type 1:7581971" | material: "M-316_04 - Panneautage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7582174" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7589053", "RA319_Glass Ext:Type 1:7589054" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7589243" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:7589266" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 430mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 430mm:7706390" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 430mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 430mm:7709522" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCGRID | names: "Default Grid"
          30 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2215938", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2575527", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2595331" (+27 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 4:Generic Models 1" | object type "Generic Models 4:Generic Models 1" | names: "Generic Models 4:Generic Models 1:2592601" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2642191", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2958736", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2962259" (+1 more) | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:2642196", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:3514607" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Arial 600 mm" | object type "Model Text:Arial 600 mm" | names: "Model Text:Arial 600 mm:3498644", "Model Text:Arial 600 mm:3693146" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:2214152", "Floor:RA232_Stru - Béton générique - 200mm:7265004", "Floor:RA232_Stru - Béton générique - 200mm:7543639" | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          19 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2437538", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2437970", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2438288" (+16 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2438050", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2494463", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5884403" (+2 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2642194", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2642198", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3808727" (+1 more) | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:2917495" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 320mm" | object type "Floor:RA232_Stru - Béton générique - 320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 320mm:2918114", "Floor:RA232_Stru - Béton générique - 320mm:4258973" | material: "M-280_02 - Beton Arme"; layers "Floor:RA232_Stru - Béton générique - 320mm" ("M-280_02 - Beton Arme" 32.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3012548", "RA232_Stru - Poutre rectangulaire:270 x 500mm:3037642" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | object type "RA232_Stru - Colonne carrée:700 x 700mm" | names: "RA232_Stru - Colonne carrée:700 x 700mm:3039961" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | object type "RA232_Stru - Colonne carrée:600 x 600mm" | names: "RA232_Stru - Colonne carrée:600 x 600mm:3039963" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4253163" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:4259110", "Floor:RA232_Stru - Béton générique - 260 mm:5829425", "Floor:RA232_Stru - Béton générique - 260 mm:7061370" | material: layers "Floor:RA232_Stru - Béton générique - 260 mm" ("M-280_02 - Beton Arme" 26.); "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 940mm" | object type "RA232_Stru - Poutre rectangulaire:350 x 940mm" | names: "RA232_Stru - Poutre rectangulaire:350 x 940mm:6179979", "RA232_Stru - Poutre rectangulaire:350 x 940mm:6180472", "RA232_Stru - Poutre rectangulaire:350 x 940mm:6180578" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:6920633" | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6944626", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7697943", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7704411" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7114356" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | object type "RA232_Stru - Poutre rectangulaire:400 x720mm" | names: "RA232_Stru - Poutre rectangulaire:400 x720mm:7135823" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 520mm:7258699" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7259747" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 720mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 720mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 720mm:7543781" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634217" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "00-012" | long name "T1" | INTERNAL
        IFCSPACE "00-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "00-020" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7740084" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "00-005" | long name "ESC. 1" | INTERNAL
        IFCSPACE "00-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "00-003" | long name "BUREAU DE GESTION" | INTERNAL
        IFCSPACE "00-019" | long name "SALLE D'ENREGISTREMENT" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7539850" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "00-022" | long name "SAS ENTREE" | INTERNAL
        IFCSPACE "00-008" | long name "HALL ENTREE" | INTERNAL
        IFCSPACE "00-013" | long name "T2" | INTERNAL
        IFCSPACE "00-010" | long name "Local poubelles" | INTERNAL
        IFCSPACE "00-004" | long name "CAFETERIA" | INTERNAL
        IFCSPACE "00-009" | long name "KITCHENETTE" | INTERNAL
        IFCSPACE "00-007" | long name "ESPACE COWORKING" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7205995" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "00-023" | long name "-" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:3395171" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7538798" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "00-011" | long name "LOCAL ENTRETIENT" | INTERNAL
        IFCSPACE "00-006" | long name "ESC. 2" | INTERNAL
        IFCSPACE "00-021" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7740182" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "00-014" | long name "T5" | INTERNAL
        IFCSPACE "00-016" | long name "-" | INTERNAL
        IFCSPACE "00-017" | long name "T4" | INTERNAL
        IFCSPACE "00-018" | long name "T3" | INTERNAL
        IFCSPACE "60-038" | long name "SALLE D'ENREGISTREMENT" | INTERNAL
        IFCSPACE "60-039" | long name "LOCAL STOCKAGE" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm:7540829" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" ("M-000_Panneau de plafond 600 x 600" 10.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-040" | long name "LOCAL STOCKAGE" | INTERNAL
      IFCBUILDINGSTOREY "FFL-01" | long name "FFL-01" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 434.99999999999983
        contains 483 elements
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:2521979", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:3447833", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:3447893" (+9 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:2523204" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCROOF | type IFCCURTAINWALLTYPE "Sloped Glazing:Vitres inclinées" | object type "Sloped Glazing:Vitres inclinées" | names: "Sloped Glazing:Vitres inclinées:2544763" | parts: 1 IFCPLATE | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:2642545" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          14 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2868730", "RA319_Window-sill-brick:RA_Windows_Sill:2868927", "RA319_Window-sill-brick:RA_Windows_Sill:2868969" (+11 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2868731", "RA314_Window-frame-2x(OB+Al):Type 1:2868928", "RA314_Window-frame-2x(OB+Al):Type 1:2868970" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2868732", "RA311_Windows-sill-int-standard:Type 1:2868929", "RA311_Windows-sill-int-standard:Type 1:2868971" (+11 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          11 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2869126", "RA314_Window-frame-2x(OB+Al):Type 1:2869131", "RA314_Window-frame-2x(OB+Al):Type 1:2869136" (+8 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          22 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957181", "RA319_Glass Ext:Type 1:2957182", "RA319_Glass Ext:Type 1:2957185" (+19 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          22 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957183", "RA319_Glass Ext:Type 1:2957184", "RA319_Glass Ext:Type 1:2957187" (+19 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957229", "RA319_Glass Ext:Type 1:2957230", "RA319_Glass Ext:Type 1:2957233" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957231", "RA319_Glass Ext:Type 1:2957232", "RA319_Glass Ext:Type 1:2957235" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2958738", "RA319_Window-sill-brick:RA_Windows_Sill:2958743", "RA319_Window-sill-brick:RA_Windows_Sill:2958748" (+5 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2958739", "RA314_Window-frame-2x(OB+Al):Type 1:2958744", "RA314_Window-frame-2x(OB+Al):Type 1:2958749" (+2 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2958740", "RA311_Windows-sill-int-standard:Type 1:2958745", "RA311_Windows-sill-int-standard:Type 1:2958750" (+5 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          10 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2958782", "RA319_Glass Ext:Type 1:2958783", "RA319_Glass Ext:Type 1:2958786" (+7 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          10 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2958784", "RA319_Glass Ext:Type 1:2958785", "RA319_Glass Ext:Type 1:2958788" (+7 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2962262", "RA314_Window-frame-2x(OB+Al):Type 1:2962267", "RA314_Window-frame-2x(OB+Al):Type 1:3255105" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2962307", "RA319_Glass Ext:Type 1:2962308", "RA319_Glass Ext:Type 1:2962311" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2962309", "RA319_Glass Ext:Type 1:2962310", "RA319_Glass Ext:Type 1:2962313" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2999363" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:2999364" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:2999365" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2999366" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2999367" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3002496" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3002497" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3002498" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3052412" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3052413" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3052414" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3052415" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3052416" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3058498", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4022743", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4022791" (+12 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3281271" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:3281272" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3281273" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281275", "RA319_Glass Ext:Type 1:3281276" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281277", "RA319_Glass Ext:Type 1:3281278" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          11 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3361348", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:7007263", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:7007789" (+8 more) | parts: 64 IFCMEMBER, 11 IFCCURTAINWALL, 11 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:3386868", "RA325_081_Menuiserie:Panneau 211/73:4399795" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:3386883", "RA325_081_Menuiserie:Panneau 211/73:3463262" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:3395756" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:3446375", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:3446400", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:3462756" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:3448159" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:3453522", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:3463842", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:7217434" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:3453525" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:3453526" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:3453527" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:3453528" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:3988353" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:4022828" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4240844" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4240846" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:4240847" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4250914" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4250915" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:4257965" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:4385130" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          10 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833582", "RA319_Wall-Mullion:Brick:4833600", "RA319_Wall-Mullion:Brick:4833601" (+7 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833681", "RA319_Wall-Mullion:Brick:4833682", "RA319_Wall-Mullion:Brick:4833683" (+11 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4833995" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | object type "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | names: "RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4833996" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:4833997" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4833998" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4834000" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5477779" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5477780" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512240", "RA319_Windows-Lintel:Brick:5512273", "RA319_Windows-Lintel:Brick:5512275" (+5 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512241", "RA311_Windows-stretcher-steel:Type 1:5512274", "RA311_Windows-stretcher-steel:Type 1:5512276" (+5 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512384", "RA319_Windows-Lintel:Brick:5512386", "RA319_Windows-Lintel:Brick:5512388" (+11 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512385", "RA311_Windows-stretcher-steel:Type 1:5512387", "RA311_Windows-stretcher-steel:Type 1:5512389" (+11 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5514687" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5514688" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550808" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550809" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550837" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550838" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5846173" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:5864526", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5864803", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5864849" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5869635", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7007268", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7010960" (+4 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm:5985867" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 12.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5986168" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:6181286" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:6181381" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:6328355", "Precast Stair:Stair:6330151" | parts: 4 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          4 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7007794", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7011771", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7012335" (+1 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm:7008536" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193569", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193573" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7193570" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7193572" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194880" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7459121" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7706857" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7709525" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCGRID | names: "Default Grid"
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798783", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798795", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798751" (+3 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6328395", "Railing:A340_RA_Railing - Full - H1000mm:6331924" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2391664", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2564777", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2564779" (+11 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2433046", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2564778", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3223874" (+4 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2749206", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2959866", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2963356" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | object type "RA232_Stru - Colonne carrée:700 x 700mm" | names: "RA232_Stru - Colonne carrée:700 x 700mm:3039989" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | object type "RA232_Stru - Colonne carrée:600 x 600mm" | names: "RA232_Stru - Colonne carrée:600 x 600mm:3039991" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:3040372" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 520mm:3040375", "RA232_Stru - Poutre rectangulaire:600 x 520mm:7258921" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040377" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3133154", "Floor:RA232_Stru - Béton générique - 200mm:7215421", "Floor:RA232_Stru - Béton générique - 200mm:7265366" (+2 more) | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:3133179" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 320mm" | object type "Floor:RA232_Stru - Béton générique - 320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 320mm:5829277" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6281167", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6281289", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6973169" (+2 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:6920638" | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6944850", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946198", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946435" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945716", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6947198", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459923" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6948048", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7697790", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7704858" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7120501" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | object type "RA232_Stru - Poutre rectangulaire:400 x720mm" | names: "RA232_Stru - Poutre rectangulaire:400 x720mm:7135978" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7260679" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          29 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7308069", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309043", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309232" (+26 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1210mm:7460022" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:7470308" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632228", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635140", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635929" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7633152", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634287", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7635711" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7705695" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "10-026" | long name "Phone-Box" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849429" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-018" | long name "T2" | INTERNAL
        IFCSPACE "10-005" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5879662" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-025" | long name "OPEN_SPACE" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852027", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852034" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-030" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "10-019" | long name "T3" | INTERNAL
        IFCSPACE "10-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "10-017" | long name "ESC. 2" | INTERNAL
        IFCSPACE "10-006" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5879746", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054308" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "10-039" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855574" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-016" | long name "ESC. 1" | INTERNAL
        IFCSPACE "10-020" | long name "T1" | INTERNAL
        IFCSPACE "10-034" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852802" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-031" | long name "RACK DATA" | INTERNAL
        IFCSPACE "10-014" | long name "-" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193568" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7226420" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "10-035" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "10-029" | long name "WC PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849947" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7450970" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "10-007" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852501" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-003" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5851709", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5851878" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-040" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849908" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-037" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849981" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451014" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "10-041" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849124" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-038" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5850306" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7450850" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "10-032" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "10-033" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "10-004" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054352", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054359" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-027" | long name "Phone-Box" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7054984" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-028" | long name "Phone-Box" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5849356" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-021" | long name "T4" | INTERNAL
        IFCSPACE "10-022" | long name "GAINE" | INTERNAL
        IFCSPACE "10-023" | long name "GAINE" | INTERNAL
        IFCSPACE "10-024" | long name "T5" | INTERNAL
        IFCSPACE "10-011" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5850824" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-012" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852453" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-013" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5879739" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "10-036" | long name "SALLE DE REUNION" | INTERNAL
      IFCBUILDINGSTOREY "FFL-02" | long name "FFL-02" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 794.99999999999989
        contains 468 elements
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:2791500" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2870526", "RA319_Window-sill-brick:RA_Windows_Sill:2870536", "RA319_Window-sill-brick:RA_Windows_Sill:2870541" (+12 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870527", "RA314_Window-frame-2x(OB+Al):Type 1:2870537", "RA314_Window-frame-2x(OB+Al):Type 1:2870542" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2870528", "RA311_Windows-sill-int-standard:Type 1:2870538", "RA311_Windows-sill-int-standard:Type 1:2870543" (+12 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          12 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870547", "RA314_Window-frame-2x(OB+Al):Type 1:2870552", "RA314_Window-frame-2x(OB+Al):Type 1:2870557" (+9 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:2918950" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957272", "RA319_Glass Ext:Type 1:2957273", "RA319_Glass Ext:Type 1:2957276" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957274", "RA319_Glass Ext:Type 1:2957275", "RA319_Glass Ext:Type 1:2957278" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957320", "RA319_Glass Ext:Type 1:2957321", "RA319_Glass Ext:Type 1:2957324" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957322", "RA319_Glass Ext:Type 1:2957323", "RA319_Glass Ext:Type 1:2957326" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2959868", "RA319_Window-sill-brick:RA_Windows_Sill:2959873", "RA319_Window-sill-brick:RA_Windows_Sill:2959878" (+4 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2959869", "RA314_Window-frame-2x(OB+Al):Type 1:2959874", "RA314_Window-frame-2x(OB+Al):Type 1:2959879" (+1 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2959870", "RA311_Windows-sill-int-standard:Type 1:2959875", "RA311_Windows-sill-int-standard:Type 1:2959880" (+4 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2959912", "RA319_Glass Ext:Type 1:2959913", "RA319_Glass Ext:Type 1:2959916" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2959914", "RA319_Glass Ext:Type 1:2959915", "RA319_Glass Ext:Type 1:2959918" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2963359", "RA314_Window-frame-2x(OB+Al):Type 1:2963364", "RA314_Window-frame-2x(OB+Al):Type 1:3255196" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963404", "RA319_Glass Ext:Type 1:2963405", "RA319_Glass Ext:Type 1:2963408" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963406", "RA319_Glass Ext:Type 1:2963407", "RA319_Glass Ext:Type 1:2963410" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3000090" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3000091" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3000092" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000093" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000094" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3002828" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3002829" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3002830" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002831" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002832" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3059400", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4027772", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4027773" (+12 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          11 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3223832", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5834321", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5834400" (+8 more) | parts: 64 IFCMEMBER, 11 IFCCURTAINWALL, 11 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3255189" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3255190" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3255191" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3255192" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3255193" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3281470" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:3281471" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3281472" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281474", "RA319_Glass Ext:Type 1:3281475" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281476", "RA319_Glass Ext:Type 1:3281477" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4027761", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4027763", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4027768" (+6 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4027764" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:4027769" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          9 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833581", "RA319_Wall-Mullion:Brick:4833593", "RA319_Wall-Mullion:Brick:4833598" (+6 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833666", "RA319_Wall-Mullion:Brick:4833667", "RA319_Wall-Mullion:Brick:4833668" (+12 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4997999" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | object type "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | names: "RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4998000" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:4998001" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998002" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998004" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5477777" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5477778" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512238", "RA319_Windows-Lintel:Brick:5512269", "RA319_Windows-Lintel:Brick:5512271" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512239", "RA311_Windows-stretcher-steel:Type 1:5512270", "RA311_Windows-stretcher-steel:Type 1:5512272" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512360", "RA319_Windows-Lintel:Brick:5512362", "RA319_Windows-Lintel:Brick:5512364" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512361", "RA311_Windows-stretcher-steel:Type 1:5512363", "RA311_Windows-stretcher-steel:Type 1:5512365" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5514685" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5514686" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550806" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550807" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550835" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550836" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5847298" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865846", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865854", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6281172" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870386", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870448", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870612" (+4 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870877", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7018585", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7021180" (+1 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:5921299", "Precast Stair:Stair:6331096" | parts: 4 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5986671" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:6181285" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:6181380" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6281134", "RA325_081_Menuiserie:Panneau 211/73:6281169" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6281139", "RA325_081_Menuiserie:Panneau 211/73:6281162" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6281143", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6281144", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6281159" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6281150", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6281163", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:7443040" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6281153" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:6281164", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:7272567" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6281168" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7017670" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7024879" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7024881" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:7024882" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:7024883" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:7024929" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:7079569" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193679", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193683" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7193680" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7193682" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194946" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7208565" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7458392" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm:7533046" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 12.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7706860" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7709528" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCGRID | names: "Default Grid"
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6328121", "Railing:A340_RA_Railing - Full - H1000mm:6331981" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2478599", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2479533", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2698932" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2479470", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2496877", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2698931" (+6 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2750413", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2959927", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2963415" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | object type "RA232_Stru - Colonne carrée:700 x 700mm" | names: "RA232_Stru - Colonne carrée:700 x 700mm:3040027" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | object type "RA232_Stru - Colonne carrée:600 x 600mm" | names: "RA232_Stru - Colonne carrée:600 x 600mm:3040029" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:3040402" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 520mm:3040405", "RA232_Stru - Poutre rectangulaire:600 x 520mm:7259026" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040407" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3133278", "Floor:RA232_Stru - Béton générique - 200mm:7215565", "Floor:RA232_Stru - Béton générique - 200mm:7265570" (+2 more) | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique -320mm" | object type "Floor:RA232_Stru - Béton générique -320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique -320mm:3133302" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4217690", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6280589", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6973546" (+2 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:5833486" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:6920643" | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6944909", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946158", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946457" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945701", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6947131", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459926" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6948078", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7697517", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7704986" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7121425" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | object type "RA232_Stru - Poutre rectangulaire:400 x720mm" | names: "RA232_Stru - Poutre rectangulaire:400 x720mm:7136050" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7260551" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          29 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7308337", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309064", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309284" (+26 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7316610", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7316618", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7431584" (+1 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1210mm:7460025" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:7470368" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632280", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635189", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635933" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7633242", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634419", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7635714" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7705756" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "20-005" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852992", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7742670" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-015" | long name "OPEN SPACE" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054886", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7742560" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-014" | long name "ESC. 2" | INTERNAL
        IFCSPACE "20-004" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852936", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054613" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-006" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852880", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054647" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-002" | long name "ASC. 1" | INTERNAL
        IFCSPACE "20-011" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855557" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-013" | long name "ESC. 1" | INTERNAL
        IFCSPACE "20-022" | long name "T1" | INTERNAL
        IFCSPACE "20-018" | long name "RACK DATA" | INTERNAL
        IFCSPACE "20-023" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854209" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-024" | long name "T2" | INTERNAL
        IFCSPACE "20-029" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5853013" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-001" | long name "3 PHONE BOX" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854192" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-028" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "20-030" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "20-032" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919626" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451170" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "20-034" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7055071" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-017" | long name "WC PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854252" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451169" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "20-033" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919638" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451168" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "20-003" | long name "ASC. 2" | INTERNAL
        IFCSPACE "20-025" | long name "T3" | INTERNAL
        IFCSPACE "20-019" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "20-020" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "20-035" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5853876" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-021" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "20-012" | long name "COULOIR" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193678" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7226489" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "20-026" | long name "-" | INTERNAL
        IFCSPACE "20-027" | long name "T5" | INTERNAL
        IFCSPACE "20-007" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7742572" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-008" | long name "BUREAU" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5852978", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7742515" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-031" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054624" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "20-010" | long name "BUREAU" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7054474" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-037" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854201" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "FFL-03" | long name "FFL-03" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 1155.
        contains 478 elements
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2479118", "RA325_011:GO 215/101 - Panneau 211/93:2496875" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2479822" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:2791534" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:2792588", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6280571", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6280584" (+2 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2870688", "RA319_Window-sill-brick:RA_Windows_Sill:2870698", "RA319_Window-sill-brick:RA_Windows_Sill:2870703" (+12 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870689", "RA314_Window-frame-2x(OB+Al):Type 1:2870699", "RA314_Window-frame-2x(OB+Al):Type 1:2870704" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2870690", "RA311_Windows-sill-int-standard:Type 1:2870700", "RA311_Windows-sill-int-standard:Type 1:2870705" (+12 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          12 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870709", "RA314_Window-frame-2x(OB+Al):Type 1:2870714", "RA314_Window-frame-2x(OB+Al):Type 1:2870719" (+9 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957363", "RA319_Glass Ext:Type 1:2957364", "RA319_Glass Ext:Type 1:2957367" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957365", "RA319_Glass Ext:Type 1:2957366", "RA319_Glass Ext:Type 1:2957369" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957411", "RA319_Glass Ext:Type 1:2957412", "RA319_Glass Ext:Type 1:2957415" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957413", "RA319_Glass Ext:Type 1:2957414", "RA319_Glass Ext:Type 1:2957417" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2959929", "RA319_Window-sill-brick:RA_Windows_Sill:2959934", "RA319_Window-sill-brick:RA_Windows_Sill:2959939" (+4 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2959930", "RA314_Window-frame-2x(OB+Al):Type 1:2959935", "RA314_Window-frame-2x(OB+Al):Type 1:2959940" (+1 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2959931", "RA311_Windows-sill-int-standard:Type 1:2959936", "RA311_Windows-sill-int-standard:Type 1:2959941" (+4 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2959973", "RA319_Glass Ext:Type 1:2959974", "RA319_Glass Ext:Type 1:2959977" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2959975", "RA319_Glass Ext:Type 1:2959976", "RA319_Glass Ext:Type 1:2959979" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2963418", "RA314_Window-frame-2x(OB+Al):Type 1:2963423", "RA314_Window-frame-2x(OB+Al):Type 1:3255386" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963463", "RA319_Glass Ext:Type 1:2963464", "RA319_Glass Ext:Type 1:2963467" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963465", "RA319_Glass Ext:Type 1:2963466", "RA319_Glass Ext:Type 1:2963469" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3000099" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3000100" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3000101" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000102" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000103" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3002843" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3002844" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3002845" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002846" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002847" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3059498", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4217696", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4217697" (+14 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:3232135" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3233941", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5837033" | parts: 12 IFCMEMBER, 2 IFCCURTAINWALL, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3255379" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3255380" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3255381" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3255382" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3255383" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3281640" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:3281641" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3281642" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281644", "RA319_Glass Ext:Type 1:3281645" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281646", "RA319_Glass Ext:Type 1:3281647" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4217675", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4217676", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4217682" (+14 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4217677" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:4217684" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4217688" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:4217693" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:4217695" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:4218419" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241304" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241307" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4241308" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          9 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833580", "RA319_Wall-Mullion:Brick:4833592", "RA319_Wall-Mullion:Brick:4833596" (+6 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833651", "RA319_Wall-Mullion:Brick:4833652", "RA319_Wall-Mullion:Brick:4833653" (+12 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4998012" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | object type "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | names: "RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4998013" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:4998014" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998015" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998017" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5477775" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5477776" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512236", "RA319_Windows-Lintel:Brick:5512265", "RA319_Windows-Lintel:Brick:5512267" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512237", "RA311_Windows-stretcher-steel:Type 1:5512266", "RA311_Windows-stretcher-steel:Type 1:5512268" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512336", "RA319_Windows-Lintel:Brick:5512338", "RA319_Windows-Lintel:Brick:5512340" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512337", "RA311_Windows-stretcher-steel:Type 1:5512339", "RA311_Windows-stretcher-steel:Type 1:5512341" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5514683" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5514684" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550804" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550805" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550833" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550834" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5836707", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5905202", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5906287" (+11 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_200_PorteSimple_Coulissante:201/1x93" | object type "RA325_200_PorteSimple_Coulissante:201/1x93" | names: "RA325_200_PorteSimple_Coulissante:201/1x93:5837747" | material: "<Unnamed>" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5847322" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865949", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6280594", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6280595" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870994" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871064" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:5921333", "Precast Stair:Stair:6331140" | parts: 4 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5987124" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:6181284" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:6181379" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6280555", "RA325_081_Menuiserie:Panneau 211/73:6280591" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6280560", "RA325_081_Menuiserie:Panneau 211/73:6280583" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6280564", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6280565", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6280580" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6280573" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6280574" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6280575" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6280590" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193751", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193755", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193810" (+1 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7193752" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7193754" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7195033" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7459125" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm:7533058" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 12.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7706863" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7709531" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7753120" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCGRID | names: "Default Grid"
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6328738", "Railing:A340_RA_Railing - Full - H1000mm:6332111" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2497170", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2709797", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3234103" (+2 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2751111" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798611", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:3514995", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:3514996" (+4 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2959988", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2963474", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3683248" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:3040058" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:3040060" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:3040428" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 520mm:3040431", "RA232_Stru - Poutre rectangulaire:600 x 520mm:7259086" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040433" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3133345", "Floor:RA232_Stru - Béton générique - 200mm:7218102", "Floor:RA232_Stru - Béton générique - 200mm:7266216" (+2 more) | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique -320mm" | object type "Floor:RA232_Stru - Béton générique -320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique -320mm:3133369" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6288175", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6974126", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7122710" (+2 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:6920648" | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6944982", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946126", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946514" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945664", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6947092", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459929" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6948103", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7705190", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7715366" (+1 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:6987371" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:7061662" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7123137" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | object type "RA232_Stru - Poutre rectangulaire:400 x720mm" | names: "RA232_Stru - Poutre rectangulaire:400 x720mm:7136137" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7260425" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          28 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7308491", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309122", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:7309313" (+25 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1210mm:7460028" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:7470502" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632389", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635306", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635937" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7633379", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634532", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7635717" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7697363" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7705855" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "30-027" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7055256" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-006" | long name "KITCHENETTE" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854793" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-028" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854644" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-021" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7743361" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-022" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5915500" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-009" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "30-010" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "30-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "30-007" | long name "KITCHENETTE" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7744237" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-029" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855540" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "30-004" | long name "ESC. 1" | INTERNAL
        IFCSPACE "30-013" | long name "T1" | INTERNAL
        IFCSPACE "30-014" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854487" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-015" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854504" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-016" | long name "T2" | INTERNAL
        IFCSPACE "30-011" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "30-005" | long name "ESC. 2" | INTERNAL
        IFCSPACE "30-025" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919675" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451197" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "30-026" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919687" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451195" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "30-003" | long name "BUREAU PAYSAGER" | INTERNAL
          contains 7 elements
            6 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5879673", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5879680", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890813" (+3 more) | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193750" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "30-023" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "30-024" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "30-017" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5854496" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "30-008" | long name "WC PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855040" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451196" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "30-012" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "30-018" | long name "T3" | INTERNAL
        IFCSPACE "30-019" | long name "-" | INTERNAL
        IFCSPACE "30-020" | long name "T5" | INTERNAL
        IFCSPACE "60-043" | long name "LOCAL DATA" | INTERNAL
      IFCBUILDINGSTOREY "FFL-04" | long name "FFL-04" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 1515.
        contains 465 elements
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2497171" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2497172" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2698478" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:2791577" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2870850", "RA319_Window-sill-brick:RA_Windows_Sill:2870860", "RA319_Window-sill-brick:RA_Windows_Sill:2870865" (+12 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870851", "RA314_Window-frame-2x(OB+Al):Type 1:2870861", "RA314_Window-frame-2x(OB+Al):Type 1:2870866" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2870852", "RA311_Windows-sill-int-standard:Type 1:2870862", "RA311_Windows-sill-int-standard:Type 1:2870867" (+12 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          12 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2870871", "RA314_Window-frame-2x(OB+Al):Type 1:2870876", "RA314_Window-frame-2x(OB+Al):Type 1:2870881" (+9 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957454", "RA319_Glass Ext:Type 1:2957455", "RA319_Glass Ext:Type 1:2957458" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957456", "RA319_Glass Ext:Type 1:2957457", "RA319_Glass Ext:Type 1:2957460" (+21 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957502", "RA319_Glass Ext:Type 1:2957503", "RA319_Glass Ext:Type 1:2957506" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2957504", "RA319_Glass Ext:Type 1:2957505", "RA319_Glass Ext:Type 1:2957508" (+3 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:2959990", "RA319_Window-sill-brick:RA_Windows_Sill:2959995", "RA319_Window-sill-brick:RA_Windows_Sill:2960000" (+4 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2959991", "RA314_Window-frame-2x(OB+Al):Type 1:2959996", "RA314_Window-frame-2x(OB+Al):Type 1:2960001" (+1 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:2959992", "RA311_Windows-sill-int-standard:Type 1:2959997", "RA311_Windows-sill-int-standard:Type 1:2960002" (+4 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2960034", "RA319_Glass Ext:Type 1:2960035", "RA319_Glass Ext:Type 1:2960038" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2960036", "RA319_Glass Ext:Type 1:2960037", "RA319_Glass Ext:Type 1:2960040" (+5 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:2963477", "RA314_Window-frame-2x(OB+Al):Type 1:2963482", "RA314_Window-frame-2x(OB+Al):Type 1:3258339" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963522", "RA319_Glass Ext:Type 1:2963523", "RA319_Glass Ext:Type 1:2963526" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:2963524", "RA319_Glass Ext:Type 1:2963525", "RA319_Glass Ext:Type 1:2963528" (+4 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3000108" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3000109" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3000110" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000111" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3000112" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3002858" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3002859" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3002860" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002861" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3002862" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3059698", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4219143", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4219144" (+17 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:3233663" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3234091", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5838710" | parts: 12 IFCMEMBER, 2 IFCCURTAINWALL, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3258332" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:3258333" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3258334" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3258335" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3258336" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:3281652" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | object type "RA314_Window-frame-2x(OB+Al):Type 1" | names: "RA314_Window-frame-2x(OB+Al):Type 1:3281653" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:3281654" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281656", "RA319_Glass Ext:Type 1:3281657" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:3281658", "RA319_Glass Ext:Type 1:3281659" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4219122", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4219123", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4219129" (+11 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4219124" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:4219131" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4219135" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:4219140" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:4219142" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:4219146" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241442" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241445" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4241446" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4330839", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:6288163" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833578", "RA319_Wall-Mullion:Brick:4833591", "RA319_Wall-Mullion:Brick:4833594" (+6 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | object type "RA319_Wall-Mullion:Brick" | names: "RA319_Wall-Mullion:Brick:4833615", "RA319_Wall-Mullion:Brick:4833617", "RA319_Wall-Mullion:Brick:4833618" (+12 more) | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4998025" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | object type "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | names: "RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4998026" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | object type "RA311_Windows-sill-int-standard:Type 1" | names: "RA311_Windows-sill-int-standard:Type 1:4998027" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998028" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4998030" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5477771" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5477772" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512232", "RA319_Windows-Lintel:Brick:5512261", "RA319_Windows-Lintel:Brick:5512263" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512233", "RA311_Windows-stretcher-steel:Type 1:5512262", "RA311_Windows-stretcher-steel:Type 1:5512264" (+4 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5512294", "RA319_Windows-Lintel:Brick:5512298", "RA319_Windows-Lintel:Brick:5512300" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          15 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5512295", "RA311_Windows-stretcher-steel:Type 1:5512299", "RA311_Windows-stretcher-steel:Type 1:5512301" (+12 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5514679" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5514680" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550800" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550801" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5550828" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550829" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5838262", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5906227", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5915006" (+10 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_200_PorteSimple_Coulissante:201/1x93" | object type "RA325_200_PorteSimple_Coulissante:201/1x93" | names: "RA325_200_PorteSimple_Coulissante:201/1x93:5839206" | material: "<Unnamed>" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5847345", "Compound Ceiling:Quadrillage 600 x 600 mm:5855598" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865965", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865966", "Basic Wall:RA223 - Mur Int - Finition Carrelage:5865971" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871125" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871161" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:5921367", "Precast Stair:Stair:6331184" | parts: 4 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5994434" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:6181282" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:6181376" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6288141", "RA325_081_Menuiserie:Panneau 211/73:6288177" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6288146" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6288150", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6288151", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6288166" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6288157", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6288170", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:7225659" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6288159" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6288160" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6288161" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6288169" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6288176" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7193811" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7193813" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7195103" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7459128" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm:7533070" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 12.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7706866" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:7709534" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7755199" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCGRID | names: "Default Grid"
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6329213", "Railing:A340_RA_Railing - Full - H1000mm:6332049" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Système d'ossature" | BEAM_GRID | names: "Structural Beam System:Système d'ossature:3134920" | parts: 6 IFCBEAM | property sets: Pset_QuantityTakeOff
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2701283", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:2710148", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3365114" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:3003460", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:3774687" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3003462", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3043488" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:3040089" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:3040091" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | object type "RA232_Stru - Poutre rectangulaire:600 x 460mm" | names: "RA232_Stru - Poutre rectangulaire:600 x 460mm:3040454" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:500 x 620mm" | object type "RA232_Stru - Poutre rectangulaire:500 x 620mm" | names: "RA232_Stru - Poutre rectangulaire:500 x 620mm:3040457", "RA232_Stru - Poutre rectangulaire:500 x 620mm:7259206" | material: "M-280_02 - Beton Arme"; "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040459" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3133412", "Floor:RA232_Stru - Béton générique - 200mm:7266417", "Floor:RA232_Stru - Béton générique - 200mm:7468785" (+2 more) | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique -320mm" | object type "Floor:RA232_Stru - Béton générique -320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique -320mm:3133436" | material: layers "Floor:RA232_Stru - Béton générique -320mm" ("M-280_02 - Beton Arme" 32.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3360766" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361265" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361272" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361278" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361284" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361290" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361296" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361302" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE450AA" | object type "H-Wide Flange Beams:HE450AA" | names: "H-Wide Flange Beams:HE450AA:4258651", "H-Wide Flange Beams:HE450AA:4258705" | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4380566", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4380567", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5821949" (+1 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5820478" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 300mm" | object type "Floor:RA239_Finition - Sol terrasse - 300mm" | FLOOR | names: "Floor:RA239_Finition - Sol terrasse - 300mm:5961784" | material: layers "Floor:RA239_Finition - Sol terrasse - 300mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm" | object type "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm" | names: "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm:5981076", "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm:5981547", "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm:5981628" (+1 more) | material: layers "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm" ("M-479_02 - FinExt - Plaque type1" 4., "M-000_000_Div. Vides - Air" 4., "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6289296", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6289300", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7123209" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | object type "Basic Wall:RA2xx_ isolant - Mitoyen" | names: "Basic Wall:RA2xx_ isolant - Mitoyen:6920653" | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6944608", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7697130", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7705367" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945003", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946087", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946534" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945617", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6947052", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459932" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 320mm" | object type "Floor:RA232_Stru - Béton générique - 320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 320mm:7061021" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:7061776" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7123008" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | object type "RA232_Stru - Poutre rectangulaire:400 x720mm" | names: "RA232_Stru - Poutre rectangulaire:400 x720mm:7136175" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7260316" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7316784", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7316796", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:7316808" (+4 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1110mm:7460031" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632554", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635941" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7633596", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634593", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7635720" (+3 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635365", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7705881" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "40-025" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919736" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451320" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "40-026" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855432" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-020" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5915683" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-021" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5915676" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-009" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "40-010" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "40-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "40-006" | long name "KITCHENETTE" | INTERNAL
        IFCSPACE "40-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "40-027" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855495" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-004" | long name "ESC. 1" | INTERNAL
        IFCSPACE "40-013" | long name "T1" | INTERNAL
        IFCSPACE "40-014" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855443" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-015" | long name "T2" | INTERNAL
        IFCSPACE "40-011" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "40-005" | long name "ESC. 2" | INTERNAL
        IFCSPACE "40-022" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "40-023" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "40-003" | long name "BUREAU PAYSAGER" | INTERNAL
          contains 5 elements
            4 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890770", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890777", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890823" (+1 more) | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193809" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "40-007" | long name "KITCHENETTE" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7756145" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-016" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855451" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-017" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855459" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-024" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919724" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451322" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "40-028" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7055393" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "40-008" | long name "WC PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5855468" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451321" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "40-012" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "40-018" | long name "T3" | INTERNAL
        IFCSPACE "40-019" | long name "T5" | INTERNAL
        IFCSPACE "60-041" | long name "-" | INTERNAL
        IFCSPACE "60-044" | long name "LOCAL DATA" | INTERNAL
      IFCBUILDINGSTOREY "FFL-05" | long name "FFL-05" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 1875.
        contains 659 elements
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2567298" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          101 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2589548", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2589549", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:2589550" (+98 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:2701284" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/111 - Panneau 211/103" | object type "RA325_011:GO 215/111 - Panneau 211/103" | names: "RA325_011:GO 215/111 - Panneau 211/103:2701285" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:3003466" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 300mm" | object type "Floor:RA239_Finition - Sol terrasse - 300mm" | FLOOR | names: "Floor:RA239_Finition - Sol terrasse - 300mm:3006053" | material: layers "Floor:RA239_Finition - Sol terrasse - 300mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA479_Roof-edge-60" | object type "Floor:RA479_Roof-edge-60" | FLOOR | names: "Floor:RA479_Roof-edge-60:3030916" | material: layers "Floor:RA479_Roof-edge-60" ("M-479_RoofFin-mpx" 1.8, "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100:3031032" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3059849", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6992257", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7128023" (+10 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:3234626" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3235891", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5840256" | parts: 12 IFCMEMBER, 2 IFCCURTAINWALL, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220057", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220058", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220064" (+14 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4220059" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220066" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4220070" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:4220075" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:4220077" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | object type "RA325_011:GO 215/91 - Panneau 211/83" | names: "RA325_011:GO 215/91 - Panneau 211/83:4220081" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241571" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241574" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4241575" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4375558", "RA314_Window-frame-1x(OB+Al):Type 1:5962879", "RA314_Window-frame-1x(OB+Al):Type 1:5962955" (+4 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375564", "RA319_Glass Ext:Type 1:4377027", "RA319_Glass Ext:Type 1:5962880" (+10 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375565", "RA319_Glass Ext:Type 1:5962881", "RA319_Glass Ext:Type 1:5962957" (+4 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          18 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4375721", "RA314_Window-frame-1x(OB+Al):Type 1:5963524", "RA314_Window-frame-1x(OB+Al):Type 1:5963797" (+15 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          18 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375723", "RA319_Glass Ext:Type 1:5963525", "RA319_Glass Ext:Type 1:5963798" (+15 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          18 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375725", "RA319_Glass Ext:Type 1:5963526", "RA319_Glass Ext:Type 1:5963799" (+15 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          18 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4376201", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5963527", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5963800" (+15 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          7 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4376350", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5962882", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5962958" (+4 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-stone:RA_Windows_Sill" | object type "RA319_Window-sill-stone:RA_Windows_Sill" | names: "RA319_Window-sill-stone:RA_Windows_Sill:4377019", "RA319_Window-sill-stone:RA_Windows_Sill:5967131", "RA319_Window-sill-stone:RA_Windows_Sill:5967179" (+3 more) | material: "M-313_14 - Seuil de Porte en Beton" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4377020", "RA314_Window-frame-1x(OB+Al):Type 1:5967132", "RA314_Window-frame-1x(OB+Al):Type 1:5967180" (+3 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377029", "RA319_Glass Ext:Type 1:5967134", "RA319_Glass Ext:Type 1:5967182" (+3 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4377037", "RA319_Window-sill-brick:RA_Windows_Sill:5964865", "RA319_Window-sill-brick:RA_Windows_Sill:5964930" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4377038", "RA314_Window-frame-1x(OB+Al):Type 1:5964866", "RA314_Window-frame-1x(OB+Al):Type 1:5964931" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377044", "RA319_Glass Ext:Type 1:5964867", "RA319_Glass Ext:Type 1:5964932" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377045", "RA319_Glass Ext:Type 1:5964868", "RA319_Glass Ext:Type 1:5964933" | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4377065", "RA319_Window-sill-brick:RA_Windows_Sill:5964339", "RA319_Window-sill-brick:RA_Windows_Sill:5964410" (+10 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4377066", "RA314_Window-frame-1x(OB+Al):Type 1:5964340", "RA314_Window-frame-1x(OB+Al):Type 1:5964411" (+10 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377072", "RA319_Glass Ext:Type 1:5964341", "RA319_Glass Ext:Type 1:5964412" (+10 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377073", "RA319_Glass Ext:Type 1:5964342", "RA319_Glass Ext:Type 1:5964413" (+10 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4378028", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5964869", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5964934" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4378045", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5964343", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5964414" (+10 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4381798", "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4381799", "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4381853" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 13.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          20 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550780", "RA311_Windows-stretcher-steel:Type 1:5550876", "RA311_Windows-stretcher-steel:Type 1:5962883" (+17 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          21 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550865", "RA311_Windows-stretcher-steel:Type 1:5685782", "RA311_Windows-stretcher-steel:Type 1:5963528" (+18 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          20 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5587170", "RA319_Windows-Lintel:Brick:5686370", "RA319_Windows-Lintel:Brick:5962884" (+17 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5685850", "RA311_Windows-stretcher-steel:Type 1:5967136", "RA311_Windows-stretcher-steel:Type 1:5967184" (+3 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          21 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5686200", "RA319_Windows-Lintel:Brick:5686363", "RA319_Windows-Lintel:Brick:5963529" (+18 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5686404", "RA319_Windows-Lintel:Brick:5967137", "RA319_Windows-Lintel:Brick:5967185" (+3 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5839729", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5906230", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5915009" (+21 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5847368", "Compound Ceiling:Quadrillage 600 x 600 mm:7757079" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871234" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871296" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:5921401", "Precast Stair:Stair:6331228" | parts: 4 IFCRAILING, 4 IFCSLAB, 4 IFCSTAIRFLIGHT | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:5963294", "RA314_Window-frame-1x(OB+Al):Type 1:5963378" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:5963295", "RA319_Glass Ext:Type 1:5963379" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:5963296", "RA319_Glass Ext:Type 1:5963380" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:5963297", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5963381" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5963298", "RA311_Windows-stretcher-steel:Type 1:5963382" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5963299", "RA319_Windows-Lintel:Brick:5963383" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5997473" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:6289254", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6289255", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6289256" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6289266", "RA325_081_Menuiserie:Panneau 211/73:6289302" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6289271", "RA325_081_Menuiserie:Panneau 211/73:6289294" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6289275", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6289276", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6289291" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6289282", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6289295", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:7482625" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6289284" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6289285" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6289286" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6289301" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:6978400", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:6987664", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:2594132" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193906", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193910" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7193907" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7193909" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7195171" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7459131" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm:7531321", "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm:7531322" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" ("M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm:7533082" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 22.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7706869" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7709537" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7756523" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing:RA340_Railing Ext - Partiel - H1100mm" | object type "Railing:RA340_Railing Ext - Partiel - H1100mm" | names: "Railing:RA340_Railing Ext - Partiel - H1100mm:2497544" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCGRID | names: "Default Grid"
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798819", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:3906271", "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm:2798831" (+11 more) | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3003458", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2755023", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2755024" (+1 more) | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3003459", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3043487", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:2532892" (+3 more) | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:6979335", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:2755025", "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm:3778441" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6329153", "Railing:A340_RA_Railing - Full - H1000mm:6332157" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:3040120" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 660mm" | object type "RA232_Stru - Poutre rectangulaire:350 x 660mm" | names: "RA232_Stru - Poutre rectangulaire:350 x 660mm:3040506" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:500 x 620mm" | object type "RA232_Stru - Poutre rectangulaire:500 x 620mm" | names: "RA232_Stru - Poutre rectangulaire:500 x 620mm:3040509" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040511" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:3133546", "Floor:RA232_Stru - Béton générique - 200mm:7218836", "Floor:RA232_Stru - Béton générique - 200mm:7266818" (+2 more) | material: "M-280_02 - Beton Arme"; layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique -320mm" | object type "Floor:RA232_Stru - Béton générique -320mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique -320mm:3133570" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          8 x IFCBEAM | type IFCBEAMTYPE "HE-M:HEM300" | object type "HE-M:HEM300" | names: "HE-M:HEM300:3360132", "HE-M:HEM300:3360134", "HE-M:HEM300:3360138" (+5 more) | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 160 mm" | object type "Floor:RA232_Stru - Béton générique - 160 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 160 mm:3360173" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361312" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361314" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361316" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361318" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361320" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361322" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HE-A Column:HEA260" | object type "HE-A Column:HEA260" | names: "HE-A Column:HEA260:3361324" | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3399896", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:3399899", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:5886197" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:3769924" | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:4220751", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6290198", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6290202" (+2 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:4252322", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:6915358", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7705409" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4380058", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4380225", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:7168992" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:4380164", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5984165", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5984285" (+1 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:4380409", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:4380455", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:7459935" (+5 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm" | object type "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm" | names: "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm:5982275", "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm:5982277", "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm:5984381" (+1 more) | material: layers "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm" ("M-479_02 - FinExt - Plaque type1" 4., "M-000_000_Div. Vides - Air" 4.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6945885", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:6946569" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:7061158" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | object type "RA232_Stru - Colonne rectangulaire:500 x 600mm" | names: "RA232_Stru - Colonne rectangulaire:500 x 600mm:7124264" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | object type "RA232_Stru - Colonne carrée:500 x 500mm" | names: "RA232_Stru - Colonne carrée:500 x 500mm:7133198" | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:400 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:400 x 520mm:7136288" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:350 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:350 x 520mm:7259388" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7260174" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          7 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE200A" | object type "H-Wide Flange Beams:HE200A" | names: "H-Wide Flange Beams:HE200A:7297692", "H-Wide Flange Beams:HE200A:7297694", "H-Wide Flange Beams:HE200A:7297696" (+4 more) | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1110mm:7460034" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7632628", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635447", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:7635945" (+1 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7633698", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7634701", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:7635723" (+1 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "50-006" | long name "KITCHENETTE" | INTERNAL
        IFCSPACE "50-027" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5856486" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-021" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5915935" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-008" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "50-009" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "50-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "50-022" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5856757" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-012" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Roof Drain:380 mm Strainer - 200 mm Drain" | object type "M_Roof Drain:380 mm Strainer - 200 mm Drain" | names: "M_Roof Drain:380 mm Strainer - 200 mm Drain:3625774" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "50-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "50-013" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5857218" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-004" | long name "ESC. 1" | INTERNAL
        IFCSPACE "50-014" | long name "T1" | INTERNAL
        IFCSPACE "50-015" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5857166" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-016" | long name "T2" | INTERNAL
        IFCSPACE "50-010" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "50-005" | long name "ESC. 2" | INTERNAL
        IFCSPACE "50-025" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919770" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451339" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "50-003" | long name "BUREAU PAYSAGER" | INTERNAL
          contains 7 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1" | object type "Generic Models 1:Generic Models 1" | names: "Generic Models 1:Generic Models 1:4379874" | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            5 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890792", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890831", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7748096" (+2 more) | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193905" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "50-023" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "50-024" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "50-026" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919782" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451352" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "50-028" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7055580" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-007" | long name "WC PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5857191" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451338" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "50-017" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5857174" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-018" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5857182" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "50-011" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "50-019" | long name "T3" | INTERNAL
        IFCSPACE "50-020" | long name "-" | INTERNAL
        IFCSPACE "60-045" | long name "LOCAL DATA" | INTERNAL
      IFCBUILDINGSTOREY "FFL-06" | long name "FFL-06" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 2235.
        contains 516 elements
          12 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | object type "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | names: "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:2718385", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:3237416", "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM:5841052" (+9 more) | parts: 120 IFCMEMBER, 31 IFCPLATE, 8 IFCCURTAINWALL | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | object type "Curtain Wall:RA313 - Window_Gris Clair" | names: "Curtain Wall:RA313 - Window_Gris Clair:2791663" | parts: 13 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 300mm" | object type "Floor:RA239_Finition - Sol terrasse - 300mm" | FLOOR | names: "Floor:RA239_Finition - Sol terrasse - 300mm:3005543" | material: layers "Floor:RA239_Finition - Sol terrasse - 300mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 250mm" | object type "Floor:RA239_Finition - Sol terrasse - 250mm" | FLOOR | names: "Floor:RA239_Finition - Sol terrasse - 250mm:3006815" | material: layers "Floor:RA239_Finition - Sol terrasse - 250mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 12.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA479_Roof-edge-60" | object type "Floor:RA479_Roof-edge-60" | FLOOR | names: "Floor:RA479_Roof-edge-60:3031616", "Floor:RA479_Roof-edge-60:3047891" | material: materials ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)", "M-479_RoofFin-mpx", "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100:3048364", "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100:3323225" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3059994", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6992264", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7128786" (+3 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | object type "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 370mm:3238356" | material: materials ("M-430_01 - Sol Finition Gén Type 1", "M-000_000_Div. Vides - Air") | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Roof Drain:380 mm Strainer - 200 mm Drain" | object type "M_Roof Drain:380 mm Strainer - 200 mm Drain" | names: "M_Roof Drain:380 mm Strainer - 200 mm Drain:3625108", "M_Roof Drain:380 mm Strainer - 200 mm Drain:3625226", "M_Roof Drain:380 mm Strainer - 200 mm Drain:3625332" (+1 more) | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220737", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220746", "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm:4220748" (+9 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/111 - Panneau 211/103 - EI30" | object type "RA325_011:GO 215/111 - Panneau 211/103 - EI30" | names: "RA325_011:GO 215/111 - Panneau 211/103 - EI30:4220738" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | object type "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | names: "RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220745" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_001:GO 215/101 - Panneau 211/93 - EI30:4220749" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4220760" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | object type "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | names: "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241683" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | object type "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | names: "RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241686" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4241687" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | object type "RA325_001:GO 215/91 - Panneau 211/83" | names: "RA325_001:GO 215/91 - Panneau 211/83:4287332" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4375824", "RA319_Window-sill-brick:RA_Windows_Sill:4375863", "RA319_Window-sill-brick:RA_Windows_Sill:4375881" (+20 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4375825", "RA314_Window-frame-1x(OB+Al):Type 1:4375864", "RA314_Window-frame-1x(OB+Al):Type 1:4375882" (+20 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          27 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375827", "RA319_Glass Ext:Type 1:4375871", "RA319_Glass Ext:Type 1:4375884" (+24 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4375829", "RA319_Glass Ext:Type 1:4375873", "RA319_Glass Ext:Type 1:4375886" (+20 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:4377145", "RA319_Window-sill-brick:RA_Windows_Sill:4377220", "RA319_Window-sill-brick:RA_Windows_Sill:5966291" (+10 more) | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4377146", "RA314_Window-frame-1x(OB+Al):Type 1:4377221", "RA314_Window-frame-1x(OB+Al):Type 1:5966292" (+10 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377147", "RA319_Glass Ext:Type 1:4377223", "RA319_Glass Ext:Type 1:5966293" (+10 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377148", "RA319_Glass Ext:Type 1:4377225", "RA319_Glass Ext:Type 1:5966294" (+10 more) | material: "M-316_02 - Vitrage - Type 2" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-stone:RA_Windows_Sill" | object type "RA319_Window-sill-stone:RA_Windows_Sill" | names: "RA319_Window-sill-stone:RA_Windows_Sill:4377233", "RA319_Window-sill-stone:RA_Windows_Sill:5966768", "RA319_Window-sill-stone:RA_Windows_Sill:5966919" (+1 more) | material: "M-313_14 - Seuil de Porte en Beton" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:4377234", "RA314_Window-frame-1x(OB+Al):Type 1:5966769", "RA314_Window-frame-1x(OB+Al):Type 1:5966920" (+1 more) | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:4377238", "RA319_Glass Ext:Type 1:5966771", "RA319_Glass Ext:Type 1:5966922" (+1 more) | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4378682", "RA311_Windows-sill-int-standard:Tablette + ebrasement:4378692", "RA311_Windows-sill-int-standard:Tablette + ebrasement:4378802" (+20 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:4379129", "RA311_Windows-sill-int-standard:Tablette + ebrasement:4379491", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5966295" (+10 more) | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4380843", "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4380956", "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm:4381008" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 13.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5550874", "RA311_Windows-stretcher-steel:Type 1:5685859", "RA311_Windows-stretcher-steel:Type 1:5966296" (+10 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5685744", "RA311_Windows-stretcher-steel:Type 1:5685807", "RA311_Windows-stretcher-steel:Type 1:5685818" (+20 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5685797", "RA311_Windows-stretcher-steel:Type 1:5966773", "RA311_Windows-stretcher-steel:Type 1:5966924" (+1 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          23 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5685925", "RA319_Windows-Lintel:Brick:5686226", "RA319_Windows-Lintel:Brick:5686324" (+20 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          13 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5686268", "RA319_Windows-Lintel:Brick:5686369", "RA319_Windows-Lintel:Brick:5966297" (+10 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5686417", "RA319_Windows-Lintel:Brick:5966774", "RA319_Windows-Lintel:Brick:5966925" (+1 more) | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5847392", "Compound Ceiling:Quadrillage 600 x 600 mm:7607167" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm:5857825" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5., "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871328", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871429", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871535" (+3 more) | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | object type "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | names: "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5871382", "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:7048326" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Precast Stair:Precast Stair" | object type "Precast Stair:Precast Stair" | names: "Precast Stair:Stair:5921435" | parts: 2 IFCSLAB, 2 IFCSTAIRFLIGHT, 1 IFCRAILING | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_StairCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | object type "RA319_Window-sill-brick:RA_Windows_Sill" | names: "RA319_Window-sill-brick:RA_Windows_Sill:5965433", "RA319_Window-sill-brick:RA_Windows_Sill:5965441" | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | object type "RA314_Window-frame-1x(OB+Al):Type 1" | names: "RA314_Window-frame-1x(OB+Al):Type 1:5965434", "RA314_Window-frame-1x(OB+Al):Type 1:5965442" | material: "M-310_01 - Chassis - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:5965435", "RA319_Glass Ext:Type 1:5965443" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | object type "RA319_Glass Ext:Type 1" | names: "RA319_Glass Ext:Type 1:5965436", "RA319_Glass Ext:Type 1:5965444" | material: "M-316_01 - Vitrage - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | object type "RA311_Windows-sill-int-standard:Tablette + ebrasement" | names: "RA311_Windows-sill-int-standard:Tablette + ebrasement:5965437", "RA311_Windows-sill-int-standard:Tablette + ebrasement:5965445" | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | object type "RA311_Windows-stretcher-steel:Type 1" | names: "RA311_Windows-stretcher-steel:Type 1:5965438", "RA311_Windows-stretcher-steel:Type 1:5965446" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | object type "RA319_Windows-Lintel:Brick" | names: "RA319_Windows-Lintel:Brick:5965439", "RA319_Windows-Lintel:Brick:5965447" | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | object type "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _ Carrelage- 250mm:5998514" | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif" | object type "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif" | names: "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif:6205177", "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif:6205180", "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif:6205184" | parts: 6 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | object type "Basic Wall:RA223 - Mur Int - Finition Carrelage" | names: "Basic Wall:RA223 - Mur Int - Finition Carrelage:6290163", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6290164", "Basic Wall:RA223 - Mur Int - Finition Carrelage:6290165" (+17 more) | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6290168", "RA325_081_Menuiserie:Panneau 211/73:6290204" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | object type "RA325_081_Menuiserie:Panneau 211/73" | names: "RA325_081_Menuiserie:Panneau 211/73:6290173", "RA325_081_Menuiserie:Panneau 211/73:6290196" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | object type "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | names: "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6290177", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6290178", "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm:6290193" (+1 more) | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6290184", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:6290197", "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm:7482880" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6290186" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6290187" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:6290188" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | object type "RA325_001:GO 215/101 - Panneau 211/93" | names: "RA325_001:GO 215/101 - Panneau 211/93:6290203" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7193999", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm:7194003" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | object type "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | names: "Basic Wall:RA220 -Panneau - Type 1 - 22 mm:7194000" | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194002" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | object type "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | names: "RA325_001:GO 215/91 - Panneau 211/83 - EI30:7195269" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BLUEKIT_360x360:BLUEKIT_360x360" | object type "BLUEKIT_360x360:BLUEKIT_360x360" | names: "BLUEKIT_360x360:BLUEKIT_360x360:7281834", "BLUEKIT_360x360:BLUEKIT_360x360:7281865", "BLUEKIT_360x360:BLUEKIT_360x360:7282019" (+1 more) | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | object type "RA_A-570_Ventelles:Occurence" | names: "RA_A-570_Ventelles:Occurence:7286130" | material: materials ("A-570_Grille de ventilation en aluminium de teinte - RAL 7039", "A-570_Châssis en aluminium de teinte - RAL 7039") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | object type "RA_A-570_Ventelles:Occurence" | names: "RA_A-570_Ventelles:Occurence:7287056" | material: materials ("A-570_Châssis en aluminium de teinte - RAL 7039", "A-570_Grille de ventilation en aluminium de teinte - RAL 7039") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7459134" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm:7531229", "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm:7531257" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" ("M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" | object type "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" | FLOOR | names: "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm:7533095" | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 22.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7706872" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7709540" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | object type "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | names: "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:7757668", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:7757669", "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm:7757670" | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | object type "RA325_011:GO 215/101 - Panneau 211/93" | names: "RA325_011:GO 215/101 - Panneau 211/93:7757671" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:RA340_Railing Ext - Partiel - H1100mm" | object type "Railing:RA340_Railing Ext - Partiel - H1100mm" | names: "Railing:RA340_Railing Ext - Partiel - H1100mm:2549392", "Railing:RA340_Railing Ext - Partiel - H1100mm:3004894" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCGRID | names: "Default Grid"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | object type "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | names: "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm:3043021" | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | object type "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | names: "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm:3047442" | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Ceilings 1:Ceilings 1" | object type "Ceilings 1:Ceilings 1" | names: "Ceilings 1:Ceilings 1:7607857" | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | object type "Railing:A340_RA_Railing - Full - H1000mm" | names: "Railing:A340_RA_Railing - Full - H1000mm:6329275" | material: "M-340_Railing - Teinte gris clair" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCROOF | object type "Basic Roof:Générique - 250 mm - Toiture Végétalisée" | names: "Basic Roof:Générique - 250 mm - Toiture Végétalisée:3005311" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 250 mm - Toiture Végétalisée" ("M-471_71 - Toiture végétalisée - Type 1" 5., "M-271_20 - Forme de Pente" 13., "M-279_01 - Toiture Isolation - Type 1" 12.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 660mm" | object type "RA232_Stru - Poutre rectangulaire:350 x 660mm" | names: "RA232_Stru - Poutre rectangulaire:350 x 660mm:3040480" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:500 x 560mm" | object type "RA232_Stru - Poutre rectangulaire:500 x 560mm" | names: "RA232_Stru - Poutre rectangulaire:500 x 560mm:3040483" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 500mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 500mm:3040485" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3060094", "Basic Wall:RA280 - Stru - Prémur béton - 350mm:3060096" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 270mm:3060095", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:3299083", "Basic Wall:RA280 - Stru - Prémur béton - 270mm:5983228" (+2 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3060099", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3060101", "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3299086" (+1 more) | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:3060105" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          21 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:3060107", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5894910", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm:5895021" (+18 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | object type "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | names: "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:3060108" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure" | object type "RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure" | names: "RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure:3242203" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 220mm:3299084" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Beton Arme - 200mm" | object type "Basic Wall:RA280 - Stru - Beton Arme - 200mm" | names: "Basic Wall:RA280 - Stru - Beton Arme - 200mm:3299087" | material: layers "Basic Wall:RA280 - Stru - Beton Arme - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCBEAM | type IFCBEAMTYPE "HE-M:HEM300" | object type "HE-M:HEM300" | names: "HE-M:HEM300:3360206", "HE-M:HEM300:3360208", "HE-M:HEM300:3360210" (+4 more) | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 160 mm" | object type "Floor:RA232_Stru - Béton générique - 160 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 160 mm:3360218" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | object type "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 260 mm:3432541", "Floor:RA232_Stru - Béton générique - 260 mm:7061877" | material: "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | object type "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | names: "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256040" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | object type "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | names: "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256182" | material: "<Unnamed>" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm" | object type "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm" | names: "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm:5896747", "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm:5896840", "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm:7186814" (+3 more) | material: layers "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm" ("M-279_610 - Isolation Accoustique Ext" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA239 - Etanchéité - 10mm" | object type "Basic Wall:RA239 - Etanchéité - 10mm" | names: "Basic Wall:RA239 - Etanchéité - 10mm:5985075", "Basic Wall:RA239 - Etanchéité - 10mm:5985123", "Basic Wall:RA239 - Etanchéité - 10mm:5985161" (+4 more) | material: layers "Basic Wall:RA239 - Etanchéité - 10mm" ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)" 1.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" | object type "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" | names: "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm:5985328", "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm:5985476", "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm:5985516" (+3 more) | material: layers "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)" 1., "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" | object type "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" | names: "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm:5985387" | material: layers "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)" 1., "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCROOF | type IFCTYPEPRODUCT "Basic Roof:Générique - 250 mm - Toiture Gravier" | object type "Basic Roof:Générique - 250 mm - Toiture Gravier" | names: "Basic Roof:Générique - 250 mm - Toiture Gravier:6917626" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 250 mm - Toiture Gravier" ("M-471_71 - Lestage en Gravier - Type 1" 5., "M-271_20 - Forme de Pente" 13., "M-279_01 - Toiture Isolation - Type 1 - 120mm" 12.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          5 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | object type "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 200mm:6918044", "Floor:RA232_Stru - Béton générique - 200mm:7469093", "Floor:RA232_Stru - Béton générique - 200mm:7469305" (+2 more) | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.); "M-280_02 - Beton Arme" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x 520mm" | object type "RA232_Stru - Poutre rectangulaire:400 x 520mm" | names: "RA232_Stru - Poutre rectangulaire:400 x 520mm:7136367" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 400mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 400mm:7259917" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          6 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE200A" | object type "H-Wide Flange Beams:HE200A" | names: "H-Wide Flange Beams:HE200A:7297145", "H-Wide Flange Beams:HE200A:7297489", "H-Wide Flange Beams:HE200A:7297506" (+3 more) | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7457323", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7474676" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7459481" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 1110mm:7460037" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | object type "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | names: "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7715706", "Basic Wall:RA280 - Stru - Prémur béton - 300mm:7716824" | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "60-009" | long name "-" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890869", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5890876" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-026" | long name "SALLE DE REUNION" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7056107" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-010" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Roof Drain:380 mm Strainer - 200 mm Drain" | object type "M_Roof Drain:380 mm Strainer - 200 mm Drain" | names: "M_Roof Drain:380 mm Strainer - 200 mm Drain:3625708" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-011" | long name "-" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5891023", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7750004" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-012" | long name "-" | INTERNAL
        IFCSPACE "60-001" | long name "ASC. 1" | INTERNAL
        IFCSPACE "60-033" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5858522" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-003" | long name "ESC. 1" | INTERNAL
        IFCSPACE "60-013" | long name "-" | INTERNAL
        IFCSPACE "60-006" | long name "STOCKAGE" | INTERNAL
        IFCSPACE "60-027" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "60-014" | long name "-" | INTERNAL
        IFCSPACE "60-028" | long name "SALLE DE REUNION" | INTERNAL
        IFCSPACE "60-015" | long name "LOCAL ENTRETIENT" | INTERNAL
        IFCSPACE "60-002" | long name "ASC. 2" | INTERNAL
        IFCSPACE "60-030" | long name "LOCAL DATA" | INTERNAL
        IFCSPACE "60-016" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7749664" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-017" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7749704" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-018" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5891538" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-019" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5858474" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-004" | long name "ESC. 2" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | object type "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | names: "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm:3294467" | material: materials ("<Unnamed>", "M-310_01 - Chassis Exutoire - Type 1") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-020" | long name "-" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5891002", "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:5891009" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-021" | long name "-" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | object type "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot:7056173" | material: layers "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" ("M-000_Par défaut" 23.399999999999999, "M-000_Panneau de plafond 600 x 1800" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7193998" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | object type "A678_RA_Hydrant:Type 1" | names: "A678_RA_Hydrant:Type 1:7227101" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-022" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5858466" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-023" | long name "-" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5858458" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
        IFCSPACE "60-007" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "60-034" | long name "SAS" | INTERNAL
        IFCSPACE "60-031" | long name "WC FEMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919813" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451487" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-005" | long name "PMR" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:5858483" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451486" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-032" | long name "WC HOMMES" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:6919825" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | object type "BE_621 Prise avec Terre:Type 1" | names: "BE_621 Prise avec Terre:Type 1:7451490" | material: "White - Plastic" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "60-008" | long name "RANGEMENTS" | INTERNAL
        IFCSPACE "60-024" | long name "T3" | INTERNAL
        IFCSPACE "60-025" | long name "-" | INTERNAL
        IFCSPACE "60-035" | long name "SAS" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | object type "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | names: "Compound Ceiling:Quadrillage 600 x 600 mm:7055722" | material: layers "Compound Ceiling:Quadrillage 600 x 600 mm" ("M-000_Par défaut" 1.8999999999999999, "M-000_Panneau de plafond 600 x 600" 1.6000000000000001) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "FFL-T0" | long name "FFL-T0" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 2595.0000000000014
        contains 109 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 250mm" | object type "Floor:RA239_Finition - sol _faux plancher - 250mm" | FLOOR | names: "Floor:RA239_Finition - sol _faux plancher - 250mm:2920584" | material: layers "Floor:RA239_Finition - sol _faux plancher - 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-000_000_Div. Vides - Air" 34.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          70 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat" | object type "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat" | names: "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat:3298961", "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat:3298967", "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat:3298977" (+67 more) | material: "Default" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:3300392", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:5894413", "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:6992271" (+2 more) | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 150mm" | object type "Floor:RA232_Stru - Béton générique - 150mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 150mm:5894548", "Floor:RA232_Stru - Béton générique - 150mm:6339974" | material: layers "Floor:RA232_Stru - Béton générique - 150mm" ("M-280_02 - Beton Arme" 15.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | object type "RA_A-570_Ventelles:Occurence" | names: "RA_A-570_Ventelles:Occurence:7286462" | material: materials ("A-570_Grille de ventilation en aluminium de teinte - RAL 7039", "A-570_Châssis en aluminium de teinte - RAL 7039") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "CFCHS139.7X4.0 139 x 140" | object type "COLUMN" | names: "PI - Poteau métallique" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          4 x IFCBEAM | type IFCBEAMTYPE "CFCHS139.7X4.0 139 x 140" | object type "BEAM" | names: "PI - Poutre Métallique" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | object type "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | names: "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm:7456277" | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7707129" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | object type "RA232_Stru - Poutre rectangulaire:270 x 600mm" | names: "RA232_Stru - Poutre rectangulaire:270 x 600mm:7709543" | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCGRID | names: "Default Grid"
          2 x IFCSLAB | type IFCSLABTYPE "Floor:RA479_Roof-edge-60" | object type "Floor:RA479_Roof-edge-60" | FLOOR | names: "Floor:RA479_Roof-edge-60:3027473", "Floor:RA479_Roof-edge-60:6205317" | material: layers "Floor:RA479_Roof-edge-60" ("M-479_RoofFin-mpx" 1.8, "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 720/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 720/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 720/100:3027656" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm" | object type "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm" | names: "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm:3241961", "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm:4255900", "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm:6997178" (+1 more) | material: layers "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm" ("M-476_00 - Couverture Metallique" 0.5, "M-411_10 - Isolation Exterieure en Facade" 14., "M-476_00 - Couverture Metallique" 0.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm" | object type "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm" | names: "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm:3241993", "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm:3242028", "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm:6997230" (+2 more) | material: layers "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm" ("M-476_00 - Couverture Metallique" 0.5, "M-411_10 - Isolation Exterieure en Facade" 14., "M-476_00 - Couverture Metallique" 0.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCROOF | object type "Basic Roof:Générique - 180 mm" | names: "Basic Roof:Générique - 180 mm:3299207" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 180 mm" ("M-279_01 - Toiture Isolation - Type 1" 12., "M-271_20 - Forme de Pente" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:Générique - 300 mm" | names: "Basic Roof:Générique - 300 mm:6205280" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 300 mm" ("M-279_01 - Toiture Isolation - Type 1" 18., "M-271_20 - Forme de Pente" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:Générique - 100mm" | names: "Basic Roof:Générique - 100mm:6205291" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 100mm" ("M-280_02 - Beton Arme" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 90/300" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 90/300" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 90/300:6205326" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 520/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 520/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 520/100:7437604" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 420/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 420/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 420/100:7437695" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "70-002" | long name "ESC. 1" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | object type "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | names: "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm:3285337" | material: materials ("<Unnamed>", "M-310_01 - Chassis Exutoire - Type 1") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "70-004" | long name "Room" | INTERNAL
        IFCSPACE "70-003" | long name "PAC" | INTERNAL
        IFCSPACE "70-001" | long name "Chaudière" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BLUEKIT_360x360:BLUEKIT_360x360" | object type "BLUEKIT_360x360:BLUEKIT_360x360" | names: "BLUEKIT_360x360:BLUEKIT_360x360:7282930" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "FFL-T1" | long name "FFL-T1" | object type "Level:SY_M_Marqueur de niveau FINI" | elevation 2825.
        contains 5 elements
          1 x IFCROOF | type IFCTYPEPRODUCT "Basic Roof:Générique - 250 mm - Toiture Gravier" | object type "Basic Roof:Générique - 250 mm - Toiture Gravier" | names: "Basic Roof:Générique - 250 mm - Toiture Gravier:2474296" | parts: 1 IFCSLAB | material: layers "Basic Roof:Générique - 250 mm - Toiture Gravier" ("M-471_71 - Lestage en Gravier - Type 1" 5., "M-271_20 - Forme de Pente" 13., "M-279_01 - Toiture Isolation - Type 1 - 120mm" 12.) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 150mm" | object type "Floor:RA232_Stru - Béton générique - 150mm" | FLOOR | names: "Floor:RA232_Stru - Béton générique - 150mm:5894734" | material: layers "Floor:RA232_Stru - Béton générique - 150mm" ("M-280_02 - Beton Arme" 15.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCGRID | names: "Default Grid"
          1 x IFCSLAB | type IFCSLABTYPE "Floor:RA479_Roof-edge-60" | object type "Floor:RA479_Roof-edge-60" | FLOOR | names: "Floor:RA479_Roof-edge-60:7435811" | material: layers "Floor:RA479_Roof-edge-60" ("M-479_RoofFin-mpx" 1.8, "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 150/100" | object type "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 150/100" | names: "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 150/100:7455492" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff

Types
  IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" | STANDARD | 199 occurrences | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" ("M-220_01 - Maconnerie interieure - Type 1" 14.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:2408949, RA325_001:GO 215/91 - Panneau 211/83:2408949:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/111 - Panneau 211/103" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/111 - Panneau 211/103:2409035, RA325_001:GO 215/111 - Panneau 211/103:2409035:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 2 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:2409059, RA325_001:GO 215/91 - Panneau 211/83:2409059:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:2409165, RA325_001:GO 215/101 - Panneau 211/93 - EI30:2409165:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm" | STANDARD | 2 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 1x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" | STANDARD | 91 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS125 2x2F - 125mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" | STANDARD | 40 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison Stratifié - 25mm" ("M-223_20 - Cloison Legere" 2.5) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | 21 occurrences | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/73:2410896, RA325_081_Menuiserie:Panneau 211/73:2410896:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:2448277, RA325_001:GO 215/101 - Panneau 211/93 - EI30:2448277:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | 20 occurrences | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/73:2712335, RA325_081_Menuiserie:Panneau 211/73:2712335:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCTYPEPRODUCT "Precast Stair:Precast Stair" | 14 occurrences
  IFCDOORSTYLE "RA325_101:GO 215/195 - Panneau 211/2x113 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_101:GO 215/195 - Panneau 211/2x113 - EI30:3143287, RA325_101:GO 215/195 - Panneau 211/2x113 - EI30:3143287:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:3228196, RA325_001:GO 215/101 - Panneau 211/93 - EI30:3228196:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | 1 occurrence | material: "<Unnamed>"
  IFCTYPEPRODUCT "Precast Stair:Precast Stair" | 1 occurrence
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 2 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:4014754, RA325_001:GO 215/101 - Panneau 211/93 - EI30:4014754:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30:4024486, RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30:4024486:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:4230325, RA325_001:GO 215/101 - Panneau 211/93 - EI30:4230325:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241753, RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241753:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241756, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241756:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA239_Finition - Sous-sol 2 - 140mm" | FLOOR | 2 occurrences | material: layers "Floor:RA239_Finition - Sous-sol 2 - 140mm" ("M-430_01 - Sol Finition Gén Type 2" 1.5, "M-431_01 - Chape Type 1" 9.5, "M-239_01 - Isolation Sol Int - Type 1" 3., "M-431_01 - Natte drainante - Type 1" 3.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS75 Iso 1x2F - 75mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-219_610 - Isolation résistant à l'humidité - 60mm" 5.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Finition Carrelage" | STANDARD | 148 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Finition Carrelage" ("M-000_Render Material 127-127-0" 1.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/113 - EI30 2" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/113 - EI30 2:6334040, RA325_001:GO 215/101 - Panneau 211/113 - EI30 2:6334040:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA239_Finition - Sous-sol - 110mm" | FLOOR | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:6874632, RA325_001:GO 215/91 - Panneau 211/83:6874632:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | 8 occurrences | material: "<Unnamed>"
  IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" | STANDARD | 10 occurrences | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm" ("M-320_01 - Porte - Panneau Type 1" 2.1999999999999997) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194089, RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194089:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 7 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194880, RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194880:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/63" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/63:7494362, RA325_081_Menuiserie:Panneau 211/63:7494362:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA220 -Panneau - Type 1 - 22 mm 2" ("M-353_03 - Faux-Plafond - Type 3" 9.5) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Walls 3:Walls 3" | 1 occurrence | material: "M-000_Béton, coulé sur place" | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWINDOWSTYLE "Windows 1:Windows 1" | 1 occurrence | material: "A-000_Poche" | property sets: Windows 1:Windows 1:7130245, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:RA2xx_ isolant - Mitoyen" | STANDARD | 11 occurrences | material: layers "Basic Wall:RA2xx_ isolant - Mitoyen" ("M-359_21 - Isolation en panneau - PIR - 160mm" 5.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 220mm" | STANDARD | 51 occurrences | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 220mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 10., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 350mm" | STANDARD | 33 occurrences | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 350mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 23., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:350 x 700mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:350 x 700mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 200mm" | FLOOR | 36 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:350 x 350mm" | COLUMN | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:700 x 700mm" | 1 occurrence | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 460mm" | 6 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" | STANDARD | 6 occurrences | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 190mm" ("M-220_01 - Maconnerie interieure - Type 1" 19.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" | STANDARD | 15 occurrences | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 1 - 100mm" ("M-220_01 - Maconnerie interieure - Type 1" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" | STANDARD | 125 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS180 2x2F - 175mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 12.5, "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" | STANDARD | 3 occurrences | material: layers "Basic Wall:RA221 - Mur Ext BETON - Préfab Iso - 260mm" ("M-280_02 - Beton Arme" 10., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 300mm" | STANDARD | 41 occurrences | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 300mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 18., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Beton Arme - 200mm" | STANDARD | 2 occurrences | material: layers "Basic Wall:RA280 - Stru - Beton Arme - 200mm" ("M-280_02 - Beton Arme" 20.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 660mm" | FLOOR | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 260 mm" | FLOOR | 11 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 260 mm" ("M-280_02 - Beton Arme" 26.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 800mm" | FLOOR | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 500mm" | FLOOR | 3 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 500mm" ("M-280_02 - Beton Arme" 50.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 140mm" ("M-220_11 - Maconnerie interieure Portante - Type 1" 14.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 860mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 860mm" ("M-280_02 - Beton Arme" 86.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 350mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 350mm" ("M-280_02 - Beton Arme" 35.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 250mm" | FLOOR | 2 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 250mm" ("M-280_02 - Beton Arme" 25.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Prémur béton - 270mm" | STANDARD | 85 occurrences | material: layers "Basic Wall:RA280 - Stru - Prémur béton - 270mm" ("M-280_03 - Element en Beton Prefabrique" 6., "M-280_02 - Beton Arme" 15., "M-280_03 - Element en Beton Prefabrique" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 140mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 140mm" ("M-280_02 - Beton Arme" 14.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1200mm" | 1 occurrence | property sets: Pset_BeamCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 820mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 820mm" ("M-280_02 - Beton Arme" 82.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm" | CEILING | 72 occurrences | property sets: Pset_CoveringCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | 21 occurrences | material: "White - Plastic"
  IFCBUILDINGELEMENTPROXYTYPE "BE_621 Prise avec Terre:Type 1" | 1 occurrence | material: "White - Plastic"
  IFCCOVERINGTYPE "Compound Ceiling:Heracklith" | CEILING | 6 occurrences | property sets: Pset_CoveringCommon, Pset_ManufacturerTypeInformation
  IFCDISTRIBUTIONELEMENTTYPE "F 83_005b1:F 83_005b 2" | 4 occurrences | material: "Matériau du rendu 255-255-255"
  IFCDISTRIBUTIONELEMENTTYPE "F 83_005b1:F 83_005b 2" | 4 occurrences | material: "Matériau du rendu 255-255-255"
  IFCCURTAINWALLTYPE "Curtain Wall:RA214 - Mur-rideau Ex Rez - 34 mm" | 4 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 300mm" | FLOOR | 2 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 300mm" ("M-280_02 - Beton Arme" 30.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Standard" | 6 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Curtain Wall:171_CW_Secant Piled Wall 530mm" | 9 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" | STANDARD | 10 occurrences | material: layers "Basic Wall:RA220 - Mur Porteur - Blocs - Type 1 - 190mm" ("M-220_11 - Maconnerie interieure Portante - Type 1" 19.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:2418414, RA325_001:GO 215/101 - Panneau 211/93 - EI30:2418414:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:2553776, RA325_001:GO 215/101 - Panneau 211/93 - EI30:2553776:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCTYPEPRODUCT "Cast-In-Place Stair:A-245_Escalier_Int - Béton_Escalier monobloc" | 1 occurrence
  IFCWALLTYPE "Basic Wall:RA280 - Stru - Beton Arme - 250mm" | STANDARD | 11 occurrences | material: layers "Basic Wall:RA280 - Stru - Beton Arme - 250mm" ("M-280_02 - Beton Arme" 25.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA220 - Mur Ext Plinthe BETON - Type 1 - 100mm" ("M-280_02 - Beton Arme" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "RA325_101:GO 205/155 - Panneau 201/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_101:GO 205/155 - Panneau 201/2x83 - EI30:3360772, RA325_101:GO 205/155 - Panneau 201/2x83 - EI30:3360772:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:3439274, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:3439274:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:3456848, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:M-419_01 - Couvre-murs - Type 1" | STANDARD | 1 occurrence | material: layers "Basic Wall:M-419_01 - Couvre-murs - Type 1" ("M-419_01 - Couvre-murs - Type 1" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M-340_Railing - Teinte gris clair" | STANDARD | 1 occurrence | material: layers "Basic Wall:M-340_Railing - Teinte gris clair" ("M-340_Railing - Teinte gris clair" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M-214_01 - Mur rideau - Type 1" | STANDARD | 1 occurrence | material: layers "Basic Wall:M-214_01 - Mur rideau - Type 1" ("M-214_01 - Mur rideau - Type 1" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "RA325_001:GO 215/131 - Panneau 211/123 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/131 - Panneau 211/123 - EI30:4018414, RA325_001:GO 215/131 - Panneau 211/123 - EI30:4018414:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93:4019852, RA325_001:GO 215/101 - Panneau 211/93:4019852:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA239_Finition - Sol Rez - 200 mm" | FLOOR | 4 occurrences | material: layers "Floor:RA239_Finition - Sol Rez - 200 mm" ("M-431_01 - Chape Type 2 - 8cm" 8., "M-431_01 - Insulit BI+9 - Type 1" 1., "M-431_01 - Chape Type 1 - 6cm" 6., "M-239_01 - Isolation Sol Int - Type 1" 5.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033562, RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033562:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93 - EI30:7090900, RA325_011:GO 215/101 - Panneau 211/93 - EI30:7090900:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 600mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 600mm" ("M-280_02 - Beton Arme" 60.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 1000mm" | FLOOR | 1 occurrence | material: layers "Floor:RA232_Stru - Béton générique - 1000mm" ("M-280_02 - Beton Arme" 100.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 7 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192092, RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192092:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192265, RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192265:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:7207360, RA325_001:GO 215/91 - Panneau 211/83 - EI30:7207360:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | 1 occurrence | property sets: Pset_BeamCommon
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "M_Footing-Rectangular:1000 x 1000 x 600mm" | 1 occurrence | material: "M-280_02 - Beton Arme"
  IFCTYPEPRODUCT "Foundation Slab:Radier 1000mm" | 2 occurrences | material: layers "Foundation Slab:Radier 1000mm" ("M-280_02 - Beton Arme" 100.)
  IFCTYPEPRODUCT "Foundation Slab:Radier 1590mm" | 2 occurrences | material: layers "Foundation Slab:Radier 1590mm" ("M-280_02 - Beton Arme" 159.)
  IFCTYPEPRODUCT "Foundation Slab:Radier 1500mm" | 1 occurrence | material: layers "Foundation Slab:Radier 1500mm" ("M-280_02 - Beton Arme" 150.)
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:500mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCTYPEPRODUCT "M_Pile-Steel Pipe:600mm Diameter" | 1 occurrence | material: "Steel, 45-345"
  IFCSLABTYPE "Floor:RA232_Stru - Empierrement - 300mm" | FLOOR | 3 occurrences | material: layers "Floor:RA232_Stru - Empierrement - 300mm" ("M-940 - Site - Empierrement" 30.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 600 mm - 100mm" | CEILING | 8 occurrences | property sets: Pset_CoveringCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7552905, RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7552905:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7553261, RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7553261:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 38 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7572881, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7572893, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7572899, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 3 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7574304, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7574310, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7578011, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7578088, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7578094, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7578100, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7578385, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair" | 9 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_04 - Panneautage - Type 1" | property sets: RA319_Glass Ext:Type 1:7581970, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7582174, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7589053, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7589243, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 1 occurrence | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:7589266, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 430mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" | STANDARD | 219 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" ("M-210_01 - Maconnerie de parement - Type 1" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 4:Generic Models 1" | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique"
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" | STANDARD | 31 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 1 - 280mm" ("M-210_01 - Maconnerie de parement - Type 1" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" | STANDARD | 11 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - BARDAGE BRIQUE - Type 2 - 280mm" ("M-210_02 - Maconnerie de parement - Type 2" 10., "M-000_000_Div. Vides - Air" 2., "M-359_21 - Isolation en panneau - PIR - 160mm" 16.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Arial 600 mm" | 2 occurrences | property sets: Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 320mm" | FLOOR | 4 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 320mm" ("M-280_02 - Beton Arme" 32.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | 7 occurrences | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" | STANDARD | 37 occurrences | material: layers "Basic Wall:RA220 - Mur Non Porteur - Blocs - Type 4 - 140mm" ("M-220_04 - Maconnerie interieure - Type 4" 14.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 940mm" | 3 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x720mm" | 5 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 520mm" | 7 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 400mm" | 7 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:600 x 720mm" | 1 occurrence | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | 1 occurrence | material: "<Unnamed>"
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:2523204, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:2523204:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Sloped Glazing:Vitres inclinées" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 59 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:2868730, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | 12 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al):Type 1:2868731, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | 59 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Type 1:2868732, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | 47 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al):Type 1:2869126, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 94 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:2957181, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 94 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:2957183, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 24 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2957229, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 24 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2957231, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 29 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:2958738, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | 17 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al):Type 1:2958739, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | 29 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Type 1:2958740, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 34 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:2958782, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 34 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:2958784, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | 12 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al):Type 1:2962262, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 28 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2962307, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 28 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2962309, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 4 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:2999363, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 4 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:2999364, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 4 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:2999365, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2999366, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:2999367, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 4 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:3002496, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 6 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:3002497, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 6 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:3002498, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 4 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:3052412, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 4 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:3052413, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 4 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:3052414, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:3052415, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:3052416, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 4 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:3281271, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al):Type 1" | 4 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al):Type 1:3281272, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 4 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:3281273, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 8 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:3281275, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 8 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:3281277, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:RA213 - CW_Cloison vitrée - Type BEDDELEM" | 40 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/131 - Panneau 211/123 - EI30:3395756, RA325_011:GO 215/131 - Panneau 211/123 - EI30:3395756:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 4 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:3448159, RA325_001:GO 215/101 - Panneau 211/93 - EI30:3448159:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" | STANDARD | 22 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 1x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 7.5) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 6 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:3453525, RA325_011:GO 215/101 - Panneau 211/93:3453525:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | 6 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93:3453526, RA325_001:GO 215/101 - Panneau 211/93:3453526:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:3453527, RA325_011:GO 215/101 - Panneau 211/93:3453527:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83 - EI30" | 5 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83 - EI30:3988353, RA325_001:GO 215/91 - Panneau 211/83 - EI30:3988353:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/91 - Panneau 211/83:4022828, RA325_011:GO 215/91 - Panneau 211/83:4022828:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 6 occurrences | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4240844, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4240844:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93 - EI30" | 6 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93 - EI30:4240846, RA325_011:GO 215/101 - Panneau 211/93 - EI30:4240846:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | 2 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/91 - Panneau 211/83:4240847, RA325_011:GO 215/91 - Panneau 211/83:4240847:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 6 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:3002831, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 6 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:3002832, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 370mm" | FLOOR | 6 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93" | 6 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93:4385130, RA325_001:GO 215/101 - Panneau 211/93:4385130:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | 37 occurrences | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: RA319_Wall-Mullion:Brick:4833578, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Wall-Mullion:Brick" | 59 occurrences | material: "M-210_01 - Maconnerie de parement - Type 1" | property sets: RA319_Wall-Mullion:Brick:4833615, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 4 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:4833995, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-2x(OB+Al)_Asym:Type 1" | 4 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4833996, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Type 1" | 4 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Type 1:4833997, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4833998, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4834000, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5477771, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5477772, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 29 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5512232, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 29 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5512233, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 59 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5512294, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 59 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5512295, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5514679, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5514680, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 6 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5550800, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 6 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5550801, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5550828, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5550829, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | 19 occurrences | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5869635, RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5869635:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" | FLOOR | 4 occurrences | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 120mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 12.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:RA239_Finition - sol _ Carrelage- 250mm" | FLOOR | 6 occurrences | material: layers "Floor:RA239_Finition - sol _ Carrelage- 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-431_01 - Chape Type 1" 12., "Matériau du rendu 0-0-0" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:6181282, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:6181376, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM" | 17 occurrences | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870877, RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870877:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS75 1x2F - 75mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 2 occurrences | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" | STANDARD | 38 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - BRIQUE - TYPE 2 - 100mm" ("M-210_02 - Maconnerie de parement - Type 2" 10.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCRAILINGTYPE "Railing:A340_RA_Railing - Full - H1000mm" | 11 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_RailingCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1210mm" | 3 occurrences | property sets: Pset_BeamCommon
  IFCCOVERINGTYPE "Compound Ceiling:Quadrillage 600 x 1800 mm - Ilot" | CEILING | 59 occurrences | property sets: Pset_CoveringCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "A678_RA_Hydrant:Type 1" | 6 occurrences | material: "<Unnamed>"
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:4027764, RA325_001:GO 215/101 - Panneau 211/93 - EI30:4027764:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7017670, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7017670:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/91 - Panneau 211/83" | 4 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/91 - Panneau 211/83:4218419, RA325_011:GO 215/91 - Panneau 211/83:4218419:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/131 - Panneau 211/123 - EI30:7079569, RA325_011:GO 215/131 - Panneau 211/123 - EI30:7079569:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 5 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:6280575, RA325_011:GO 215/101 - Panneau 211/93:6280575:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:700 x 700mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:600 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique -320mm" | FLOOR | 4 occurrences | material: layers "Floor:RA232_Stru - Béton générique -320mm" ("M-280_02 - Beton Arme" 32.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 4 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:2479118, RA325_011:GO 215/101 - Panneau 211/93:2479118:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:2479822, RA325_011:GO 215/101 - Panneau 211/93:2479822:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_111:GO 215/175 - Panneau 211/2x83 - EI30" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4217677, RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4217677:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | 2 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/131 - Panneau 211/123 - EI30:4217684, RA325_011:GO 215/131 - Panneau 211/123 - EI30:4217684:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 3 occurrences | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:4241308, RA325_001:GO 215/91 - Panneau 211/83:4241308:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_200_PorteSimple_Coulissante:201/1x93" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_200_PorteSimple_Coulissante:201/1x93:5837747, RA325_200_PorteSimple_Coulissante:201/1x93:5837747:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 4 occurrences | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:7753120, RA325_011:GO 215/101 - Panneau 211/93:7753120:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "RA325_011:GO 215/101 - Panneau 211/93" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/101 - Panneau 211/93:2497172, RA325_011:GO 215/101 - Panneau 211/93:2497172:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/101 - Panneau 211/93 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/101 - Panneau 211/93 - EI30:4219135, RA325_001:GO 215/101 - Panneau 211/93 - EI30:4219135:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_200_PorteSimple_Coulissante:201/1x93" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_200_PorteSimple_Coulissante:201/1x93:5839206, RA325_200_PorteSimple_Coulissante:201/1x93:5839206:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_081_Menuiserie:Panneau 211/73" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_081_Menuiserie:Panneau 211/73:6288169, RA325_081_Menuiserie:Panneau 211/73:6288169:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:500 x 620mm" | 3 occurrences | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "H-Wide Flange Beams:HE450AA" | 2 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 300mm" | FLOOR | 3 occurrences | material: layers "Floor:RA239_Finition - Sol terrasse - 300mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA239 - Fin Ext - Etanchéité + Isolant - 140mm" ("M-479_02 - FinExt - Plaque type1" 4., "M-000_000_Div. Vides - Air" 4., "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 1110mm" | 3 occurrences | property sets: Pset_BeamCommon
  IFCDOORSTYLE "RA325_011:GO 215/111 - Panneau 211/103" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/111 - Panneau 211/103:2701285, RA325_011:GO 215/111 - Panneau 211/103:2701285:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:RA479_Roof-edge-60" | FLOOR | 6 occurrences | material: layers "Floor:RA479_Roof-edge-60" ("M-479_RoofFin-mpx" 1.8, "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" | 3 occurrences | property sets: Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220066, RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220066:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 7 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4375558, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 13 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4375564, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 7 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4375565, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 41 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4375721, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 45 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4375723, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 41 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4375725, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 41 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:4376201, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 7 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:4376350, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-stone:RA_Windows_Sill" | 6 occurrences | material: "M-313_14 - Seuil de Porte en Beton" | property sets: RA319_Window-sill-stone:RA_Windows_Sill:4377019, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 6 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4377020, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 6 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4377029, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 26 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:4375824, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 3 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4377038, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 3 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4377044, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 3 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4377045, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 26 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:4377065, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 26 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4377066, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 26 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4377072, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 26 occurrences | material: "M-316_02 - Vitrage - Type 2" | property sets: RA319_Glass Ext:Type 1:4377073, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 3 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:4378028, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 26 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:4378045, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" | STANDARD | 8 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS155 1x2F - 155mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 13.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 33 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5550780, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 44 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5550865, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 33 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5587170, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 6 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5685850, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 44 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5685925, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 6 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5686404, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS63 1x1F - 63mm" ("M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCSLABTYPE "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" | FLOOR | 2 occurrences | material: layers "Floor:RA280_03 - Element en Beton Prefabrique - Escalier palier - 220mm" ("M-280_03 - Element en Beton Prefabrique - Escalier palier" 22.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCRAILINGTYPE "Railing:RA340_Railing Ext - Partiel - H1100mm" | 3 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_RailingCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 660mm" | 2 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "HE-M:HEM300" | 15 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 160 mm" | FLOOR | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "HE-A Column:HEA260" | COLUMN | 1 occurrence | material: "Structural Steel - S235" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA239 - Fin Ext - Etanchéité - 80mm" ("M-479_02 - FinExt - Plaque type1" 4., "M-000_000_Div. Vides - Air" 4.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCOLUMNTYPE "RA232_Stru - Colonne rectangulaire:500 x 600mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "RA232_Stru - Colonne carrée:500 x 500mm" | COLUMN | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:400 x 520mm" | 2 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:350 x 520mm" | 1 occurrence | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "H-Wide Flange Beams:HE200A" | 13 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam
  IFCBUILDINGELEMENTPROXYTYPE "M_Roof Drain:380 mm Strainer - 200 mm Drain" | 6 occurrences | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1" | 1 occurrence | material: "M-280_03 - Element en Beton Prefabrique"
  IFCSLABTYPE "Floor:RA239_Finition - Sol terrasse - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:RA239_Finition - Sol terrasse - 250mm" ("M-473_21 - Dalles sur Plots en Beton" 2., "M-000_000_Div. Vides - Air" 5., "M-279_02 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité" 6., "M-431_01 - Béton de pente - Type 2" 12.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "RA325_011:GO 215/111 - Panneau 211/103 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/111 - Panneau 211/103 - EI30:4220738, RA325_011:GO 215/111 - Panneau 211/103 - EI30:4220738:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 215/131 - Panneau 211/123 - EI30" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220745, RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220745:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:4220760, RA325_001:GO 215/91 - Panneau 211/83:4220760:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:4241687, RA325_001:GO 215/91 - Panneau 211/83:4241687:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_001:GO 215/91 - Panneau 211/83" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_001:GO 215/91 - Panneau 211/83:4287332, RA325_001:GO 215/91 - Panneau 211/83:4287332:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWSTYLE "RA319_Window-sill-stone:RA_Windows_Sill" | 4 occurrences | material: "M-313_14 - Seuil de Porte en Beton" | property sets: RA319_Window-sill-stone:RA_Windows_Sill:4377233, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 4 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:4377234, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 4 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:4377238, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5685797, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 4 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5686417, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:RA223 - Mur Int - Cloison MS100 2x2F - 100mm" ("M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25, "M-000_000_Div. Vides - Air" 5., "M-223_20 - Cloison Legere" 1.25, "M-223_20 - Cloison Legere" 1.25) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWINDOWSTYLE "RA319_Window-sill-brick:RA_Windows_Sill" | 2 occurrences | material: "M-313_21 - Seuil de Fenetre en Briques" | property sets: RA319_Window-sill-brick:RA_Windows_Sill:5965433, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA314_Window-frame-1x(OB+Al):Type 1" | 2 occurrences | material: "M-310_01 - Chassis - Type 1" | property sets: RA314_Window-frame-1x(OB+Al):Type 1:5965434, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:5965435, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Glass Ext:Type 1" | 2 occurrences | material: "M-316_01 - Vitrage - Type 1" | property sets: RA319_Glass Ext:Type 1:5965436, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-sill-int-standard:Tablette + ebrasement" | 2 occurrences | material: "M-313_41 - Tablette de Fenetre - Type 1" | property sets: RA311_Windows-sill-int-standard:Tablette + ebrasement:5965437, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA311_Windows-stretcher-steel:Type 1" | 2 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA311_Windows-stretcher-steel:Type 1:5965438, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWSTYLE "RA319_Windows-Lintel:Brick" | 2 occurrences | material: "M-313_21 - Linteau de Fenetre en Briques" | property sets: RA319_Windows-Lintel:Brick:5965439, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:RA313 - Window_Gris Clair - Vtrage Actif" | 3 occurrences | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "BLUEKIT_360x360:BLUEKIT_360x360" | 5 occurrences | material: "<Unnamed>"
  IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | 1 occurrence | material: materials ("A-570_Grille de ventilation en aluminium de teinte - RAL 7039", "A-570_Châssis en aluminium de teinte - RAL 7039") | property sets: RA_A-570_Ventelles:Occurence:7286130, Pset_WindowCommon
  IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | 1 occurrence | material: materials ("A-570_Châssis en aluminium de teinte - RAL 7039", "A-570_Grille de ventilation en aluminium de teinte - RAL 7039") | property sets: RA_A-570_Ventelles:Occurence:7287056, Pset_WindowCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCCOVERINGTYPE "Ceilings 1:Ceilings 1" | 1 occurrence
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:500 x 560mm" | 1 occurrence | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 500mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:3060108, RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:3060108:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure:3242203, RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure:3242203:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256040, RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256040:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORSTYLE "RA325_011:GO 205/91 - Panneau 201/83 / Extérieure" | 1 occurrence | material: "<Unnamed>" | property sets: RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256182, RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256182:1, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm" | STANDARD | 6 occurrences | material: layers "Basic Wall:RA273 - Mur Ext - Isolation Accoustique - 140 mm" ("M-279_610 - Isolation Accoustique Ext" 14.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA239 - Etanchéité - 10mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:RA239 - Etanchéité - 10mm" ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)" 1.) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" | STANDARD | 7 occurrences | material: layers "Basic Wall:RA210 - Isolant Ext - Etanchéité - 60mm" ("M-279_07 - Complexe d'Etancheite et d'Isolation - Etancheité (Remonté)" 1., "M-279_08 - Complexe d'Etancheite et d'Isolation - Isolation Haute densité (Remonté)" 6.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCTYPEPRODUCT "Basic Roof:Générique - 250 mm - Toiture Gravier" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | 1 occurrence | material: materials ("<Unnamed>", "M-310_01 - Chassis Exutoire - Type 1")
  IFCSLABTYPE "Floor:RA239_Finition - sol _faux plancher - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:RA239_Finition - sol _faux plancher - 250mm" ("M-430_01 - Sol Finition Gén Type 1" 3., "M-000_000_Div. Vides - Air" 34.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "A-615_RA_PanneauSolaire_ToitPlat:A-615_RA_PanneauSolaire_ToitPlat" | 70 occurrences | material: "Default"
  IFCSLABTYPE "Floor:RA232_Stru - Béton générique - 150mm" | FLOOR | 3 occurrences | material: layers "Floor:RA232_Stru - Béton générique - 150mm" ("M-280_02 - Beton Arme" 15.) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWINDOWSTYLE "RA_A-570_Ventelles:Occurence" | 1 occurrence | material: materials ("A-570_Grille de ventilation en aluminium de teinte - RAL 7039", "A-570_Châssis en aluminium de teinte - RAL 7039") | property sets: RA_A-570_Ventelles:Occurence:7286462, Pset_WindowCommon
  IFCCOLUMNTYPE "CFCHS139.7X4.0 139 x 140" | COLUMN | 4 occurrences | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "CFCHS139.7X4.0 139 x 140" | BEAM | 4 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RA232_Stru - Poutre rectangulaire:270 x 600mm" | BEAM | 1 occurrence | material: "M-280_02 - Beton Arme" | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 720/100" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique simple face - 150 mm" ("M-476_00 - Couverture Metallique" 0.5, "M-411_10 - Isolation Exterieure en Facade" 14., "M-476_00 - Couverture Metallique" 0.5) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm" | STANDARD | 5 occurrences | material: layers "Basic Wall:RA210 - Mur Ext - Panneau sandwich metalique double face- 150 mm" ("M-476_00 - Couverture Metallique" 0.5, "M-411_10 - Isolation Exterieure en Facade" 14., "M-476_00 - Couverture Metallique" 0.5) | property sets: Pset_ManufacturerTypeInformation, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 90/300" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 520/100" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 420/100" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "RA_A-374_Dome-standard:RA_A-374_Dome-standard - 1200/1200mm" | 1 occurrence | material: materials ("<Unnamed>", "M-310_01 - Chassis Exutoire - Type 1")
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:RA376_Couvre-murs en aluminium de teinte gris clair - 150/100" | 1 occurrence | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_AirSideSystemInformation | properties | on 41 objects (41 IFCSPACE)
    Name = "-" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 22 objects (22 IFCSPACE)
    Name = "SALLE DE REUNION" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 18 objects (18 IFCSPACE)
    Name = "SAS" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 14 objects (14 IFCSPACE)
    Name = "BUREAU" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 10 objects (10 IFCSPACE)
    Name = "ESC. 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 9 objects (9 IFCSPACE)
    Name = "RANGEMENTS" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 9 objects (9 IFCSPACE)
    Name = "LOCAL DATA" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 9 objects (9 IFCSPACE)
    Name = "STOCKAGE" (IFCLABEL)
  Pset_AirSideSystemInformation: 55 more contents on 130 objects not shown
  Pset_ProductRequirements | properties | on 41 objects (41 IFCSPACE)
    Name = "-" (IFCLABEL)
  Pset_ProductRequirements | properties | on 22 objects (22 IFCSPACE)
    Name = "SALLE DE REUNION" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (18 IFCSPACE)
    Name = "SAS" (IFCLABEL)
  Pset_ProductRequirements | properties | on 14 objects (14 IFCSPACE)
    Name = "BUREAU" (IFCLABEL)
  Pset_ProductRequirements | properties | on 10 objects (10 IFCSPACE)
    Name = "ESC. 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCSPACE)
    Name = "RANGEMENTS" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCSPACE)
    Name = "LOCAL DATA" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCSPACE)
    Name = "STOCKAGE" (IFCLABEL)
  Pset_ProductRequirements: 55 more contents on 130 objects not shown
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "N/A" (IFCLABEL)
    Reference = "T1 00-012" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "N/A" (IFCLABEL)
    Reference = "ASC. 1 00-001" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "CHAPE INDUSTRIELLE LISEE + QUARTZ" (IFCLABEL)
    Reference = "SAS 00-020" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "BETON BRUT" (IFCLABEL)
    Reference = "ESC. 1 00-005" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "N/A" (IFCLABEL)
    Reference = "ASC. 2 00-002" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "CHAPE INDUSTRIELLE LISEE + QUARTZ" (IFCLABEL)
    Reference = "BUREAU DE GESTION 00-003" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "CHAPE INDUSTRIELLE LISEE + QUARTZ" (IFCLABEL)
    Reference = "SALLE D'ENREGISTREMENT 00-019" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    FloorCovering = "CHAPE INDUSTRIELLE LISEE + QUARTZ" (IFCLABEL)
    Reference = "SAS ENTREE 00-022" (IFCIDENTIFIER)
  Pset_SpaceCommon: 244 more contents on 244 objects not shown
  Pset_QuantityTakeOff | properties | on 1328 objects (1328 IFCOPENINGELEMENT)
    Reference = "2080/1850_2(OB+AL)_NoSP_SillExBrick" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1179 objects (1140 IFCWINDOW, 38 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 533 objects (533 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_NoSillEx" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 459 objects (459 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_SillExBrick - VA" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 435 objects (435 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_SillExBrick" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 348 objects (348 IFCOPENINGELEMENT)
    Reference = "2080/1850_2(OB+AL)_NoSP_SillExBrick - VA" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 307 objects (307 IFCMEMBER)
    Reference = "A210_RA_IntJoinery-50x50" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 304 objects (304 IFCMEMBER)
    Reference = "Secant Pile 530mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 186 more contents on 4021 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 36 objects (36 IFCSLAB)
    Reference = "RA232_Stru - Béton générique - 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 29 objects (29 IFCSLAB)
    Reference = "Epaisseur 250 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 11 objects (11 IFCSLAB)
    Reference = "RA232_Stru - Béton générique - 260 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 7 objects (7 IFCSLAB)
    Reference = "RA239_Finition - Sol Rez - 200 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB)
    Reference = "RA239_Finition - sol _faux plancher - 370mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB)
    Reference = "RA479_Roof-edge-60" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB)
    Reference = "RA239_Finition - sol _ Carrelage- 250mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "RA232_Stru - Béton générique - 320mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 29 more contents on 48 objects not shown
  Pset_SlabCommon | properties | on 35 objects (35 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA232_Stru - Béton générique - 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 29 objects (29 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Epaisseur 250 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 11 objects (11 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA232_Stru - Béton générique - 260 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA239_Finition - sol _faux plancher - 370mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA479_Roof-edge-60" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA239_Finition - Sol Rez - 200 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA239_Finition - sol _ Carrelage- 250mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "RA232_Stru - Béton générique - 320mm" (IFCIDENTIFIER)
  Pset_SlabCommon: 31 more contents on 50 objects not shown
  Pset_OpeningElementCommon | properties | on 1328 objects (1328 IFCOPENINGELEMENT)
    Reference = "2080/1850_2(OB+AL)_NoSP_SillExBrick" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 533 objects (533 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_NoSillEx" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 459 objects (459 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_SillExBrick - VA" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 435 objects (435 IFCOPENINGELEMENT)
    Reference = "2080/900_1(OB+AL)_NoSP_SillExBrick" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 348 objects (348 IFCOPENINGELEMENT)
    Reference = "2080/1850_2(OB+AL)_NoSP_SillExBrick - VA" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 103 objects (103 IFCOPENINGELEMENT)
    Reference = "2080/850_1(OB+AL)_NoSP_NoSillEx" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 102 objects (102 IFCOPENINGELEMENT)
    Reference = "2830/900_1(OB+AL)_NoSP_SillExBéton Archi" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 95 objects (95 IFCOPENINGELEMENT)
    Reference = "2080/2250_1(OB+AL)_NoSP_SillExBrick - VA" (IFCIDENTIFIER)
  Pset_OpeningElementCommon: 43 more contents on 377 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 219 objects (218 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Reference = "RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 199 objects (166 IFCWALLSTANDARDCASE, 33 IFCWALL)
    Reference = "RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 148 objects (148 IFCWALLSTANDARDCASE)
    Reference = "RA223 - Mur Int - Finition Carrelage" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 125 objects (97 IFCWALLSTANDARDCASE, 28 IFCWALL)
    Reference = "RA223 - Mur Int - Cloison MS180 2x2F - 175mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 91 objects (86 IFCWALLSTANDARDCASE, 5 IFCWALL)
    Reference = "RA223 - Mur Int - Cloison MS125 2x2F - 125mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 85 objects (70 IFCWALLSTANDARDCASE, 15 IFCWALL)
    Reference = "RA280 - Stru - Prémur béton - 270mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 51 objects (49 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Reference = "RA280 - Stru - Prémur béton - 220mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 41 objects (38 IFCWALLSTANDARDCASE, 3 IFCWALL)
    Reference = "RA280 - Stru - Prémur béton - 300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 38 more contents on 353 objects not shown
  Pset_WallCommon | properties | on 219 objects (218 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA210 - Mur Ext - BRIQUE - TYPE 1 - 100mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 160 objects (137 IFCWALLSTANDARDCASE, 23 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA220 - Mur Non Porteur - Blocs - Type 1 - 140mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 148 objects (148 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA223 - Mur Int - Finition Carrelage" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 91 objects (86 IFCWALLSTANDARDCASE, 5 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA223 - Mur Int - Cloison MS125 2x2F - 125mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 69 objects (53 IFCWALLSTANDARDCASE, 16 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA223 - Mur Int - Cloison MS180 2x2F - 175mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 56 objects (44 IFCWALLSTANDARDCASE, 12 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA223 - Mur Int - Cloison MS180 2x2F - 175mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 52 objects (50 IFCWALLSTANDARDCASE, 2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA280 - Stru - Prémur béton - 270mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 44 objects (43 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "RA280 - Stru - Prémur béton - 220mm" (IFCIDENTIFIER)
  Pset_WallCommon: 55 more contents on 473 objects not shown
  Pset_CurtainWallCommon | properties | on 40 objects (40 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA213 - CW_Cloison vitrée - Type BEDDELEM" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 36 objects (36 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA220 -CW Panneau - Type 2 - 50 mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 9 objects (9 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "171_CW_Secant Piled Wall 530mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 9 objects (9 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA313 - Window_Gris Clair" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 6 objects (6 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA213 - CW_Cloison vitrée - Standard" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA214 - Mur-rideau Ex Rez - 34 mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA313 - Window_Gris Clair - Vtrage Actif" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA223 - Mur Int - Cloison Stratifié - 50mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon: 1 more content on 0 objects not shown
  Pset_PlateCommon | properties | on 62 objects (62 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA214 - 38mm glazing,triple - Vitrage Int" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 27 objects (27 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA314 - 38mm glazing, triple" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 7 objects (7 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Aluminium 3" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA314 - 38mm glazing, triple - Vitrage Actif" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 3 objects (3 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Aluminium 2" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Aluminium 3" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Aluminium 2" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "RA314 - 38mm glazing, triple - Vitrage Actif" (IFCIDENTIFIER)
  Pset_PlateCommon: 2 more contents on 2 objects not shown
  Pset_MemberCommon | properties | on 121 objects (121 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Secant Pile 530mm" (IFCIDENTIFIER)
    Span = 424.00000000002996 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 116 objects (116 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Secant Pile 530mm" (IFCIDENTIFIER)
    Span = 459.99999999999989 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 112 objects (112 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A210_RA_IntJoinery-50x50" (IFCIDENTIFIER)
    Span = 250. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 62 objects (62 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A214_RA_Meneau Vertical Blanc_140_ - RAL 9011" (IFCIDENTIFIER)
    Span = 130.00000000000006 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 40 objects (40 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A310_RA_ExtJoinery-65x65 Blanc - RAL 9010" (IFCIDENTIFIER)
    Span = 90.624999999999702 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 30 objects (30 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Secant Pile 530mm" (IFCIDENTIFIER)
    Span = 454.00000000002956 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 25 objects (25 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A310_RA_ExtJoinery-65x65 Blanc - RAL 9010" (IFCIDENTIFIER)
    Span = 174.99999999999994 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 25 objects (25 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A214_RA_Meneau Vertical Blanc_140_ - RAL 9011" (IFCIDENTIFIER)
    Span = 113.49999999999999 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon: 73 more contents on 357 objects not shown
  Pset_ConcreteElementGeneral | properties | on 141 objects (141 IFCDOOR) | on 34 type objects
    FireRating = "N/A" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 76 objects (76 IFCDOOR) | on 37 type objects
    FireRating = "30" (IFCLABEL)
  Pset_DoorCommon | properties | on 42 objects (42 IFCDOOR)
    FireRating = "N/A" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Panneau 211/73" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 37 objects (37 IFCDOOR)
    FireRating = "N/A" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/101 - Panneau 211/93" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 36 objects (36 IFCDOOR)
    FireRating = "N/A" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Panneau 211/93 - Type BEDDELEEM" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 29 objects (29 IFCDOOR)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/101 - Panneau 211/93 - EI30" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 22 objects (22 IFCDOOR)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/91 - Panneau 211/83 - EI30" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 17 objects (17 IFCDOOR)
    FireRating = "N/A" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/91 - Panneau 211/83" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 14 objects (14 IFCDOOR)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/175 - Panneau 211/2x83 - EI30" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GO 215/131 - Panneau 211/123 - EI30" (IFCIDENTIFIER)
  Pset_DoorCommon: 17 more contents on 18 objects not shown
  Pset_ColumnCommon | properties | on 24 objects (24 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "350 x 350mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 15 objects (15 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HEA260" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "500 x 600mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "500 x 500mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 5 objects (5 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "700 x 700mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 5 objects (5 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "600 x 600mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CFCHS139.7X4.0 139 x 140" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "350 x 700mm" (IFCIDENTIFIER)
  Pset_ColumnCommon: 1 more content on 0 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 24 objects (24 IFCCOLUMN)
    Reference = "350 x 350mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 15 objects (15 IFCCOLUMN)
    Reference = "HEA260" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 8 objects (8 IFCCOLUMN)
    Reference = "500 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 6 objects (6 IFCCOLUMN)
    Reference = "500 x 500mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 5 objects (5 IFCCOLUMN)
    Reference = "700 x 700mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 5 objects (5 IFCCOLUMN)
    Reference = "600 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 4 objects (4 IFCCOLUMN)
    Reference = "CFCHS139.7X4.0 139 x 140" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "350 x 700mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn: 1 more content on 0 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 23 objects (16 IFCSTAIR, 7 IFCROOF) | on 277 type objects
    Manufacturer = "Copyright © ReservoirA - all rights reserved" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 50.019604940707715 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Générique - 250 mm - Toiture Gravier" (IFCIDENTIFIER)
    TotalArea = 46.992004940709172 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 12.155429967626739 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Vitres inclinées" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 240.43789150285644 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Générique - 250 mm - Toiture Végétalisée" (IFCIDENTIFIER)
    TotalArea = 240.43789150285642 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.7085000000020889 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Générique - 180 mm" (IFCIDENTIFIER)
    TotalArea = 4.7085000000020871 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 9.1490165073897085 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Générique - 300 mm" (IFCIDENTIFIER)
    TotalArea = 9.1490165073897103 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 9.1490165073897103 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Générique - 100mm" (IFCIDENTIFIER)
    TotalArea = 9.1490165073897103 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Générique - 250 mm - Toiture Gravier" (IFCIDENTIFIER)
    TotalArea = 161.89323376169347 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_BuildingElementProxyCommon | properties | on 70 objects (70 IFCBUILDINGELEMENTPROXY)
    Reference = "A-615_RA_PanneauSolaire_ToitPlat" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 38 objects (38 IFCBUILDINGELEMENTPROXY)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Reference = "380 mm Strainer - 200 mm Drain" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "BLUEKIT_360x360" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "RA376_Couvre-murs en aluminium de teinte gris clair - 590/100" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "RA_A-374_Dome-standard - 1200/1200mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Arial 600 mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 5 more contents on 5 objects not shown
  Pset_StairCommon | properties | on 11 objects (11 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Precast Stair" (IFCIDENTIFIER)
    RiserHeight = 18.000000000000004 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 26. (IFCCOUNTMEASURE)
    Reference = "Precast Stair" (IFCIDENTIFIER)
    RiserHeight = 17.708333333333329 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    Reference = "Precast Stair" (IFCIDENTIFIER)
    RiserHeight = 18. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "A-245_Escalier_Int - Béton_Escalier monobloc" (IFCIDENTIFIER)
    RiserHeight = 17.333333333333336 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 8 objects (8 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 18.000000000000004 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 8 objects (8 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 18.000000000000004 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.9685039370078741 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 17.999999999999979 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 18.000000000000021 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 17.333333333333336 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 2.4688320209973025 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 17.708333333333329 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 17.708333333333332 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 3. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run - Int" (IFCIDENTIFIER)
    RiserHeight = 18. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 26. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.4763779527559056 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon: 7 more contents on 7 objects not shown
  Pset_WindowCommon | properties | on 1140 objects (1140 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 295 objects (295 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Brick" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 172 objects (172 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA_Windows_Sill" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 97 objects (97 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Tablette + ebrasement" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Occurence" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Windows 1" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 116 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BeamCommon | properties | on 13 objects (13 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE200A" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 270.00000000001137 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HEM300" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 822.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "600 x 460mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 788.54188340822259 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "270 x 500mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 259.25856225924065 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HEM300" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 759.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE450AA" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 937.49999999999193 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "400 x720mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 474.71184448602651 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "270 x 400mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 181.99999999999977 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon: 48 more contents on 72 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 19 objects (19 IFCBEAM)
    Reference = "270 x 500mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 15 objects (15 IFCBEAM)
    Reference = "HEM300" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 13 objects (13 IFCBEAM)
    Reference = "HE200A" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 10 objects (10 IFCBEAM)
    Reference = "270 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 8 objects (8 IFCBEAM)
    Reference = "HE450AA" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 7 objects (7 IFCBEAM)
    Reference = "600 x 520mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 7 objects (7 IFCBEAM)
    Reference = "270 x 400mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 6 objects (6 IFCBEAM)
    Reference = "600 x 460mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam: 15 more contents on 33 objects not shown
  Pset_CoveringCommon | properties | on 72 objects (72 IFCCOVERING)
    Finish = "M-000_Par défaut;M-000_Panneau de plafond 600 x 600;" (IFCTEXT)
    Reference = "Quadrillage 600 x 600 mm" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 59 objects (59 IFCCOVERING)
    Finish = "M-000_Par défaut;M-000_Panneau de plafond 600 x 1800;" (IFCTEXT)
    Reference = "Quadrillage 600 x 1800 mm - Ilot" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 8 objects (8 IFCCOVERING)
    Finish = "M-000_Panneau de plafond 600 x 600;" (IFCTEXT)
    Reference = "Quadrillage 600 x 600 mm - 100mm" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 6 objects (6 IFCCOVERING)
    Finish = "M-353_03 - Faux-Plafond - Type 3;" (IFCTEXT)
    Reference = "Heracklith" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Reference = "Ceilings 1" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 3.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 9.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 10. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon: 1 more content on 0 objects not shown
  Pset_DistributionFlowElementCommon | properties | on 8 objects (8 IFCFLOWTERMINAL)
    Reference = "F 83_005b 2" (IFCIDENTIFIER)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 44 objects (44 IFCFOOTING)
    Reference = "600mm Diameter" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 6 objects (6 IFCFOOTING)
    Reference = "1000 x 1000 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "Radier 1000mm" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "Radier 1590mm" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "Radier 1500mm" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "500mm Diameter" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 44 objects (44 IFCFOOTING)
    Reference = "600mm Diameter" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 6 objects (6 IFCFOOTING)
    Reference = "1000 x 1000 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "Radier 1000mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "Radier 1590mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "Radier 1500mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "500mm Diameter" (IFCLABEL)
  Pset_RailingCommon | properties | on 26 objects (26 IFCRAILING)
    Height = 75. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A340_RA_Railing - Full - H1000mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 18 objects (18 IFCRAILING)
    Height = 75. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "A340_RA_Railing - Lisse sup - H1000mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 3 objects (3 IFCRAILING)
    Height = 75. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RA340_Railing Ext - Partiel - H1100mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 10 objects (10 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 10 (IFCINTEGER)
  RA325_001:GO 215/91 - Panneau 211/83:2408949 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:2408949:1 | predefined | on 1 type object
  RA325_001:GO 215/111 - Panneau 211/103:2409035 | predefined | on 1 type object
  RA325_001:GO 215/111 - Panneau 211/103:2409035:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:2409059 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:2409059:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2409165 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2409165:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:2410896 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:2410896:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2448277 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2448277:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:2712335 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:2712335:1 | predefined | on 1 type object
  RA325_101:GO 215/195 - Panneau 211/2x113 - EI30:3143287 | predefined | on 1 type object
  RA325_101:GO 215/195 - Panneau 211/2x113 - EI30:3143287:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:3228196 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:3228196:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4014754 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4014754:1 | predefined | on 1 type object
  RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30:4024486 | predefined | on 1 type object
  RA325_141_NO_90°:GO 215/175 - Panneau 211/2x83 - EI30:4024486:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4230325 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4230325:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241753 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:4241753:1 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241756 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4241756:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/113 - EI30 2:6334040 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/113 - EI30 2:6334040:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:6874632 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:6874632:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194089 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194089:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194880 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7194880:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/63:7494362 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/63:7494362:1 | predefined | on 1 type object
  Windows 1:Windows 1:7130245 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2418414 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2418414:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2553776 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:2553776:1 | predefined | on 1 type object
  RA325_101:GO 205/155 - Panneau 201/2x83 - EI30:3360772 | predefined | on 1 type object
  RA325_101:GO 205/155 - Panneau 201/2x83 - EI30:3360772:1 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:3439274 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:3439274:1 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3456848 | predefined | on 1 type object
  RA325_001:GO 215/131 - Panneau 211/123 - EI30:4018414 | predefined | on 1 type object
  RA325_001:GO 215/131 - Panneau 211/123 - EI30:4018414:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:4019852 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:4019852:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033562 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:7033562:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:7090900 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:7090900:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192092 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192092:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192265 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7192265:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7207360 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:7207360:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7552905 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7552905:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7553261 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/103 - Vitrée - Menuiserie:7553261:1 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7572881 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7572893 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7572899 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7574304 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7574310 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7578011 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7578088 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7578094 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7578100 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7578385 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7581970 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7582174 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7589053 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7589243 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:7589266 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:2523204 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:2523204:1 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:2868730 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al):Type 1:2868731 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Type 1:2868732 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al):Type 1:2869126 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2957181 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2957183 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2957229 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2957231 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:2958738 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al):Type 1:2958739 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Type 1:2958740 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2958782 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2958784 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al):Type 1:2962262 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2962307 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2962309 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:2999363 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:2999364 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:2999365 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2999366 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:2999367 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:3002496 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:3002497 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:3002498 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:3052412 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:3052413 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:3052414 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3052415 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3052416 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:3281271 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al):Type 1:3281272 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:3281273 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3281275 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3281277 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:3395756 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:3395756:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:3448159 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:3448159:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:3453525 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:3453525:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:3453526 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:3453526:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:3453527 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:3453527:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:3988353 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83 - EI30:3988353:1 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4022828 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4022828:1 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4240844 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4240844:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:4240846 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93 - EI30:4240846:1 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4240847 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4240847:1 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3002831 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:3002832 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:4385130 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93:4385130:1 | predefined | on 1 type object
  RA319_Wall-Mullion:Brick:4833578 | predefined | on 1 type object
  RA319_Wall-Mullion:Brick:4833615 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:4833995 | predefined | on 1 type object
  RA314_Window-frame-2x(OB+Al)_Asym:Type 1:4833996 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Type 1:4833997 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4833998 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4834000 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5477771 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5477772 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5512232 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5512233 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5512294 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5512295 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5514679 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5514680 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5550800 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5550801 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5550828 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5550829 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5869635 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5869635:1 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:6181282 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:6181376 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870877 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/93 - Type BEDDELEEM:5870877:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4027764 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4027764:1 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7017670 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:7017670:1 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4218419 | predefined | on 1 type object
  RA325_011:GO 215/91 - Panneau 211/83:4218419:1 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:7079569 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:7079569:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:6280575 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:6280575:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2479118 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2479118:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2479822 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2479822:1 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4217677 | predefined | on 1 type object
  RA325_111:GO 215/175 - Panneau 211/2x83 - EI30:4217677:1 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4217684 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4217684:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4241308 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4241308:1 | predefined | on 1 type object
  RA325_200_PorteSimple_Coulissante:201/1x93:5837747 | predefined | on 1 type object
  RA325_200_PorteSimple_Coulissante:201/1x93:5837747:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:7753120 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:7753120:1 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2497172 | predefined | on 1 type object
  RA325_011:GO 215/101 - Panneau 211/93:2497172:1 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4219135 | predefined | on 1 type object
  RA325_001:GO 215/101 - Panneau 211/93 - EI30:4219135:1 | predefined | on 1 type object
  RA325_200_PorteSimple_Coulissante:201/1x93:5839206 | predefined | on 1 type object
  RA325_200_PorteSimple_Coulissante:201/1x93:5839206:1 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:6288169 | predefined | on 1 type object
  RA325_081_Menuiserie:Panneau 211/73:6288169:1 | predefined | on 1 type object
  RA325_011:GO 215/111 - Panneau 211/103:2701285 | predefined | on 1 type object
  RA325_011:GO 215/111 - Panneau 211/103:2701285:1 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220066 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220066:1 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4375558 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4375564 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4375565 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4375721 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4375723 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4375725 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:4376201 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:4376350 | predefined | on 1 type object
  RA319_Window-sill-stone:RA_Windows_Sill:4377019 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4377020 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377029 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:4375824 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4377038 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377044 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377045 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:4377065 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4377066 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377072 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377073 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:4378028 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:4378045 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5550780 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5550865 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5587170 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5685850 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5685925 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5686404 | predefined | on 1 type object
  RA325_011:GO 215/111 - Panneau 211/103 - EI30:4220738 | predefined | on 1 type object
  RA325_011:GO 215/111 - Panneau 211/103 - EI30:4220738:1 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220745 | predefined | on 1 type object
  RA325_011:GO 215/131 - Panneau 211/123 - EI30:4220745:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4220760 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4220760:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4241687 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4241687:1 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4287332 | predefined | on 1 type object
  RA325_001:GO 215/91 - Panneau 211/83:4287332:1 | predefined | on 1 type object
  RA319_Window-sill-stone:RA_Windows_Sill:4377233 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:4377234 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:4377238 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5685797 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5686417 | predefined | on 1 type object
  RA319_Window-sill-brick:RA_Windows_Sill:5965433 | predefined | on 1 type object
  RA314_Window-frame-1x(OB+Al):Type 1:5965434 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:5965435 | predefined | on 1 type object
  RA319_Glass Ext:Type 1:5965436 | predefined | on 1 type object
  RA311_Windows-sill-int-standard:Tablette + ebrasement:5965437 | predefined | on 1 type object
  RA311_Windows-stretcher-steel:Type 1:5965438 | predefined | on 1 type object
  RA319_Windows-Lintel:Brick:5965439 | predefined | on 1 type object
  RA_A-570_Ventelles:Occurence:7286130 | predefined | on 1 type object
  RA_A-570_Ventelles:Occurence:7287056 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:3060108 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:3060108:1 | predefined | on 1 type object
  RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure:3242203 | predefined | on 1 type object
  RA325_101:GO 205/195 - Panneau 201/2x93 / Extérieure:3242203:1 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256040 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256040:1 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256182 | predefined | on 1 type object
  RA325_011:GO 205/91 - Panneau 201/83 / Extérieure:4256182:1 | predefined | on 1 type object
  RA_A-570_Ventelles:Occurence:7286462 | predefined | on 1 type object