IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 271fbc3d-b723-4394-9839-180bc37685b9, NumberOfSaves: 245]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "Project Number"
Time stamp: "2023-08-30T12:26:25"
Preprocessor: "ODA IFC SDK 22.6"
Originating system: "22.1.1.516 - Exporter 22.6.2.0 - Alternate UI 22.6.2.0"
Application: "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)"

People and organizations
  Person "meray.nassimos" of Organization (no name given)
  Owner history of Person "meray.nassimos" of Organization (no name given) | application "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)" | change NOCHANGE | created 1692954028 (2023-08-25T09:00:28Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "WIERDE - BUREAUX TP" | phase "Project Status"
  IFCSITE "Default" | latitude 50° 26′ 11.41571″ | longitude 4° 54′ 59.321365″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Rue du Fort d'Andoy 5, 5100 Namur", "Rue", "du Fort d'Andoy 5", "5100 Namur"
      IFCBUILDINGSTOREY "RDC -ANDOY000-AR-AB-109" | long name "RDC -ANDOY000-AR-AB-109" | object type "Level:Circle Head - Project Datum" | elevation -7.8780025283262631
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Sous sol -2 -ANDOY000-AR-AB-80" | long name "Sous sol -2 -ANDOY000-AR-AB-80" | object type "Level:Circle Head - Project Datum" | elevation -7.4780025283262637
        contains 8 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:CAVE_M-cave-01 (Fibraroc" | object type "Basic Wall:CAVE_M-cave-01 (Fibraroc" | names: "Basic Wall:CAVE_M-cave-01 (Fibraroc:814741", "Basic Wall:CAVE_M-cave-01 (Fibraroc:815618", "Basic Wall:CAVE_M-cave-01 (Fibraroc:815919" | material: layers "Basic Wall:CAVE_M-cave-01 (Fibraroc" ("J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.29999999999999993, "Rigid insulation" 0.12499999999999999) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:CAVE_M-cave-01 (Fibraroc" | object type "Basic Wall:CAVE_M-cave-01 (Fibraroc" | names: "Basic Wall:CAVE_M-cave-01 (Fibraroc:818005" | material: layers "Basic Wall:CAVE_M-cave-01 (Fibraroc" ("J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.29999999999999993, "Rigid insulation" 0.12499999999999999) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCDOOR | type IFCDOORSTYLE "Sliding Door - 4 Panel (AUS):Type 1" | object type "Sliding Door - 4 Panel (AUS):Type 1" | names: "Sliding Door - 4 Panel (AUS):Type 1:839914" | material: materials ("Sliding Door Glass", "Sliding Door Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCSLAB | type IFCSLABTYPE "Floor:***PKG_Dalle sur parking_D-" | object type "Floor:***PKG_Dalle sur parking_D-" | FLOOR | names: "Floor:***PKG_Dalle sur parking_D-:902749" | material: layers "Floor:***PKG_Dalle sur parking_D-" ("J- Cave-Linoléum, carreaux de PVC (Divers) λ=0.19- (TENACITY-Vinilo-LOSETA)" 0.0050000000000000001, "J- Cave-Béton léger en dalles, panneaux pleins ou chape (Eléments de construction pierreux sans joints) λ=0.12 (Concrete, Lightweight, 50)" 0.080000000000000002, "J- Cave/SOL_Dalla_Atrium-Nestaan Holland BV λU=0.026" 0.20000000000000001, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.34999999999999998) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          2 x IFCGRID | names: "Default Grid"
        IFCSPACE "418" | long name "Parking" | INTERNAL
      IFCBUILDINGSTOREY "Sous sol -1 -ANDOY000-AR-AB-90" | long name "Sous sol -1 -ANDOY000-AR-AB-90" | object type "Level:Circle Head - Project Datum" | elevation -3.7080025283262641
        contains 336 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "UC-Universal Columns-Column:UC305x305x97" | object type "UC-Universal Columns-Column:UC305x305x97" | names: "UC-Universal Columns-Column:UC305x305x97:403836" | material: "Metal - Steel 43-275" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | object type "Concrete Square:400 x 400mm" | names: "Concrete Square:400 x 400mm:602095" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Rectangular:300 x 450mm" | object type "Rectangular:300 x 450mm" | names: "Rectangular:300 x 450mm:602118" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          48 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:705212", "Basic Wall:Wall-Partn_12P-75Std-12P:705218", "Basic Wall:Wall-Partn_12P-75Std-12P:705220" (+45 more) | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          53 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 10 bloc Wall-Partn" | object type "Basic Wall:J- 10 bloc Wall-Partn" | names: "Basic Wall:J- 10 bloc Wall-Partn:705226", "Basic Wall:J- 10 bloc Wall-Partn:705227", "Basic Wall:J- 10 bloc Wall-Partn:705230" (+50 more) | material: layers "Basic Wall:J- 10 bloc Wall-Partn" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:705236", "Basic Wall:EXT_M-ext-01 (FT FA-02:705237", "Basic Wall:EXT_M-ext-01 (FT FA-02:705238" (+3 more) | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:705240", "Basic Wall:EXT_M-ext-01 (FT FA-02:706887", "Basic Wall:EXT_M-ext-01 (FT FA-02:706888" (+12 more) | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:705241", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:705267", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:706858" (+6 more) | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.125, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          36 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:705245", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:705246", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:705247" (+33 more) | material: layers "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.185, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | object type "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | names: "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:705255", "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:705258", "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:728231" | material: layers "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          25 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_22" | object type "Basic Wall:J- escalier Wall-Int_22" | names: "Basic Wall:J- escalier Wall-Int_22:705264", "Basic Wall:J- escalier Wall-Int_22:705265", "Basic Wall:J- escalier Wall-Int_22:705266" (+22 more) | material: layers "Basic Wall:J- escalier Wall-Int_22" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          6 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:705270", "Doors_IntSgl:J-1000x2110mm 2:709830", "Doors_IntSgl:J-1000x2110mm 2:709841" (+3 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:705272" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:705276" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:705277" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:705373" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:705384" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:705386", "Doors_IntSgl:J-1000x2110mm 2:750619", "Doors_IntSgl:J-1000x2110mm 2:753598" (+1 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | object type "Concrete Square:400 x 400mm" | names: "Concrete Square:400 x 400mm:705387", "Concrete Square:400 x 400mm:743374" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          40 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SH_Curtain wall" | object type "Curtain Wall:SH_Curtain wall" | names: "Curtain Wall:SH_Curtain wall:705389", "Curtain Wall:SH_Curtain wall:706862", "Curtain Wall:SH_Curtain wall:709613" (+37 more) | parts: 684 IFCMEMBER, 241 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Rectangular:300 x 450mm" | object type "Rectangular:300 x 450mm" | names: "Rectangular:300 x 450mm:705405" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte" | object type "Curtain Wall:J- wall latte" | names: "Curtain Wall:J- wall latte:706430", "Curtain Wall:J- wall latte:706532", "Curtain Wall:J- wall latte:707474" (+1 more) | parts: 80 IFCPLATE, 76 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:706857" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:706883" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:706884" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:706919", "Doors_IntSgl:J-1000x2110mm 2:709827", "Doors_IntSgl:J-1000x2110mm 2:709843" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:707008" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:707010", "Doors_IntSgl:J-1000x2110mm 2:748905", "Doors_IntSgl:J-1000x2110mm 2:749653" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:707012", "Doors_IntSgl:J-1000x2110mm 2:729123" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:709576", "Doors_IntSgl:J-1000x2110mm 2:766792" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone" | object type "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone" | names: "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone:709832", "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone:722858", "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone:754473" (+1 more) | material: layers "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone" ("Brick, Engineering, Grey" 0.059999999999999998, "Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.18999999999999997, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:709933", "Concrete Square:300 x 300mm:709935" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          5 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame w Glass:1770 x 2500" | object type "Double-Standard Frame w Glass:1770 x 2500" | names: "Double-Standard Frame w Glass:1770 x 2500:710453", "Double-Standard Frame w Glass:1770 x 2500:723207", "Double-Standard Frame w Glass:1770 x 2500:723298" (+2 more) | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Text, Constraints, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2" | object type "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2" | names: "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2:711193", "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2:768441" | material: layers "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:730099" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 27 bloc Wall-Partn" | object type "Basic Wall:J- 27 bloc Wall-Partn" | names: "Basic Wall:J- 27 bloc Wall-Partn:741932" | material: layers "Basic Wall:J- 27 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.23000000000000001, "Plaster" 0.02) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:742362", "Basic Wall:Wall-Partn_12P-75Std-12P:746554" | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 35 bloc Wall-Partn" | object type "Basic Wall:J- 35 bloc Wall-Partn" | names: "Basic Wall:J- 35 bloc Wall-Partn:744561", "Basic Wall:J- 35 bloc Wall-Partn:745051", "Basic Wall:J- 35 bloc Wall-Partn:755228" | material: layers "Basic Wall:J- 35 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.23000000000000001, "Concrete Masonry Units _Low Density" 0.12, "Plaster" 0.02) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:400 x 400mm with cover" | object type "Concrete Square:400 x 400mm with cover" | names: "Concrete Square:400 x 400mm with cover:745141", "Concrete Square:400 x 400mm with cover:745834" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:400 x 400mm with cover" | object type "Concrete Square:400 x 400mm with cover" | names: "Concrete Square:400 x 400mm with cover:745627", "Concrete Square:400 x 400mm with cover:745836" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:747142", "Doors_IntSgl:J-900x2110mm 3:747412" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:747468", "Doors_IntSgl:J-640x2000mm 4:747672", "Doors_IntSgl:J-640x2000mm 4:747752" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:747538", "Doors_IntSgl:J-640x2000mm 4:747592" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:750705", "Doors_IntSgl:J-1000x2110mm 2:751974", "Doors_IntSgl:J-1000x2110mm 2:752279" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1400x2110mm" | object type "Doors_IntSgl:J-1400x2110mm" | names: "Doors_IntSgl:J-1400x2110mm:750830" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:753189", "Doors_IntSgl:J-900x2110mm 3:753242" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 2000x910mm 3" | object type "Windows_Sgl_Plain:J- 2000x910mm 3" | names: "Windows_Sgl_Plain:J- 2000x910mm 3:755806", "Windows_Sgl_Plain:J- 2000x910mm 3:755988", "Windows_Sgl_Plain:J- 2000x910mm 3:756058" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame-Variable:J-1800 x 2000" | object type "Double-Standard Frame-Variable:J-1800 x 2000" | names: "Double-Standard Frame-Variable:J-1800 x 2000:756339", "Double-Standard Frame-Variable:J-1800 x 2000:775941" | material: materials ("Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12" | object type "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12" | names: "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12:756883" | material: layers "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Brick, Engineering, Grey" 0.12, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCSTAIR | object type "Assembled Stair:Private" | names: "Assembled Stair:Stair:760260" | parts: 3 IFCMEMBER, 1 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Phasing, Dimensions
          1 x IFCRAMP | object type "Ramp:Standard" | names: "Ramp:Standard:765625" | parts: 1 IFCRAMPFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RampCommon, Constraints, Phasing, Graphics
          7 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame w Glass:2060 x 2500" | object type "Double-Standard Frame w Glass:2060 x 2500" | names: "Double-Standard Frame w Glass:2060 x 2500:767743", "Double-Standard Frame w Glass:2060 x 2500:767770", "Double-Standard Frame w Glass:2060 x 2500:767870" (+4 more) | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Text, Constraints, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:769236" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          2 x IFCSTAIR | object type "Assembled Stair:Private" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:773768", "Assembled Stair:Stair:774873" | parts: 4 IFCRAILING, 2 IFCMEMBER, 2 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1800 x 2100 mm" | object type "Siliding:1800 x 2100 mm" | names: "Siliding:1800 x 2100 mm:775181" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame-Variable:J-1800 x 2000" | object type "Double-Standard Frame-Variable:J-1800 x 2000" | names: "Double-Standard Frame-Variable:J-1800 x 2000:775819" | material: materials ("Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:776307" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" | object type "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" | FLOOR | names: "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01:826979" | material: layers "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.014999999999999999, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J-SOL_Dalle_Atrium/Sous-sol-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=2.2-GFRC" 0.34999999999999998) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Plancher/plafond_ J_RDC 0.47" | object type "Floor:Plancher/plafond_ J_RDC 0.47" | FLOOR | names: "Floor:Plancher/plafond_ J_RDC 0.47:844145" | material: layers "Floor:Plancher/plafond_ J_RDC 0.47" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.12, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.34999999999999998, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          2 x IFCGRID | names: "Default Grid"
        IFCSPACE "332" | long name "Open Spaces" | INTERNAL
        IFCSPACE "334" | long name "Bureau" | INTERNAL
        IFCSPACE "335" | long name "Bureau" | INTERNAL
        IFCSPACE "336" | long name "Bureau" | INTERNAL
        IFCSPACE "337" | long name "Bureau" | INTERNAL
        IFCSPACE "338" | long name "Archive" | INTERNAL
        IFCSPACE "341" | long name "WC" | INTERNAL
        IFCSPACE "343" | long name "Bureau" | INTERNAL
        IFCSPACE "344" | long name "Bureau" | INTERNAL
        IFCSPACE "345" | long name "Bureau" | INTERNAL
        IFCSPACE "346" | long name "WC" | INTERNAL
        IFCSPACE "347" | long name "Bureau" | INTERNAL
        IFCSPACE "348" | long name "Bureau" | INTERNAL
        IFCSPACE "349" | long name "Cockpit" | INTERNAL
        IFCSPACE "350" | long name "Bureau" | INTERNAL
        IFCSPACE "351" | long name "Bureau" | INTERNAL
        IFCSPACE "356" | long name "Bureau" | INTERNAL
        IFCSPACE "358" | long name "Open Spaces" | INTERNAL
        IFCSPACE "359" | long name "Bureau" | INTERNAL
        IFCSPACE "360" | long name "WC" | INTERNAL
        IFCSPACE "368" | long name "Copie" | INTERNAL
        IFCSPACE "369" | long name "Archive" | INTERNAL
        IFCSPACE "370" | long name "Archive" | INTERNAL
        IFCSPACE "371" | long name "Archive" | INTERNAL
        IFCSPACE "373" | long name "Archive" | INTERNAL
        IFCSPACE "377" | long name "Couloir" | INTERNAL
        IFCSPACE "378" | long name "SAS" | INTERNAL
        IFCSPACE "379" | long name "Bureau" | INTERNAL
        IFCSPACE "380" | long name "Bureau" | INTERNAL
        IFCSPACE "381" | long name "Bureau" | INTERNAL
        IFCSPACE "382" | long name "Bureau" | INTERNAL
        IFCSPACE "383" | long name "Couloir" | INTERNAL
        IFCSPACE "384" | long name "Expo" | INTERNAL
        IFCSPACE "388" | long name "Couloir" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Electric Lift-4 Person Wall Based:Type 1" | object type "M_Electric Lift-4 Person Wall Based:Type 1" | names: "M_Electric Lift-4 Person Wall Based:Type 1:706880" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Electrical - Loads, Constraints
        IFCSPACE "389" | long name "Satirs" | INTERNAL
        IFCSPACE "390" | long name "Bureau" | INTERNAL
        IFCSPACE "391" | long name "Bureau" | INTERNAL
        IFCSPACE "392" | long name "Bureau" | INTERNAL
        IFCSPACE "394" | long name "Bureau" | INTERNAL
        IFCSPACE "395" | long name "Couloir" | INTERNAL
        IFCSPACE "397" | long name "Salle" | INTERNAL
        IFCSPACE "398" | long name "Coffee corner" | INTERNAL
        IFCSPACE "399" | long name "Bureau" | INTERNAL
        IFCSPACE "400" | long name "Bureau" | INTERNAL
        IFCSPACE "401" | long name "Bureau" | INTERNAL
        IFCSPACE "402" | long name "Bureau" | INTERNAL
        IFCSPACE "403" | long name "Bureau" | INTERNAL
        IFCSPACE "404" | long name "Technique" | INTERNAL
        IFCSPACE "406" | long name "Bureau" | INTERNAL
        IFCSPACE "408" | long name "Bureaux" | INTERNAL
        IFCSPACE "514" | long name "Restaurant" | INTERNAL
        IFCSPACE "515" | long name "Kitchen" | INTERNAL
      IFCBUILDINGSTOREY "-1 open offices (ramp)" | long name "-1 open offices (ramp)" | object type "Level:Circle Head - Project Datum" | elevation -3.3830025283262644
        contains 4 elements
          1 x IFCRAMP | object type "Ramp:Standard" | names: "Ramp:Standard:766211" | parts: 1 IFCRAMPFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RampCommon, Constraints, Phasing, Graphics
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Floor Ramp" | object type "Floor:Floor Ramp" | FLOOR | names: "Floor:Floor Ramp:766428" | material: layers "Floor:Floor Ramp" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01, "J- Béton léger en dalles, panneaux pleins ou chape (Eléments de construction pierreux sans joints) λ=0.14 Plancher (Concrete, Lightweight, 4 ksi)" 0.089999999999999997) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "-1 entrance (ramp)" | long name "-1 entrance (ramp)" | object type "Level:Circle Head - Project Datum" | elevation -3.0580025283262646
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Stairs" | long name "Stairs" | object type "Level:Circle Head - Project Datum" | elevation -1.5378647641311598
        contains 6 elements
          1 x IFCSTAIR | object type "Assembled Stair:Private" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:685151" | parts: 2 IFCRAILING, 1 IFCSLAB, 1 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Phasing, Dimensions
          1 x IFCRAMP | object type "Ramp:Standard" | names: "Ramp:Standard:769363" | parts: 2 IFCRAMPFLIGHT, 1 IFCSLAB | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RampCommon, Constraints, Phasing, Graphics
          2 x IFCRAILING | object type "Railing:1100mm" | names: "Railing:1100mm:769399", "Railing:1100mm:769403" | material: "<Unnamed>" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RailingCommon, Constraints, Phasing, Dimensions
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "-1 interior plafond" | long name "-1 interior plafond" | object type "Level:Circle Head - Project Datum" | elevation -0.15259271884309669
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "RDC -ANDOY000-AR-AB-100" | long name "RDC -ANDOY000-AR-AB-100" | object type "Level:Circle Head - Project Datum" | elevation 0.32199747167373571
        contains 450 elements
          1 x IFCSTAIR | object type "Assembled Stair:Private" | names: "Assembled Stair:Stair:352280" | parts: 3 IFCMEMBER, 1 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Phasing, Dimensions
          114 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:601666", "Basic Wall:Wall-Partn_12P-75Std-12P:601668", "Basic Wall:Wall-Partn_12P-75Std-12P:601669" (+111 more) | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 24 bloc Wall-Partn" | object type "Basic Wall:J- 24 bloc Wall-Partn" | names: "Basic Wall:J- 24 bloc Wall-Partn:601676", "Basic Wall:J- 24 bloc Wall-Partn:601677" | material: layers "Basic Wall:J- 24 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.20000000000000001, "Plaster" 0.02) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:601697", "Basic Wall:Wall-Partn_12P-75Std-12P:666233" | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 10 bloc Wall-Partn" | object type "Basic Wall:J- 10 bloc Wall-Partn" | names: "Basic Wall:J- 10 bloc Wall-Partn:601708", "Basic Wall:J- 10 bloc Wall-Partn:601709", "Basic Wall:J- 10 bloc Wall-Partn:601710" (+14 more) | material: layers "Basic Wall:J- 10 bloc Wall-Partn" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:601718", "Basic Wall:EXT_M-ext-01 (FT FA-02:601721", "Basic Wall:EXT_M-ext-01 (FT FA-02:601722" (+21 more) | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:601719", "Basic Wall:EXT_M-ext-01 (FT FA-02:601720", "Basic Wall:EXT_M-ext-01 (FT FA-02:605409" | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:601723", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:601754", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:605220" (+10 more) | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.125, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:601727", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:601728", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:601729" (+9 more) | material: layers "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.185, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | object type "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | names: "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:601738", "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:601741" | material: layers "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_22" | object type "Basic Wall:J- escalier Wall-Int_22" | names: "Basic Wall:J- escalier Wall-Int_22:601751", "Basic Wall:J- escalier Wall-Int_22:601752", "Basic Wall:J- escalier Wall-Int_22:601753" (+12 more) | material: layers "Basic Wall:J- escalier Wall-Int_22" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          9 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:601774", "Doors_IntSgl:J-1000x2110mm 2:605463", "Doors_IntSgl:J-1000x2110mm 2:605506" (+6 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-920x2110mm 3" | object type "Doors_IntSgl:J-920x2110mm 3" | names: "Doors_IntSgl:J-920x2110mm 3:601775" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:601776" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:601777" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:601778" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:601785", "Doors_IntSgl:J-640x2000mm 4:601786" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:601787", "Doors_IntSgl:J-640x2000mm 4:601788" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:601789", "Doors_IntSgl:J-900x2110mm 3:601790", "Doors_IntSgl:J-900x2110mm 3:653012" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          41 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:601792", "Windows_Sgl_Plain:J- 900x910mm 2:601793", "Windows_Sgl_Plain:J- 900x910mm 2:601794" (+38 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          27 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:601830", "Windows_Sgl_Plain:J- 900x910mm 2:601831", "Windows_Sgl_Plain:J- 900x910mm 2:601832" (+24 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          14 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SH_Curtain wall" | object type "Curtain Wall:SH_Curtain wall" | names: "Curtain Wall:SH_Curtain wall:601850", "Curtain Wall:SH_Curtain wall:602100", "Curtain Wall:SH_Curtain wall:602122" (+11 more) | parts: 461 IFCMEMBER, 177 IFCPLATE, 4 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:601985" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:602022", "Concrete Square:300 x 300mm:666853", "Concrete Square:300 x 300mm:667337" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:602094" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          34 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte" | object type "Curtain Wall:J- wall latte" | names: "Curtain Wall:J- wall latte:602265", "Curtain Wall:J- wall latte:602632", "Curtain Wall:J- wall latte:602906" (+31 more) | parts: 588 IFCPLATE, 563 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          15 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte plant" | object type "Curtain Wall:J- wall latte plant" | names: "Curtain Wall:J- wall latte plant:604026", "Curtain Wall:J- wall latte plant:604214", "Curtain Wall:J- wall latte plant:641855" (+12 more) | parts: 181 IFCPLATE, 167 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:605218" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:605404" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:605405" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          5 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:605462", "Doors_IntSgl:J-1000x2110mm 2:605564", "Doors_IntSgl:J-1000x2110mm 2:652186" (+2 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          14 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | object type "Windows_Sgl_Plain:J- 1270x910mm 2" | names: "Windows_Sgl_Plain:J- 1270x910mm 2:605465", "Windows_Sgl_Plain:J- 1270x910mm 2:605466", "Windows_Sgl_Plain:J- 1270x910mm 2:605478" (+11 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          12 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | object type "Windows_Sgl_Plain:J- 820x910mm" | names: "Windows_Sgl_Plain:J- 820x910mm:605467", "Windows_Sgl_Plain:J- 820x910mm:605468", "Windows_Sgl_Plain:J- 820x910mm:605470" (+9 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:605511" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          14 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:605512", "Doors_IntSgl:J-1000x2110mm 2:605513", "Doors_IntSgl:J-1000x2110mm 2:605565" (+11 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:605558", "Doors_IntSgl:J-640x2000mm 4:605559" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:605561", "Doors_IntSgl:J-640x2000mm 4:605562" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:605563" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          7 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:605566", "Doors_IntSgl:J-1000x2110mm 2:605571", "Doors_IntSgl:J-1000x2110mm 2:605574" (+4 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:655832", "Doors_IntSgl:J-900x2110mm 3:655868" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:657147" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:661137" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          3 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:661338", "Doors_IntSgl:J-1000x2110mm 2:664116", "Doors_IntSgl:J-1000x2110mm 2:666066" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:664350" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | object type "Windows_Sgl_Plain:J- 1270x910mm 2" | names: "Windows_Sgl_Plain:J- 1270x910mm 2:665502" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone" | object type "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone" | names: "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone:669983", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone:670166", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone:670467" (+3 more) | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone" ("Brick, Engineering, Grey" 0.059999999999999998, "Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.12499999999999999, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | object type "Windows_Sgl_Plain:J- 820x910mm" | names: "Windows_Sgl_Plain:J- 820x910mm:670554", "Windows_Sgl_Plain:J- 820x910mm:670636" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1800 x 2100 mm" | object type "Siliding:1800 x 2100 mm" | names: "Siliding:1800 x 2100 mm:670720" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame w Glass:1770 x 2500" | object type "Double-Standard Frame w Glass:1770 x 2500" | names: "Double-Standard Frame w Glass:1770 x 2500:671404" | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Text, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1800 x 2100 mm" | object type "Siliding:1800 x 2100 mm" | names: "Siliding:1800 x 2100 mm:671480" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Double-Standard Frame w Glass:1770 x 2500" | object type "Double-Standard Frame w Glass:1770 x 2500" | names: "Double-Standard Frame w Glass:1770 x 2500:671481" | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Text, Constraints, Phasing
          4 x IFCSLAB | type IFCSLABTYPE "Floor:Plancher/plafond_ J_RDC 0.47" | object type "Floor:Plancher/plafond_ J_RDC 0.47" | FLOOR | names: "Floor:Plancher/plafond_ J_RDC 0.47:674882", "Floor:Plancher/plafond_ J_RDC 0.47:675346", "Floor:Plancher/plafond_ J_RDC 0.47:675630" (+1 more) | material: layers "Floor:Plancher/plafond_ J_RDC 0.47" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.12, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.34999999999999998, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          1 x IFCROOF | object type "Basic Roof:EXT_Toiture principale_T-ext-" | names: "Basic Roof:EXT_Toiture principale_T-ext-:895513" | parts: 1 IFCSLAB | material: layers "Basic Roof:EXT_Toiture principale_T-ext-" ("J-EXT_Toiture principale-Membrane bitumineuse (Divers)- λU=0.23 Asphalt, Bitumen" 0.0050000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.28000000000000003) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Phasing, Construction
          2 x IFCGRID | names: "Default Grid"
        IFCSPACE "108" | long name "Bureau" | INTERNAL
        IFCSPACE "109" | long name "Bureau" | INTERNAL
        IFCSPACE "110" | long name "Bureaux" | INTERNAL
        IFCSPACE "111" | long name "Bureau" | INTERNAL
        IFCSPACE "112" | long name "Bureau" | INTERNAL
        IFCSPACE "113" | long name "Bureau" | INTERNAL
        IFCSPACE "115" | long name "WC" | INTERNAL
        IFCSPACE "116" | long name "Bureau" | INTERNAL
        IFCSPACE "117" | long name "Bureau" | INTERNAL
        IFCSPACE "118" | long name "Bureau" | INTERNAL
        IFCSPACE "119" | long name "Bureau" | INTERNAL
        IFCSPACE "120" | long name "Couloir" | INTERNAL
        IFCSPACE "121" | long name "Stairs" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Electric Lift-4 Person Wall Based:Type 1" | object type "M_Electric Lift-4 Person Wall Based:Type 1" | names: "M_Electric Lift-4 Person Wall Based:Type 1:605262" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Electrical - Loads, Constraints
        IFCSPACE "122" | long name "Bureau" | INTERNAL
        IFCSPACE "124" | long name "Bureau" | INTERNAL
        IFCSPACE "125" | long name "Bureau" | INTERNAL
        IFCSPACE "126" | long name "SDR 6P" | INTERNAL
        IFCSPACE "127" | long name "Bureau" | INTERNAL
        IFCSPACE "128" | long name "Bureau" | INTERNAL
        IFCSPACE "129" | long name "Bureau" | INTERNAL
        IFCSPACE "130" | long name "Bureau" | INTERNAL
        IFCSPACE "132" | long name "Bureau" | INTERNAL
        IFCSPACE "135" | long name "Stairs" | INTERNAL
        IFCSPACE "136" | long name "Technique" | INTERNAL
        IFCSPACE "137" | long name "Technique" | INTERNAL
        IFCSPACE "139" | long name "Bureau" | INTERNAL
        IFCSPACE "140" | long name "WC" | INTERNAL
        IFCSPACE "145" | long name "Bureau" | INTERNAL
        IFCSPACE "146" | long name "Cockpit" | INTERNAL
        IFCSPACE "147" | long name "Technique" | INTERNAL
        IFCSPACE "150" | long name "Cockpit" | INTERNAL
        IFCSPACE "151" | long name "Bureau" | INTERNAL
        IFCSPACE "152" | long name "Couloir" | INTERNAL
        IFCSPACE "153" | long name "Bureau" | INTERNAL
        IFCSPACE "154" | long name "Bureau" | INTERNAL
        IFCSPACE "155" | long name "Bureau" | INTERNAL
        IFCSPACE "156" | long name "Bureau" | INTERNAL
        IFCSPACE "157" | long name "Couloir" | INTERNAL
        IFCSPACE "158" | long name "SDR 4P" | INTERNAL
        IFCSPACE "159" | long name "Bureau" | INTERNAL
        IFCSPACE "160" | long name "Bureau" | INTERNAL
        IFCSPACE "163" | long name "Bureau" | INTERNAL
        IFCSPACE "165" | long name "SAS" | INTERNAL
        IFCSPACE "166" | long name "Bureau" | INTERNAL
        IFCSPACE "167" | long name "Bureau" | INTERNAL
        IFCSPACE "168" | long name "Technique" | INTERNAL
        IFCSPACE "169" | long name "Bureau" | INTERNAL
        IFCSPACE "170" | long name "Bureau" | INTERNAL
        IFCSPACE "171" | long name "Bureau" | INTERNAL
        IFCSPACE "172" | long name "Cockpit" | INTERNAL
        IFCSPACE "175" | long name "Atrium" | INTERNAL
        IFCSPACE "179" | long name "Couloir" | INTERNAL
        IFCSPACE "183" | long name "Bureau" | INTERNAL
        IFCSPACE "184" | long name "Bureau" | INTERNAL
        IFCSPACE "185" | long name "Bureau" | INTERNAL
        IFCSPACE "187" | long name "Technique" | INTERNAL
        IFCSPACE "188" | long name "Bureau" | INTERNAL
        IFCSPACE "189" | long name "Bureau" | INTERNAL
        IFCSPACE "190" | long name "Bureau" | INTERNAL
        IFCSPACE "193" | long name "SDR 4P" | INTERNAL
        IFCSPACE "194" | long name "Cockpit" | INTERNAL
        IFCSPACE "195" | long name "Cockpit" | INTERNAL
        IFCSPACE "197" | long name "Bureaux SAV" | INTERNAL
        IFCSPACE "200" | long name "Bureaux" | INTERNAL
        IFCSPACE "201" | long name "Bureaux" | INTERNAL
        IFCSPACE "202" | long name "Bureaux" | INTERNAL
        IFCSPACE "203" | long name "Bureaux" | INTERNAL
        IFCSPACE "161" | long name "Bureau" | INTERNAL
        IFCSPACE "162" | long name "Space" | INTERNAL
        IFCSPACE "164" | long name "Space" | INTERNAL
        IFCSPACE "165" | long name "Space" | INTERNAL
        IFCSPACE "166" | long name "Space" | INTERNAL
        IFCSPACE "168" | long name "Space" | INTERNAL
        IFCSPACE "169" | long name "Space" | INTERNAL
        IFCSPACE "170" | long name "Space" | INTERNAL
        IFCSPACE "171" | long name "Space" | INTERNAL
        IFCSPACE "172" | long name "Space" | INTERNAL
        IFCSPACE "173" | long name "Space" | INTERNAL
        IFCSPACE "174" | long name "Space" | INTERNAL
        IFCSPACE "177" | long name "Space" | INTERNAL
        IFCSPACE "178" | long name "Space" | INTERNAL
        IFCSPACE "179" | long name "Space" | INTERNAL
        IFCSPACE "180" | long name "Space" | INTERNAL
        IFCSPACE "181" | long name "Space" | INTERNAL
        IFCSPACE "182" | long name "Space" | INTERNAL
        IFCSPACE "183" | long name "Space" | INTERNAL
        IFCSPACE "184" | long name "Space" | INTERNAL
        IFCSPACE "186" | long name "Space" | INTERNAL
        IFCSPACE "187" | long name "Space" | INTERNAL
        IFCSPACE "188" | long name "Space" | INTERNAL
        IFCSPACE "189" | long name "Space" | INTERNAL
        IFCSPACE "190" | long name "Space" | INTERNAL
        IFCSPACE "192" | long name "Space" | INTERNAL
        IFCSPACE "193" | long name "Space" | INTERNAL
        IFCSPACE "194" | long name "Space" | INTERNAL
        IFCSPACE "195" | long name "Space" | INTERNAL
        IFCSPACE "196" | long name "Space" | INTERNAL
        IFCSPACE "197" | long name "Space" | INTERNAL
        IFCSPACE "199" | long name "Space" | INTERNAL
        IFCSPACE "200" | long name "Space" | INTERNAL
        IFCSPACE "201" | long name "Space" | INTERNAL
        IFCSPACE "203" | long name "Space" | INTERNAL
        IFCSPACE "204" | long name "Space" | INTERNAL
        IFCSPACE "205" | long name "Space" | INTERNAL
        IFCSPACE "206" | long name "Space" | INTERNAL
        IFCSPACE "207" | long name "Space" | INTERNAL
        IFCSPACE "208" | long name "Space" | INTERNAL
        IFCSPACE "209" | long name "Space" | INTERNAL
        IFCSPACE "211" | long name "Space" | INTERNAL
        IFCSPACE "212" | long name "Space" | INTERNAL
        IFCSPACE "213" | long name "Space" | INTERNAL
        IFCSPACE "214" | long name "Space" | INTERNAL
        IFCSPACE "215" | long name "Space" | INTERNAL
        IFCSPACE "216" | long name "Space" | INTERNAL
        IFCSPACE "217" | long name "Space" | INTERNAL
        IFCSPACE "218" | long name "Space" | INTERNAL
        IFCSPACE "219" | long name "Space" | INTERNAL
        IFCSPACE "220" | long name "Space" | INTERNAL
        IFCSPACE "221" | long name "Space" | INTERNAL
        IFCSPACE "222" | long name "Space" | INTERNAL
        IFCSPACE "223" | long name "Space" | INTERNAL
        IFCSPACE "224" | long name "Space" | INTERNAL
        IFCSPACE "225" | long name "Space" | INTERNAL
        IFCSPACE "226" | long name "Space" | INTERNAL
        IFCSPACE "227" | long name "Space" | INTERNAL
        IFCSPACE "228" | long name "Space" | INTERNAL
        IFCSPACE "229" | long name "Space" | INTERNAL
        IFCSPACE "230" | long name "Space" | INTERNAL
        IFCSPACE "231" | long name "Space" | INTERNAL
        IFCSPACE "232" | long name "Space" | INTERNAL
        IFCSPACE "233" | long name "Space" | INTERNAL
        IFCSPACE "234" | long name "Space" | INTERNAL
        IFCSPACE "235" | long name "Space" | INTERNAL
        IFCSPACE "236" | long name "Space" | INTERNAL
        IFCSPACE "237" | long name "Space" | INTERNAL
        IFCSPACE "238" | long name "Space" | INTERNAL
        IFCSPACE "239" | long name "Space" | INTERNAL
        IFCSPACE "240" | long name "Space" | INTERNAL
        IFCSPACE "241" | long name "Space" | INTERNAL
        IFCSPACE "242" | long name "Space" | INTERNAL
        IFCSPACE "243" | long name "Space" | INTERNAL
        IFCSPACE "245" | long name "Space" | INTERNAL
        IFCSPACE "246" | long name "Space" | INTERNAL
        IFCSPACE "247" | long name "Space" | INTERNAL
        IFCSPACE "248" | long name "Space" | INTERNAL
        IFCSPACE "249" | long name "Space" | INTERNAL
        IFCSPACE "250" | long name "Space" | INTERNAL
        IFCSPACE "251" | long name "Space" | INTERNAL
        IFCSPACE "252" | long name "Space" | INTERNAL
        IFCSPACE "253" | long name "Space" | INTERNAL
        IFCSPACE "254" | long name "Space" | INTERNAL
        IFCSPACE "255" | long name "Space" | INTERNAL
        IFCSPACE "413" | long name "Bureau" | INTERNAL
        IFCSPACE "414" | long name "Entrance" | INTERNAL
        IFCSPACE "416" | long name "Bureau" | INTERNAL
        IFCSPACE "257" | long name "Space" | INTERNAL
      IFCBUILDINGSTOREY "int plafond RDC" | long name "int plafond RDC" | object type "Level:Circle Head - Project Datum" | elevation 3.3219974716737091
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Top level beton plafond RDC" | long name "Top level beton plafond RDC" | object type "Level:Circle Head - Project Datum" | elevation 3.6019974716737093
        contains 5 elements
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:640066", "Concrete Square:300 x 300mm:640136", "Concrete Square:300 x 300mm:640269" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Etage 1 -ANDOY000-AR-AB-110" | long name "Etage 1 -ANDOY000-AR-AB-110" | object type "Level:Circle Head - Project Datum" | elevation 3.7019974716737125
        contains 471 elements
          3 x IFCSLAB | type IFCSLABTYPE "Floor:Plancher/plafond_ J_R1 0.38" | object type "Floor:Plancher/plafond_ J_R1 0.38" | FLOOR | names: "Floor:Plancher/plafond_ J_R1 0.38:334625", "Floor:Plancher/plafond_ J_R1 0.38:675570", "Floor:Plancher/plafond_ J_R1 0.38:779612" | material: layers "Floor:Plancher/plafond_ J_R1 0.38" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.10000000000000001, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.28000000000000003, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          157 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:334786", "Basic Wall:Wall-Partn_12P-75Std-12P:334875", "Basic Wall:Wall-Partn_12P-75Std-12P:334949" (+154 more) | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:339480", "Basic Wall:Wall-Partn_12P-75Std-12P:341431" | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 10 bloc Wall-Partn" | object type "Basic Wall:J- 10 bloc Wall-Partn" | names: "Basic Wall:J- 10 bloc Wall-Partn:341509", "Basic Wall:J- 10 bloc Wall-Partn:341709", "Basic Wall:J- 10 bloc Wall-Partn:341764" (+12 more) | material: layers "Basic Wall:J- 10 bloc Wall-Partn" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          28 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:345343", "Basic Wall:EXT_M-ext-01 (FT FA-02:345347", "Basic Wall:EXT_M-ext-01 (FT FA-02:345516" (+25 more) | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:346166", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:352249", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:439744" (+1 more) | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.125, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:347179", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:348002", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:348106" (+7 more) | material: layers "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.185, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | object type "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | names: "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:349468", "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4:350225" | material: layers "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          26 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_22" | object type "Basic Wall:J- escalier Wall-Int_22" | names: "Basic Wall:J- escalier Wall-Int_22:351400", "Basic Wall:J- escalier Wall-Int_22:351807", "Basic Wall:J- escalier Wall-Int_22:351966" (+23 more) | material: layers "Basic Wall:J- escalier Wall-Int_22" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          14 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SH_Curtain wall" | object type "Curtain Wall:SH_Curtain wall" | names: "Curtain Wall:SH_Curtain wall:357103", "Curtain Wall:SH_Curtain wall:357865", "Curtain Wall:SH_Curtain wall:358011" (+11 more) | parts: 278 IFCMEMBER, 92 IFCPLATE, 12 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          7 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:359217", "Doors_IntSgl:J-1000x2110mm 2:361469", "Doors_IntSgl:J-1000x2110mm 2:926759" (+4 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-920x2110mm 3" | object type "Doors_IntSgl:J-920x2110mm 3" | names: "Doors_IntSgl:J-920x2110mm 3:360002" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:360136" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:360536" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:360730" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:361081" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:361128" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | object type "Doors_IntSgl:J-900x2110mm 3" | names: "Doors_IntSgl:J-900x2110mm 3:361187", "Doors_IntSgl:J-900x2110mm 3:434882" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          13 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:361531", "Doors_IntSgl:J-1000x2110mm 2:361587", "Doors_IntSgl:J-1000x2110mm 2:435024" (+10 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          4 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:361908", "Doors_IntSgl:J-640x2000mm 4:362091", "Doors_IntSgl:J-640x2000mm 4:362272" (+1 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:362165", "Doors_IntSgl:J-640x2000mm 4:362230" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          38 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:362666", "Windows_Sgl_Plain:J- 900x910mm 2:362968", "Windows_Sgl_Plain:J- 900x910mm 2:363042" (+35 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          21 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:367281", "Windows_Sgl_Plain:J- 900x910mm 2:367460", "Windows_Sgl_Plain:J- 900x910mm 2:367558" (+18 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:405445", "Concrete Square:300 x 300mm:408988" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | object type "Concrete Square:400 x 400mm" | names: "Concrete Square:400 x 400mm:407379" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:408853" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Rectangular:300 x 450mm" | object type "Rectangular:300 x 450mm" | names: "Rectangular:300 x 450mm:410350" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Single-Narrow Frame w Glass:900 x 2000" | object type "Single-Narrow Frame w Glass:900 x 2000" | names: "Single-Narrow Frame w Glass:900 x 2000:413108" | material: materials ("Metal - Chrome", "Default Frame", "J-MURS-RIDEAUX_Glass") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          29 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte" | object type "Curtain Wall:J- wall latte" | names: "Curtain Wall:J- wall latte:414120", "Curtain Wall:J- wall latte:420663", "Curtain Wall:J- wall latte:421310" (+26 more) | parts: 481 IFCPLATE, 460 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          6 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte plant" | object type "Curtain Wall:J- wall latte plant" | names: "Curtain Wall:J- wall latte plant:422046", "Curtain Wall:J- wall latte plant:429051", "Curtain Wall:J- wall latte plant:429513" (+3 more) | parts: 115 IFCPLATE, 109 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:434419" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 24 bloc Wall-Partn" | object type "Basic Wall:J- 24 bloc Wall-Partn" | names: "Basic Wall:J- 24 bloc Wall-Partn:514247" | material: layers "Basic Wall:J- 24 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.20000000000000001, "Plaster" 0.02) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          2 x IFCSTAIR | object type "Assembled Stair:Private" | names: "Assembled Stair:Stair:520367", "Assembled Stair:Stair:675076" | parts: 7 IFCMEMBER, 3 IFCRAILING, 2 IFCSTAIRFLIGHT | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_StairCommon, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:538230" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Siliding:1200 x 2100 mm" | object type "Siliding:1200 x 2100 mm" | names: "Siliding:1200 x 2100 mm:538311" | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:539451", "Basic Wall:EXT_M-ext-01 (FT FA-02:926754" | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          17 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | object type "Windows_Sgl_Plain:J- 820x910mm" | names: "Windows_Sgl_Plain:J- 820x910mm:543183", "Windows_Sgl_Plain:J- 820x910mm:543521", "Windows_Sgl_Plain:J- 820x910mm:543711" (+14 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          18 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | object type "Windows_Sgl_Plain:J- 1270x910mm 2" | names: "Windows_Sgl_Plain:J- 1270x910mm 2:544925", "Windows_Sgl_Plain:J- 1270x910mm 2:545264", "Windows_Sgl_Plain:J- 1270x910mm 2:545336" (+15 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:639630" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          14 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:926760", "Doors_IntSgl:J-1000x2110mm 2:926761", "Doors_IntSgl:J-1000x2110mm 2:926762" (+11 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:926804", "Doors_IntSgl:J-640x2000mm 4:926805" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:926807", "Doors_IntSgl:J-640x2000mm 4:926808" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:926809" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          10 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:926812", "Doors_IntSgl:J-1000x2110mm 2:926817", "Doors_IntSgl:J-1000x2110mm 2:926819" (+7 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:930504" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCGRID | names: "Default Grid"
        IFCSPACE "1" | long name "Stairs" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Electric Lift-4 Person Wall Based:Type 1" | object type "M_Electric Lift-4 Person Wall Based:Type 1" | names: "M_Electric Lift-4 Person Wall Based:Type 1:513614" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Electrical - Loads, Constraints
        IFCSPACE "4" | long name "SDR 6P" | INTERNAL
        IFCSPACE "9" | long name "Technique" | INTERNAL
        IFCSPACE "10" | long name "Technique" | INTERNAL
        IFCSPACE "11" | long name "WC" | INTERNAL
        IFCSPACE "16" | long name "Technique" | INTERNAL
        IFCSPACE "17" | long name "Salle Créative" | INTERNAL
        IFCSPACE "18" | long name "Technique" | INTERNAL
        IFCSPACE "19" | long name "Technique" | INTERNAL
        IFCSPACE "22" | long name "Bureau" | INTERNAL
        IFCSPACE "23" | long name "Cockpit" | INTERNAL
        IFCSPACE "24" | long name "Cockpit" | INTERNAL
        IFCSPACE "26" | long name "Bureau" | INTERNAL
        IFCSPACE "27" | long name "Bureau" | INTERNAL
        IFCSPACE "28" | long name "Bureau" | INTERNAL
        IFCSPACE "31" | long name "SDR 4P" | INTERNAL
        IFCSPACE "32" | long name "Bureau" | INTERNAL
        IFCSPACE "33" | long name "Bureau" | INTERNAL
        IFCSPACE "34" | long name "Bureau" | INTERNAL
        IFCSPACE "37" | long name "SDR 4P" | INTERNAL
        IFCSPACE "38" | long name "Open Spaces" | INTERNAL
        IFCSPACE "39" | long name "SDR" | INTERNAL
        IFCSPACE "40" | long name "SDR" | INTERNAL
        IFCSPACE "41" | long name "Bureau" | INTERNAL
        IFCSPACE "42" | long name "Technique" | INTERNAL
        IFCSPACE "45" | long name "Bureau" | INTERNAL
        IFCSPACE "47" | long name "Technique" | INTERNAL
        IFCSPACE "50" | long name "Cockpit" | INTERNAL
        IFCSPACE "52" | long name "Cockpit" | INTERNAL
        IFCSPACE "53" | long name "WC" | INTERNAL
        IFCSPACE "54" | long name "Couloir" | INTERNAL
        IFCSPACE "97" | long name "Bureau" | INTERNAL
        IFCSPACE "410" | long name "Bureau" | INTERNAL
        IFCSPACE "454" | long name "Kitchen" | INTERNAL
        IFCSPACE "455" | long name "Technique" | INTERNAL
        IFCSPACE "458" | long name "WC" | INTERNAL
        IFCSPACE "462" | long name "Stairs" | INTERNAL
        IFCSPACE "463" | long name "Bureau" | INTERNAL
        IFCSPACE "469" | long name "Bureau" | INTERNAL
        IFCSPACE "470" | long name "Bureau" | INTERNAL
        IFCSPACE "471" | long name "Bureau" | INTERNAL
        IFCSPACE "472" | long name "Bureau" | INTERNAL
        IFCSPACE "473" | long name "Bureau" | INTERNAL
        IFCSPACE "474" | long name "Bureau" | INTERNAL
        IFCSPACE "475" | long name "Bureau" | INTERNAL
        IFCSPACE "476" | long name "Bureau" | INTERNAL
        IFCSPACE "477" | long name "Bureau" | INTERNAL
        IFCSPACE "478" | long name "Bureau" | INTERNAL
        IFCSPACE "479" | long name "Bureau" | INTERNAL
        IFCSPACE "480" | long name "Bureau" | INTERNAL
        IFCSPACE "481" | long name "Bureau" | INTERNAL
        IFCSPACE "482" | long name "SDR 16p" | INTERNAL
        IFCSPACE "483" | long name "Bureau" | INTERNAL
        IFCSPACE "484" | long name "Bureau" | INTERNAL
        IFCSPACE "485" | long name "Bureau" | INTERNAL
        IFCSPACE "487" | long name "Bureau" | INTERNAL
        IFCSPACE "488" | long name "Bureau" | INTERNAL
        IFCSPACE "489" | long name "Bureau" | INTERNAL
        IFCSPACE "490" | long name "Bureau" | INTERNAL
        IFCSPACE "491" | long name "Bureau" | INTERNAL
        IFCSPACE "492" | long name "Bureau" | INTERNAL
        IFCSPACE "493" | long name "Bureau" | INTERNAL
        IFCSPACE "494" | long name "Bureau" | INTERNAL
        IFCSPACE "495" | long name "Bureau" | INTERNAL
        IFCSPACE "496" | long name "Bureau" | INTERNAL
        IFCSPACE "497" | long name "Couloir" | INTERNAL
        IFCSPACE "498" | long name "Bureau" | INTERNAL
        IFCSPACE "499" | long name "Couloir" | INTERNAL
        IFCSPACE "500" | long name "Bureau" | INTERNAL
        IFCSPACE "501" | long name "Couloir" | INTERNAL
        IFCSPACE "505" | long name "Atrium" | INTERNAL
        IFCSPACE "260" | long name "Space" | INTERNAL
        IFCSPACE "261" | long name "Space" | INTERNAL
        IFCSPACE "264" | long name "Space" | INTERNAL
        IFCSPACE "267" | long name "Space" | INTERNAL
        IFCSPACE "269" | long name "Space" | INTERNAL
        IFCSPACE "270" | long name "Space" | INTERNAL
        IFCSPACE "271" | long name "Space" | INTERNAL
        IFCSPACE "272" | long name "Space" | INTERNAL
        IFCSPACE "274" | long name "Space" | INTERNAL
        IFCSPACE "275" | long name "Space" | INTERNAL
        IFCSPACE "277" | long name "Space" | INTERNAL
        IFCSPACE "278" | long name "Space" | INTERNAL
        IFCSPACE "279" | long name "Space" | INTERNAL
        IFCSPACE "280" | long name "Space" | INTERNAL
        IFCSPACE "281" | long name "Space" | INTERNAL
        IFCSPACE "282" | long name "Space" | INTERNAL
        IFCSPACE "283" | long name "Space" | INTERNAL
        IFCSPACE "285" | long name "Space" | INTERNAL
        IFCSPACE "286" | long name "Space" | INTERNAL
        IFCSPACE "287" | long name "Space" | INTERNAL
        IFCSPACE "288" | long name "Space" | INTERNAL
        IFCSPACE "289" | long name "Space" | INTERNAL
        IFCSPACE "290" | long name "Space" | INTERNAL
        IFCSPACE "291" | long name "Space" | INTERNAL
        IFCSPACE "292" | long name "Space" | INTERNAL
        IFCSPACE "293" | long name "Space" | INTERNAL
        IFCSPACE "294" | long name "Space" | INTERNAL
        IFCSPACE "295" | long name "Space" | INTERNAL
        IFCSPACE "296" | long name "Space" | INTERNAL
        IFCSPACE "297" | long name "Space" | INTERNAL
        IFCSPACE "298" | long name "Space" | INTERNAL
        IFCSPACE "299" | long name "Space" | INTERNAL
        IFCSPACE "300" | long name "Space" | INTERNAL
        IFCSPACE "301" | long name "Space" | INTERNAL
        IFCSPACE "302" | long name "Space" | INTERNAL
        IFCSPACE "303" | long name "Space" | INTERNAL
        IFCSPACE "304" | long name "Space" | INTERNAL
        IFCSPACE "305" | long name "Space" | INTERNAL
        IFCSPACE "306" | long name "Space" | INTERNAL
        IFCSPACE "307" | long name "Space" | INTERNAL
        IFCSPACE "308" | long name "Space" | INTERNAL
        IFCSPACE "309" | long name "Space" | INTERNAL
        IFCSPACE "310" | long name "Space" | INTERNAL
        IFCSPACE "311" | long name "Space" | INTERNAL
        IFCSPACE "312" | long name "Space" | INTERNAL
        IFCSPACE "313" | long name "Space" | INTERNAL
        IFCSPACE "314" | long name "Space" | INTERNAL
        IFCSPACE "315" | long name "Space" | INTERNAL
        IFCSPACE "316" | long name "Space" | INTERNAL
        IFCSPACE "317" | long name "Space" | INTERNAL
        IFCSPACE "318" | long name "Space" | INTERNAL
        IFCSPACE "319" | long name "Space" | INTERNAL
        IFCSPACE "320" | long name "Space" | INTERNAL
        IFCSPACE "321" | long name "Space" | INTERNAL
        IFCSPACE "322" | long name "Space" | INTERNAL
        IFCSPACE "323" | long name "Space" | INTERNAL
        IFCSPACE "324" | long name "Space" | INTERNAL
        IFCSPACE "325" | long name "Space" | INTERNAL
        IFCSPACE "326" | long name "Space" | INTERNAL
        IFCSPACE "327" | long name "Space" | INTERNAL
        IFCSPACE "328" | long name "Space" | INTERNAL
        IFCSPACE "330" | long name "Space" | INTERNAL
        IFCSPACE "332" | long name "Space" | INTERNAL
        IFCSPACE "333" | long name "Space" | INTERNAL
        IFCSPACE "334" | long name "Space" | INTERNAL
        IFCSPACE "335" | long name "Space" | INTERNAL
        IFCSPACE "336" | long name "Space" | INTERNAL
        IFCSPACE "338" | long name "Space" | INTERNAL
        IFCSPACE "339" | long name "Space" | INTERNAL
        IFCSPACE "342" | long name "Space" | INTERNAL
        IFCSPACE "343" | long name "Space" | INTERNAL
      IFCBUILDINGSTOREY "int plafond Etage 1" | long name "int plafond Etage 1" | object type "Level:Circle Head - Project Datum" | elevation 6.7219918120248439
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Etage 2" | long name "Etage 2" | object type "Level:Circle Head - Project Datum" | elevation 7.0019918120248494
        contains 239 elements
          105 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:541190", "Basic Wall:Wall-Partn_12P-75Std-12P:541195", "Basic Wall:Wall-Partn_12P-75Std-12P:541200" (+102 more) | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | object type "Basic Wall:Wall-Partn_12P-75Std-12P" | names: "Basic Wall:Wall-Partn_12P-75Std-12P:541570", "Basic Wall:Wall-Partn_12P-75Std-12P:541596", "Basic Wall:Wall-Partn_12P-75Std-12P:682767" | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_22" | object type "Basic Wall:J- escalier Wall-Int_22" | names: "Basic Wall:J- escalier Wall-Int_22:551785", "Basic Wall:J- escalier Wall-Int_22:551892", "Basic Wall:J- escalier Wall-Int_22:551995" (+21 more) | material: layers "Basic Wall:J- escalier Wall-Int_22" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Toiture en verre Atrium" | object type "Compound Ceiling:Toiture en verre Atrium" | CEILING | names: "Compound Ceiling:Toiture en verre Atrium:676755" | material: layers "Compound Ceiling:Toiture en verre Atrium" ("J-Glass λU=0.91" 0.035999999999999997, "Ceiling Tile 600 x 1200" 0.015999999999999997) | property sets: Pset_CoveringCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:682571", "Basic Wall:EXT_M-ext-01 (FT FA-02:682572", "Basic Wall:EXT_M-ext-01 (FT FA-02:682573" (+17 more) | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Text
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:682584", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:682590", "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3:682592" (+3 more) | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.125, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          14 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | object type "Windows_Sgl_Plain:J- 1270x910mm 2" | names: "Windows_Sgl_Plain:J- 1270x910mm 2:682606", "Windows_Sgl_Plain:J- 1270x910mm 2:682607", "Windows_Sgl_Plain:J- 1270x910mm 2:682616" (+11 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          12 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | object type "Windows_Sgl_Plain:J- 820x910mm" | names: "Windows_Sgl_Plain:J- 820x910mm:682608", "Windows_Sgl_Plain:J- 820x910mm:682609", "Windows_Sgl_Plain:J- 820x910mm:682610" (+9 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | object type "Windows_Sgl_Plain:J- 900x910mm 2" | names: "Windows_Sgl_Plain:J- 900x910mm 2:682618", "Windows_Sgl_Plain:J- 900x910mm 2:682619", "Windows_Sgl_Plain:J- 900x910mm 2:682632" (+2 more) | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | object type "Basic Wall:EXT_M-ext-01 (FT FA-02" | names: "Basic Wall:EXT_M-ext-01 (FT FA-02:682633", "Basic Wall:EXT_M-ext-01 (FT FA-02:682635" | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          5 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682638", "Doors_IntSgl:J-1000x2110mm 2:682647", "Doors_IntSgl:J-1000x2110mm 2:682694" (+2 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          10 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682640", "Doors_IntSgl:J-1000x2110mm 2:682641", "Doors_IntSgl:J-1000x2110mm 2:682691" (+7 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:682684", "Doors_IntSgl:J-640x2000mm 4:682685" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | object type "Doors_IntSgl:J-640x2000mm 4" | names: "Doors_IntSgl:J-640x2000mm 4:682687", "Doors_IntSgl:J-640x2000mm 4:682688" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682689" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682690", "Doors_IntSgl:J-1000x2110mm 2:683037" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          5 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682692", "Doors_IntSgl:J-1000x2110mm 2:682697", "Doors_IntSgl:J-1000x2110mm 2:682702" (+2 more) | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682710" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682711" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | object type "Doors_IntSgl:J-1000x2110mm 2" | names: "Doors_IntSgl:J-1000x2110mm 2:682723" | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | object type "Windows_Sgl_Plain:J- 1270x910mm 2" | names: "Windows_Sgl_Plain:J- 1270x910mm 2:682730" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | object type "Concrete Square:300 x 300mm" | names: "Concrete Square:300 x 300mm:682769", "Concrete Square:300 x 300mm:682771" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints, Phasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | object type "Windows_Sgl_Plain:J- 820x910mm" | names: "Windows_Sgl_Plain:J- 820x910mm:683286", "Windows_Sgl_Plain:J- 820x910mm:683287" | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Text, Constraints, Phasing
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte" | object type "Curtain Wall:J- wall latte" | names: "Curtain Wall:J- wall latte:683295", "Curtain Wall:J- wall latte:683394", "Curtain Wall:J- wall latte:683594" (+1 more) | parts: 71 IFCPLATE, 69 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Cross-Section Definition, Horizontal Grid, Vertical Grid
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Plancher/plafond_ J_R2 0.38" | object type "Floor:Plancher/plafond_ J_R2 0.38" | FLOOR | names: "Floor:Plancher/plafond_ J_R2 0.38:683951" | material: layers "Floor:Plancher/plafond_ J_R2 0.38" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.10000000000000001, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.28000000000000003, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | object type "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | names: "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:766064", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:766065", "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3:766066" | material: layers "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.185, "Plaster" 0.012500000000000001) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Cross-Section Definition, Constraints
          1 x IFCROOF | object type "Basic Roof:EXT_Toiture principale_T-ext-" | names: "Basic Roof:EXT_Toiture principale_T-ext-:788983" | parts: 1 IFCSLAB | material: layers "Basic Roof:EXT_Toiture principale_T-ext-" ("J-EXT_Toiture principale-Membrane bitumineuse (Divers)- λU=0.23 Asphalt, Bitumen" 0.0050000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.28000000000000003) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Phasing, Construction
          1 x IFCROOF | object type "Basic Roof:EXT_Toiture atrium_T-ext-02" | names: "Basic Roof:EXT_Toiture atrium_T-ext-02:789923" | material: layers "Basic Roof:EXT_Toiture atrium_T-ext-02" ("J-EXT_Toiture principale-Membrane bitumineuse (Divers)- λU=0.23 Asphalt, Bitumen" 0.0050000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.28000000000000003) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Phasing, Construction
          2 x IFCGRID | names: "Default Grid"
        IFCSPACE "204" | long name "Bureau" | INTERNAL
        IFCSPACE "205" | long name "SDR 6P" | INTERNAL
        IFCSPACE "206" | long name "Bureau" | INTERNAL
        IFCSPACE "207" | long name "Bureau" | INTERNAL
        IFCSPACE "208" | long name "Bureau" | INTERNAL
        IFCSPACE "209" | long name "Bureau" | INTERNAL
        IFCSPACE "212" | long name "Technique" | INTERNAL
        IFCSPACE "214" | long name "Stairs" | INTERNAL
        IFCSPACE "215" | long name "Technique" | INTERNAL
        IFCSPACE "216" | long name "Technique" | INTERNAL
        IFCSPACE "218" | long name "Bureau" | INTERNAL
        IFCSPACE "219" | long name "WC" | INTERNAL
        IFCSPACE "220" | long name "Couloir" | INTERNAL
        IFCSPACE "221" | long name "Bureau" | INTERNAL
        IFCSPACE "222" | long name "Bureau" | INTERNAL
        IFCSPACE "223" | long name "Bureau" | INTERNAL
        IFCSPACE "224" | long name "Bureau" | INTERNAL
        IFCSPACE "225" | long name "Couloir" | INTERNAL
        IFCSPACE "226" | long name "SDR 4P" | INTERNAL
        IFCSPACE "227" | long name "Bureau" | INTERNAL
        IFCSPACE "228" | long name "Bureau" | INTERNAL
        IFCSPACE "229" | long name "Bureaux TS" | INTERNAL
        IFCSPACE "230" | long name "Couloir" | INTERNAL
        IFCSPACE "231" | long name "Couloir" | INTERNAL
        IFCSPACE "232" | long name "Bureau" | INTERNAL
        IFCSPACE "233" | long name "Bureau" | INTERNAL
        IFCSPACE "234" | long name "Technique" | INTERNAL
        IFCSPACE "235" | long name "Bureau" | INTERNAL
        IFCSPACE "236" | long name "Bureau" | INTERNAL
        IFCSPACE "237" | long name "Atrium" | INTERNAL
        IFCSPACE "239" | long name "SDR 4P" | INTERNAL
        IFCSPACE "240" | long name "Cockpit" | INTERNAL
        IFCSPACE "241" | long name "Cockpit" | INTERNAL
        IFCSPACE "242" | long name "Bureaux SAV" | INTERNAL
        IFCSPACE "420" | long name "Bureau" | INTERNAL
        IFCSPACE "421" | long name "Bureau" | INTERNAL
        IFCSPACE "422" | long name "Bureau" | INTERNAL
        IFCSPACE "424" | long name "Bureau" | INTERNAL
        IFCSPACE "425" | long name "Bureau" | INTERNAL
        IFCSPACE "428" | long name "Bureau" | INTERNAL
        IFCSPACE "429" | long name "Bureau" | INTERNAL
        IFCSPACE "437" | long name "Bureau" | INTERNAL
        IFCSPACE "441" | long name "Bureau" | INTERNAL
        IFCSPACE "445" | long name "Bureau" | INTERNAL
        IFCSPACE "446" | long name "Bureau" | INTERNAL
        IFCSPACE "447" | long name "Bureau" | INTERNAL
        IFCSPACE "448" | long name "Bureau" | INTERNAL
        IFCSPACE "450" | long name "Couloir" | INTERNAL
        IFCSPACE "507" | long name "Room" | INTERNAL
        IFCSPACE "510" | long name "Room" | INTERNAL
        IFCSPACE "512" | long name "Room" | INTERNAL
        IFCSPACE "513" | long name "Room" | INTERNAL
        IFCSPACE "346" | long name "Space" | INTERNAL
        IFCSPACE "348" | long name "Space" | INTERNAL
        IFCSPACE "349" | long name "Space" | INTERNAL
        IFCSPACE "350" | long name "Space" | INTERNAL
        IFCSPACE "352" | long name "Space" | INTERNAL
        IFCSPACE "353" | long name "Space" | INTERNAL
        IFCSPACE "354" | long name "Space" | INTERNAL
        IFCSPACE "355" | long name "Space" | INTERNAL
        IFCSPACE "356" | long name "Space" | INTERNAL
        IFCSPACE "357" | long name "Space" | INTERNAL
        IFCSPACE "358" | long name "Space" | INTERNAL
        IFCSPACE "359" | long name "Space" | INTERNAL
        IFCSPACE "360" | long name "Space" | INTERNAL
        IFCSPACE "361" | long name "Space" | INTERNAL
        IFCSPACE "362" | long name "Space" | INTERNAL
        IFCSPACE "363" | long name "Space" | INTERNAL
        IFCSPACE "364" | long name "Space" | INTERNAL
        IFCSPACE "365" | long name "Space" | INTERNAL
        IFCSPACE "366" | long name "Space" | INTERNAL
        IFCSPACE "367" | long name "Space" | INTERNAL
        IFCSPACE "368" | long name "Space" | INTERNAL
        IFCSPACE "369" | long name "Space" | INTERNAL
        IFCSPACE "370" | long name "Space" | INTERNAL
        IFCSPACE "371" | long name "Space" | INTERNAL
        IFCSPACE "372" | long name "Space" | INTERNAL
        IFCSPACE "373" | long name "Space" | INTERNAL
        IFCSPACE "375" | long name "Space" | INTERNAL
        IFCSPACE "376" | long name "Space" | INTERNAL
        IFCSPACE "377" | long name "Space" | INTERNAL
        IFCSPACE "378" | long name "Space" | INTERNAL
        IFCSPACE "379" | long name "Space" | INTERNAL
        IFCSPACE "380" | long name "Space" | INTERNAL
        IFCSPACE "381" | long name "Space" | INTERNAL
        IFCSPACE "382" | long name "Space" | INTERNAL
        IFCSPACE "383" | long name "Space" | INTERNAL
        IFCSPACE "384" | long name "Space" | INTERNAL
        IFCSPACE "385" | long name "Space" | INTERNAL
        IFCSPACE "386" | long name "Space" | INTERNAL
        IFCSPACE "387" | long name "Space" | INTERNAL
        IFCSPACE "388" | long name "Space" | INTERNAL
        IFCSPACE "389" | long name "Space" | INTERNAL
        IFCSPACE "390" | long name "Space" | INTERNAL
        IFCSPACE "391" | long name "Space" | INTERNAL
        IFCSPACE "392" | long name "Space" | INTERNAL
        IFCSPACE "393" | long name "Space" | INTERNAL
        IFCSPACE "395" | long name "Space" | INTERNAL
        IFCSPACE "397" | long name "Space" | INTERNAL
        IFCSPACE "398" | long name "Space" | INTERNAL
      IFCBUILDINGSTOREY "Upper wall Toiture" | long name "Upper wall Toiture" | object type "Level:Circle Head - Project Datum" | elevation 7.5219918120248437
        contains 2 elements
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Toiture Escalier" | long name "Toiture Escalier" | object type "Level:Circle Head - Project Datum" | elevation 9.4219974716738353
        contains 4 elements
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:EXT_Toiture_T-ext-03 (FT" | object type "Compound Ceiling:EXT_Toiture_T-ext-03 (FT" | CEILING | names: "Compound Ceiling:EXT_Toiture_T-ext-03 (FT:758274", "Compound Ceiling:EXT_Toiture_T-ext-03 (FT:766169" | material: layers "Compound Ceiling:EXT_Toiture_T-ext-03 (FT" ("J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.59999999999999987) | property sets: Pset_CoveringCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Phasing, Dimensions
          2 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Toiture 2ème étage" | long name "Toiture 2ème étage" | object type "Level:Circle Head - Project Datum" | elevation 10.551997471673735
        contains 3 elements
          1 x IFCROOF | object type "Basic Roof:EXT_Toiture principale_T-ext-" | names: "Basic Roof:EXT_Toiture principale_T-ext-:788823" | parts: 1 IFCSLAB | material: layers "Basic Roof:EXT_Toiture principale_T-ext-" ("J-EXT_Toiture principale-Membrane bitumineuse (Divers)- λU=0.23 Asphalt, Bitumen" 0.0050000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J- EXT_Toiture principale- IKO insulations BV/PIR Enertherm ALU -λU=0.023 (EIFS, Exterior Insulation)" 0.10000000000000001, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.28000000000000003) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Phasing, Construction
          2 x IFCGRID | names: "Default Grid"

Types
  IFCWALLTYPE "Basic Wall:CAVE_M-cave-01 (Fibraroc" | STANDARD | 4 occurrences | material: layers "Basic Wall:CAVE_M-cave-01 (Fibraroc" ("J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.29999999999999993, "Rigid insulation" 0.12499999999999999) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Sliding Door - 4 Panel (AUS):Type 1" | 1 occurrence | material: materials ("Sliding Door Glass", "Sliding Door Frame") | property sets: Sliding Door - 4 Panel (AUS):Type 1:839914, Sliding Door - 4 Panel (AUS):Type 1:839914:1, Analytical Properties, Construction, Dimensions, Identity Data
  IFCSLABTYPE "Floor:***PKG_Dalle sur parking_D-" | FLOOR | 1 occurrence | material: layers "Floor:***PKG_Dalle sur parking_D-" ("J- Cave-Linoléum, carreaux de PVC (Divers) λ=0.19- (TENACITY-Vinilo-LOSETA)" 0.0050000000000000001, "J- Cave-Béton léger en dalles, panneaux pleins ou chape (Eléments de construction pierreux sans joints) λ=0.12 (Concrete, Lightweight, 50)" 0.080000000000000002, "J- Cave/SOL_Dalla_Atrium-Nestaan Holland BV λU=0.026" 0.20000000000000001, "J- Toiture principale/cave-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=1.7-GFRC" 0.34999999999999998) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCCOLUMNTYPE "UC-Universal Columns-Column:UC305x305x97" | COLUMN | 1 occurrence | material: "Metal - Steel 43-275" | property sets: Structural Section Geometry, Structural Analysis, Structural, Dimensions, Identity Data, Other
  IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Rectangular:300 x 450mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCWALLTYPE "Basic Wall:Wall-Partn_12P-75Std-12P" | STANDARD | 433 occurrences | material: layers "Basic Wall:Wall-Partn_12P-75Std-12P" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J- 10 bloc Wall-Partn" | STANDARD | 85 occurrences | material: layers "Basic Wall:J- 10 bloc Wall-Partn" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.075000000000000011, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:EXT_M-ext-01 (FT FA-02" | STANDARD | 100 occurrences | material: layers "Basic Wall:EXT_M-ext-01 (FT FA-02" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" | STANDARD | 32 occurrences | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.125, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" | STANDARD | 61 occurrences | material: layers "Basic Wall:J- 21 bloc-Wall-Partn_12P-75Std-12P 3" ("Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.185, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" | STANDARD | 7 occurrences | material: layers "Basic Wall:J- 22 bloc-Wall-Partn_12P-75Std-12P 4" ("Plaster" 0.012500000000000001, "Air Infiltration Barrier" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_22" | STANDARD | 90 occurrences | material: layers "Basic Wall:J- escalier Wall-Int_22" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 8 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | SINGLE_SWING_LEFT | 7 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Doors_IntSgl:J-640x2000mm 4:361908, Doors_IntSgl:J-640x2000mm 4:361908:1, Analytical Properties, Constraints, Materials and Finishes, Graphics
  IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | SINGLE_SWING_RIGHT | 5 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 6 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCURTAINWALLTYPE "Curtain Wall:SH_Curtain wall" | 68 occurrences | property sets: Horizontal Mullions, Vertical Mullions, Horizontal Grid, Vertical Grid, Construction, Identity Data
  IFCCOLUMNTYPE "Rectangular:300 x 450mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte" | 71 occurrences | property sets: Vertical Mullions, Horizontal Grid, Vertical Grid, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Siliding:1200 x 2100 mm" | 3 occurrences | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Other(Type), Siliding:1200 x 2100 mm:538230
  IFCDOORSTYLE "Siliding:1200 x 2100 mm" | 3 occurrences | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Other(Type), Siliding:1200 x 2100 mm:538311
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 39 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 24 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCWALLTYPE "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone" | STANDARD | 4 occurrences | material: layers "Basic Wall:J-19-Wall-Partn_12P-75Std-12P with stone" ("Brick, Engineering, Grey" 0.059999999999999998, "Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.18999999999999997, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCDOORSTYLE "Double-Standard Frame w Glass:1770 x 2500" | DOUBLE_DOOR_SINGLE_SWING | 6 occurrences | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Double-Standard Frame w Glass:1770 x 2500:671404, Double-Standard Frame w Glass:1770 x 2500:671404:1, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2" | STANDARD | 2 occurrences | material: layers "Basic Wall:Mur de soutenement- Wall-Ext_102Bwk-50Air-45Ins-100DBlk-12P 2" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)" 0.01, "J- Sto-Isolant PSE (Rigid insulation)" 0.22, "J- Briques/blocs silico-calcaires (Eléments de maçonneries)" 0.17499999999999999, "J- Plâtre avec granulat léger (Plâtres, mortiers et enduits)" 0.01) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_LEFT | 4 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCWALLTYPE "Basic Wall:J- 27 bloc Wall-Partn" | STANDARD | 1 occurrence | material: layers "Basic Wall:J- 27 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.23000000000000001, "Plaster" 0.02) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWALLTYPE "Basic Wall:J- 35 bloc Wall-Partn" | STANDARD | 3 occurrences | material: layers "Basic Wall:J- 35 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.23000000000000001, "Concrete Masonry Units _Low Density" 0.12, "Plaster" 0.02) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCCOLUMNTYPE "Concrete Square:400 x 400mm with cover" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete Square:400 x 400mm with cover" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | SINGLE_SWING_RIGHT | 8 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 6 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1400x2110mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Doors_IntSgl:J-1400x2110mm:750830, Doors_IntSgl:J-1400x2110mm:750830:1, Analytical Properties, Constraints, Materials and Finishes, Graphics
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 2000x910mm 3" | SINGLE_PANEL | 3 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Windows_Sgl_Plain:J- 2000x910mm 3:755806, Analytical Properties, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Double-Standard Frame-Variable:J-1800 x 2000" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: materials ("Metal - Chrome", "Default Frame") | property sets: Double-Standard Frame-Variable:J-1800 x 2000:756339, Double-Standard Frame-Variable:J-1800 x 2000:756339:1, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12" | STANDARD | 1 occurrence | material: layers "Basic Wall:J- escalier Wall-Int_12P-100Blk-12P_avec finitions 19+12" ("Plaster" 0.012500000000000001, "Concrete Masonry Units" 0.19500000000000001, "Brick, Engineering, Grey" 0.12, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Double-Standard Frame w Glass:2060 x 2500" | DOUBLE_DOOR_SINGLE_SWING | 7 occurrences | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Double-Standard Frame w Glass:2060 x 2500:767743, Double-Standard Frame w Glass:2060 x 2500:767743:1, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | SINGLE_PANEL | 80 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Windows_Sgl_Plain:J- 900x910mm 2:362666, Analytical Properties, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Siliding:1800 x 2100 mm" | 1 occurrence | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Siliding:1800 x 2100 mm:775181
  IFCDOORSTYLE "Double-Standard Frame-Variable:J-1800 x 2000" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("Metal - Chrome", "Default Frame") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Double-Standard Frame-Variable:J-1800 x 2000:775819
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCSLABTYPE "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" | FLOOR | 1 occurrence | material: layers "Floor:Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.014999999999999999, "J-SOL_Dalle_Atrium/Sous-sol/TP-Béton lourd normal non armé (Eléments de construction pierreux sans joints)- λU=1.3" 0.080000000000000002, "J-SOL_Dalle_Atrium/Sous-sol-Béton lourd normal armé (Eléments de construction pierreux sans joints)- λU=2.2-GFRC" 0.34999999999999998) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCSLABTYPE "Floor:Plancher/plafond_ J_RDC 0.47" | FLOOR | 5 occurrences | material: layers "Floor:Plancher/plafond_ J_RDC 0.47" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.12, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.34999999999999998, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "M_Electric Lift-4 Person Wall Based:Type 1" | 3 occurrences | material: "<Unnamed>" | property sets: Constraints(Type), Identity Data(Type), Other(Type), Pset_ProductRequirements
  IFCSLABTYPE "Floor:Floor Ramp" | FLOOR | 1 occurrence | material: layers "Floor:Floor Ramp" ("J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01, "J- Béton léger en dalles, panneaux pleins ou chape (Eléments de construction pierreux sans joints) λ=0.14 Plancher (Concrete, Lightweight, 4 ksi)" 0.089999999999999997) | property sets: Analytical Properties, Graphics, Construction, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:J- 24 bloc Wall-Partn" | STANDARD | 3 occurrences | material: layers "Basic Wall:J- 24 bloc Wall-Partn" ("Plaster" 0.02, "Concrete Masonry Units _High Density" 0.20000000000000001, "Plaster" 0.02) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 21 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-920x2110mm 3" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Doors_IntSgl:J-920x2110mm 3:360002, Doors_IntSgl:J-920x2110mm 3:360002:1, Analytical Properties, Constraints, Materials and Finishes, Graphics
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Doors_IntSgl:J-900x2110mm 3:360536, Doors_IntSgl:J-900x2110mm 3:360536:1, Analytical Properties, Constraints, Materials and Finishes, Graphics
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 900x910mm 2" | SINGLE_PANEL | 53 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Dimensions, Identity Data
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 3 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCURTAINWALLTYPE "Curtain Wall:J- wall latte plant" | 21 occurrences | property sets: Vertical Mullions, Horizontal Grid, Vertical Grid, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 20 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | SINGLE_PANEL | 46 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Analytical Properties(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type), Identity Data(Type)
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | SINGLE_PANEL | 41 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Analytical Properties(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type), Identity Data(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-640x2000mm 4" | SINGLE_SWING_LEFT | 6 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 1270x910mm 2" | SINGLE_PANEL | 2 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Analytical Properties(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type), Identity Data(Type)
  IFCWALLTYPE "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone" | STANDARD | 6 occurrences | material: layers "Basic Wall:J-14-Wall-Partn_12P-75Std-12P with stone" ("Brick, Engineering, Grey" 0.059999999999999998, "Plaster" 0.012500000000000001, "Concrete Masonry Units _High Density" 0.12499999999999999, "Plaster" 0.012500000000000001) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCWINDOWSTYLE "Windows_Sgl_Plain:J- 820x910mm" | SINGLE_PANEL | 4 occurrences | material: materials ("Window Frame", "J-Glass λU=0.91") | property sets: Analytical Properties(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type), Identity Data(Type)
  IFCDOORSTYLE "Siliding:1800 x 2100 mm" | 1 occurrence | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Siliding:1800 x 2100 mm:670720, Siliding:1800 x 2100 mm:670720:1, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "Siliding:1800 x 2100 mm" | 1 occurrence | material: materials ("Glass (2)", "Light Wood", "Dark Wood") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Siliding:1800 x 2100 mm:671480
  IFCDOORSTYLE "Double-Standard Frame w Glass:1770 x 2500" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("J-MURS-RIDEAUX_Glass", "Metal - Chrome", "Default Frame") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Double-Standard Frame w Glass:1770 x 2500:671481
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 3 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCSLABTYPE "Floor:Plancher/plafond_ J_R1 0.38" | FLOOR | 3 occurrences | material: layers "Floor:Plancher/plafond_ J_R1 0.38" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.10000000000000001, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.28000000000000003, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCDOORSTYLE "Doors_IntSgl:J-900x2110mm 3" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties, Constraints, Materials and Finishes, Graphics, Construction, Dimensions
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete Square:400 x 400mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Rectangular:300 x 450mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCDOORSTYLE "Single-Narrow Frame w Glass:900 x 2000" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Metal - Chrome", "Default Frame", "J-MURS-RIDEAUX_Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Other(Type), Single-Narrow Frame w Glass:900 x 2000:413108
  IFCDOORSTYLE "Doors_IntSgl:J-1000x2110mm 2" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Architrave", "Door - Frame/Mullion (1)") | property sets: Analytical Properties(Type), Constraints(Type), Materials and Finishes(Type), Graphics(Type), Construction(Type), Dimensions(Type)
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOVERINGTYPE "Compound Ceiling:Toiture en verre Atrium" | CEILING | 1 occurrence | property sets: Analytical Properties, Graphics, Construction, Identity Data, Other, Pset_CoveringCommon
  IFCCOLUMNTYPE "Concrete Square:300 x 300mm" | COLUMN | 2 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Structural, Dimensions, Identity Data, Other, Pset_ColumnCommon, Pset_ProductRequirements
  IFCSLABTYPE "Floor:Plancher/plafond_ J_R2 0.38" | FLOOR | 1 occurrence | material: layers "Floor:Plancher/plafond_ J_R2 0.38" ("J-Pancher/SOL_Dalle_Sous-sol_D-sol-01-Carreaux de grès (Divers) λU=1.2" 0.10000000000000001, "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" 0.28000000000000003, "J- Mortier de ciment (Plâtres, mortiers et enduits)-(Plaster)(Plancher/Plafond) λU=1.5" 0.01) | property sets: Analytical Properties, Materials and Finishes, Graphics, Construction, Identity Data, Other
  IFCCOVERINGTYPE "Compound Ceiling:EXT_Toiture_T-ext-03 (FT" | CEILING | 2 occurrences | property sets: Analytical Properties, Graphics, Construction, Identity Data, Other, Pset_CoveringCommon

Property sets
  Pset_ProductRequirements | properties | on 2867 objects (2867 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2026 objects (2026 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
  Pset_ProductRequirements | properties | on 996 objects (809 IFCWALLSTANDARDCASE, 160 IFCCURTAINWALL, 23 IFCWALL, 4 IFCOPENINGELEMENT) | on 18 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 308 objects (243 IFCDOOR, 65 IFCOPENINGELEMENT) | on 44 type objects
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 259 objects (229 IFCWINDOW, 30 IFCOPENINGELEMENT) | on 7 type objects
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 204 objects (204 IFCSPACE)
    Category = "Spaces" (IFCLABEL)
    Name = "Space" (IFCLABEL)
  Pset_ProductRequirements | properties | on 136 objects (136 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Name = "Bureau" (IFCLABEL)
  Pset_ProductRequirements | properties | on 28 objects (28 IFCCOLUMN) | on 18 type objects
    Category = "Structural Columns" (IFCLABEL)
  Pset_ProductRequirements: 57 more contents on 221 objects not shown
  Pset_AirSideSystemInformation | properties | on 204 objects (204 IFCSPACE)
    Name = "Space" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 137 objects (137 IFCSPACE)
    Name = "Bureau" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 18 objects (18 IFCSPACE)
    Name = "Technique" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 17 objects (17 IFCSPACE)
    Name = "Couloir" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 12 objects (12 IFCSPACE)
    Name = "Cockpit" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 9 objects (9 IFCSPACE)
    Name = "WC" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 6 objects (5 IFCSPACE, 1 IFCBUILDINGSTOREY)
    Name = "Stairs" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 6 objects (6 IFCSPACE)
    Name = "SDR 4P" (IFCLABEL)
  Pset_AirSideSystemInformation: 36 more contents on 58 objects not shown
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Stairs 1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "SDR 6P 4" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Technique 9" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Technique 10" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "WC 11" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Technique 16" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Salle Créative 17" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Technique 18" (IFCIDENTIFIER)
  Pset_SpaceCommon: 443 more contents on 443 objects not shown
  Pset_QuantityTakeOff | properties | on 2026 objects (2026 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1436 objects (1436 IFCMEMBER)
    Reference = "64 x 128 rectangular" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1427 objects (1427 IFCMEMBER)
    Reference = "30mm_Square" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 435 objects (424 IFCWALLSTANDARDCASE, 9 IFCWALL, 2 IFCOPENINGELEMENT)
    Reference = "Wall-Partn_12P-75Std-12P" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 196 objects (145 IFCDOOR, 51 IFCOPENINGELEMENT)
    Reference = "J-1000x2110mm 2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 140 objects (133 IFCWINDOW, 7 IFCOPENINGELEMENT)
    Reference = "J- 900x910mm 2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 101 objects (87 IFCWALLSTANDARDCASE, 13 IFCWALL, 1 IFCOPENINGELEMENT)
    Reference = "EXT_M-ext-01 (FT FA-02" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 90 objects (90 IFCWALLSTANDARDCASE)
    Reference = "J- escalier Wall-Int_22" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 52 more contents on 725 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 5 objects (5 IFCSLAB)
    Reference = "Plancher/plafond_ J_RDC 0.47" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Reference = "Plancher/plafond_ J_R1 0.38" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Reference = "EXT_Toiture principale_T-ext-" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Plancher/plafond_ J_R2 0.38" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Non-Monolitic_Landing" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor Ramp" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "***PKG_Dalle sur parking_D-" (IFCLABEL)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Plancher/plafond_ J_RDC 0.47" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Plancher/plafond_ J_R1 0.38" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "EXT_Toiture principale_T-ext-" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Plancher/plafond_ J_R2 0.38" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Non-Monolitic_Landing" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor Ramp" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Plancher/plafond_ J_SOL_Dalla_Sous-sol_D-01" (IFCIDENTIFIER)
  Pset_SlabCommon: 6 more contents on 1 objects not shown
  Pset_OpeningElementCommon | properties | on 51 objects (51 IFCOPENINGELEMENT)
    Reference = "J-1000x2110mm 2" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 15 objects (15 IFCOPENINGELEMENT)
    Reference = "J- 820x910mm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 9 objects (9 IFCOPENINGELEMENT)
    Reference = "J-640x2000mm 4" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 8 objects (8 IFCOPENINGELEMENT)
    Reference = "J- 1270x910mm 2" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 7 objects (7 IFCOPENINGELEMENT)
    Reference = "J- 900x910mm 2" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 5 objects (5 IFCOPENINGELEMENT)
    Reference = "Plancher/plafond_ J_R1 0.38" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Reference = "Plancher/plafond_ J_RDC 0.47" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "1200 x 2100 mm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon: 9 more contents on 16 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 433 objects (424 IFCWALLSTANDARDCASE, 9 IFCWALL)
    Reference = "Wall-Partn_12P-75Std-12P" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 100 objects (87 IFCWALLSTANDARDCASE, 13 IFCWALL)
    Reference = "EXT_M-ext-01 (FT FA-02" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 90 objects (90 IFCWALLSTANDARDCASE)
    Reference = "J- escalier Wall-Int_22" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 85 objects (85 IFCWALLSTANDARDCASE)
    Reference = "J- 10 bloc Wall-Partn" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 61 objects (61 IFCWALLSTANDARDCASE)
    Reference = "J- 21 bloc-Wall-Partn_12P-75Std-12P 3" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 32 objects (32 IFCWALLSTANDARDCASE)
    Reference = "J-14-Wall-Partn_12P-75Std-12P 3" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Reference = "J- 22 bloc-Wall-Partn_12P-75Std-12P 4" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Reference = "J-14-Wall-Partn_12P-75Std-12P with stone" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 7 more contents on 18 objects not shown
  Pset_WallCommon | properties | on 273 objects (266 IFCWALLSTANDARDCASE, 7 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-Partn_12P-75Std-12P" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 160 objects (158 IFCWALLSTANDARDCASE, 2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-Partn_12P-75Std-12P" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 82 objects (73 IFCWALLSTANDARDCASE, 9 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "EXT_M-ext-01 (FT FA-02" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 68 objects (68 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "J- 10 bloc Wall-Partn" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 51 objects (51 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "J- escalier Wall-Int_22" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 48 objects (48 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "J- 21 bloc-Wall-Partn_12P-75Std-12P 3" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 39 objects (39 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "J- escalier Wall-Int_22" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 27 objects (27 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "J-14-Wall-Partn_12P-75Std-12P 3" (IFCIDENTIFIER)
  Pset_WallCommon: 33 more contents on 84 objects not shown
  Pset_StairCommon | properties | on 3 objects (3 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "Private" (IFCIDENTIFIER)
    RiserHeight = 0.16095238095237982 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 2. (IFCCOUNTMEASURE)
    Reference = "Private" (IFCIDENTIFIER)
    RiserHeight = 0.16250000000000014 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Private" (IFCIDENTIFIER)
    RiserHeight = 0.16777746335284072 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 11. (IFCCOUNTMEASURE)
    NumberOfTreads = 10. (IFCCOUNTMEASURE)
    Reference = "Private" (IFCIDENTIFIER)
    RiserHeight = 0.1690783850731723 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIRFLIGHT)
    NosingLength = 0.01 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "Wood_Steps_w-50mm_Tread-10mm_Nosing-13mm_Riser" (IFCIDENTIFIER)
    RiserHeight = 0.16095238095237982 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.01 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 2. (IFCCOUNTMEASURE)
    Reference = "Wood_Steps_w-50mm_Tread-10mm_Nosing-13mm_Riser" (IFCIDENTIFIER)
    RiserHeight = 0.16250000000000003 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.01 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Wood_Steps_w-50mm_Tread-10mm_Nosing-13mm_Riser" (IFCIDENTIFIER)
    RiserHeight = 0.16777746335284072 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.01 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 11. (IFCCOUNTMEASURE)
    NumberOfTreads = 10. (IFCCOUNTMEASURE)
    Reference = "Wood_Steps_w-50mm_Tread-10mm_Nosing-13mm_Riser" (IFCIDENTIFIER)
    RiserHeight = 0.1690783850731723 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 416 objects (416 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "64 x 128 rectangular" (IFCIDENTIFIER)
    Span = 3.299994340351136 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 416 objects (416 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "64 x 128 rectangular" (IFCIDENTIFIER)
    Span = 2.9899999999999758 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 344 objects (344 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "30mm_Square" (IFCIDENTIFIER)
    Span = 2.4000000000000004 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 270 objects (270 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "64 x 128 rectangular" (IFCIDENTIFIER)
    Span = 1. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 246 objects (246 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "30mm_Square" (IFCIDENTIFIER)
    Span = 0.9699999999999982 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 163 objects (163 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "30mm_Square" (IFCIDENTIFIER)
    Span = 0.95500000030480037 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 158 objects (158 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "30mm_Square" (IFCIDENTIFIER)
    Span = 1.1500000000000006 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 113 objects (113 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "64 x 128 rectangular" (IFCIDENTIFIER)
    Span = 2.9899999999999767 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon: 115 more contents on 756 objects not shown
  Pset_CurtainWallCommon | properties | on 71 objects (71 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- wall latte" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 68 objects (68 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SH_Curtain wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 21 objects (21 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- wall latte plant" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_PlateCommon | properties | on 2018 objects (2018 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 8 objects (8 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 145 objects (145 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J-1000x2110mm 2" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 29 objects (29 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J-640x2000mm 4" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 21 objects (21 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J-900x2110mm 3" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 17 objects (17 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Door - Single Glass - Framed - push plate (AUS)" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1770 x 2500" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2060 x 2500" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1200 x 2100 mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1800 x 2100 mm" (IFCIDENTIFIER)
  Pset_DoorCommon: 8 more contents on 8 objects not shown
  Pset_WindowCommon | properties | on 132 objects (132 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- 900x910mm 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 47 objects (47 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- 1270x910mm 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 44 objects (44 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- 820x910mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "J- 2000x910mm 3" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "J- 900x910mm 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "J- 820x910mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "J- 1270x910mm 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "J- 2000x910mm 3" (IFCIDENTIFIER)
  Pset_WindowCommon: 1 more content on 0 objects not shown
  Pset_ColumnCommon | properties | on 16 objects (16 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "300 x 300mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "400 x 400mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "400 x 400mm with cover" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "300 x 450mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UC305x305x97" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 18 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 16 objects (16 IFCCOLUMN)
    Reference = "300 x 300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 4 objects (4 IFCCOLUMN)
    Reference = "400 x 400mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 4 objects (4 IFCCOLUMN)
    Reference = "400 x 400mm with cover" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 3 objects (3 IFCCOLUMN)
    Reference = "300 x 450mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "UC305x305x97" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Height = 1.2550067970860657 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape = "Rectangle" (IFCLABEL)
    Width = 2. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Height = 1.2550067970860628 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape = "Rectangle" (IFCLABEL)
    Width = 1.9999999999999996 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Height = 1.2550067970860657 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape = "Rectangle" (IFCLABEL)
    Width = 1.9999999999999996 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    Reference = "EXT_Toiture_T-ext-03 (FT" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Ceiling Tile 600 x 1200;" (IFCTEXT)
    Reference = "Toiture en verre Atrium" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 0.051999999999999998 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 0.78000000000000003 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_RampFlightCommon | properties | on 2 objects (2 IFCRAMPFLIGHT)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_RampFlightCommon | properties | on 1 object (1 IFCRAMPFLIGHT)
    HeadRoom = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Reference = "" (IFCIDENTIFIER)
    Slope = 89.972116344478877 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_RampFlightCommon | properties | on 1 object (1 IFCRAMPFLIGHT)
    HeadRoom = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Reference = "" (IFCIDENTIFIER)
    Slope = 4.7636416907261836 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_RampCommon | properties | on 3 objects (3 IFCRAMP)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Standard" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 1 object (1 IFCRAMPFLIGHT)
    NetArea = 13.572594297451614 [SQUARE_METRE]
    NetVolume = 1.9590644178299934 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCRAMPFLIGHT)
    NetArea = 6.5111476539219666 [SQUARE_METRE]
    NetVolume = 2.8773926976545483 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 8.433353642309708 [SQUARE_METRE]
    NetVolume = 2.5375904477324278 [CUBIC_METRE]
    Perimeter = 12.118432897149468 [METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 834.87043325962713 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "EXT_Toiture principale_T-ext-" (IFCIDENTIFIER)
    TotalArea = 834.87043325962691 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 975.90582375056613 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "EXT_Toiture principale_T-ext-" (IFCIDENTIFIER)
    TotalArea = 946.35141819095247 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 280.54591941530668 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "EXT_Toiture atrium_T-ext-02" (IFCIDENTIFIER)
    TotalArea = 187.56431593999119 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 288.45435017376229 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "EXT_Toiture principale_T-ext-" (IFCIDENTIFIER)
    TotalArea = 288.45435017376263 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RailingCommon | properties | on 13 objects (13 IFCRAILING)
    Height = 1.1000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100mm" (IFCIDENTIFIER)
  Pset_ZoneCommon | properties | on 1 object (1 IFCZONE)
    Category = "HVAC Zones" (IFCLABEL)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 16 objects (16 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 16 (IFCINTEGER)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBLProjectId = "3ad410c6-eb7f-4729-ba68-4f22ec7c7d71" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
  Identity Data | properties | on 9 objects (7 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "209" (IFCTEXT)
  Identity Data | properties | on 7 objects (5 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "221" (IFCTEXT)
  Identity Data | properties | on 6 objects (4 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "210" (IFCTEXT)
  Identity Data | properties | on 5 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "191" (IFCTEXT)
  Identity Data | properties | on 5 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "194" (IFCTEXT)
  Identity Data | properties | on 5 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "202" (IFCTEXT)
  Identity Data | properties | on 5 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "205" (IFCTEXT)
  Identity Data | properties | on 5 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR, 1 IFCWINDOW)
    Mark = "208" (IFCTEXT)
  Identity Data: 900 more contents on 989 objects not shown
  Other | properties | on 433 objects (424 IFCWALLSTANDARDCASE, 9 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall" (IFCLABEL)
    Family and Type = "Basic Wall: Wall-Partn_12P-75Std-12P" (IFCLABEL)
    Type = "Wall-Partn_12P-75Std-12P" (IFCLABEL)
    Type Id = "45422" (IFCLABEL)
  Other | properties | on 246 objects (246 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Phase Id = "0" (IFCLABEL)
  Other | properties | on 205 objects (205 IFCSPACE)
    Category = "Spaces" (IFCLABEL)
    Phase Id = "0" (IFCLABEL)
  Other | properties | on 136 objects (136 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 30mm_Square" (IFCLABEL)
    Host Id = "677081" (IFCLABEL)
    Type = "30mm_Square" (IFCLABEL)
    Type Id = "8490" (IFCLABEL)
  Other | properties | on 136 objects (136 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 30mm_Square" (IFCLABEL)
    Host Id = "677995" (IFCLABEL)
    Type = "30mm_Square" (IFCLABEL)
    Type Id = "8490" (IFCLABEL)
  Other | properties | on 100 objects (87 IFCWALLSTANDARDCASE, 13 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall" (IFCLABEL)
    Family and Type = "Basic Wall: EXT_M-ext-01 (FT FA-02" (IFCLABEL)
    Type = "EXT_M-ext-01 (FT FA-02" (IFCLABEL)
    Type Id = "45417" (IFCLABEL)
  Other | properties | on 90 objects (90 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall" (IFCLABEL)
    Family and Type = "Basic Wall: J- escalier Wall-Int_22" (IFCLABEL)
    Type = "J- escalier Wall-Int_22" (IFCLABEL)
    Type Id = "351346" (IFCLABEL)
  Other | properties | on 85 objects (85 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall" (IFCLABEL)
    Family and Type = "Basic Wall: J- 10 bloc Wall-Partn" (IFCLABEL)
    Type = "J- 10 bloc Wall-Partn" (IFCLABEL)
    Type Id = "341557" (IFCLABEL)
  Other: 1994 more contents on 5599 objects not shown
  Energy Analysis | properties | on 246 objects (246 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Area per Person = 28.571428571428573 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0. (IFCREAL)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 10.763910416709722 (IFCREAL)
    Specified Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 13.993083541722639 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
  Energy Analysis | properties | on 3 objects (3 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 33.333333333333336 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0.08639456485411405 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0.60959999999999981 (IFCREAL)
    Outdoor Air per Person = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Inactive Storage" (IFCLABEL)
    Specified Lighting Load = 9.2994335658030192 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 3.2291731250129163 (IFCREAL)
    Specified Power Load = 9.2994335658030192 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 3.2291731250129163 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 10.000000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 2.5514999999999941 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0. (IFCREAL)
    Outdoor Air per Person = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Stairs - Inactive" (IFCLABEL)
    Specified Lighting Load = 153.79905759811484 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 6.0277898333574447 (IFCREAL)
    Specified Power Load = 54.928234856469594 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 2.1527820833419447 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 33.333333333333336 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0.17424114962120629 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0.60959999999999981 (IFCREAL)
    Outdoor Air per Person = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Inactive Storage" (IFCLABEL)
    Specified Lighting Load = 18.755161254271798 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 3.2291731250129163 (IFCREAL)
    Specified Power Load = 18.755161254271798 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 3.2291731250129163 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 20.000000000000004 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0.14574804354470858 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0.3047999999999999 (IFCREAL)
    Outdoor Air per Person = 2.3597372159999996 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Office - Enclosed" (IFCLABEL)
    Specified Lighting Load = 34.514015450770927 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 11.840301458380695 (IFCREAL)
    Specified Power Load = 47.064566523778531 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 16.145865625064584 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 2. (IFCREAL)
    Area per Person = 10.000000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 2.4763357121760521 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0. (IFCREAL)
    Outdoor Air per Person = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Restrooms" (IFCLABEL)
    Specified Lighting Load = 239.89550190805886 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 9.6875193750387503 (IFCREAL)
    Specified Power Load = 79.965167302686282 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 3.2291731250129163 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 33.333333333333336 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0.12433182274597593 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0.60959999999999981 (IFCREAL)
    Outdoor Air per Person = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Inactive Storage" (IFCLABEL)
    Specified Lighting Load = 13.382966019839172 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 3.2291731250129163 (IFCREAL)
    Specified Power Load = 13.382966019839172 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 3.2291731250129163 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Air Changes per Hour = 0. (IFCREAL)
    Area per Person = 20.000000000000004 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Condition Type = "Heated and cooled" (IFCIDENTIFIER)
    Design Cooling Load = 0. (IFCPOWERMEASURE) [WATT]
    Design Heating Load = 0. (IFCPOWERMEASURE) [WATT]
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.614214034444437 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0.1807436138093157 (IFCREAL)
    Occupancy Unit = "By Space Type" (IFCIDENTIFIER)
    Occupiable = TRUE (IFCBOOLEAN)
    Outdoor Air Information = "From Space Type" (IFCTEXT)
    Outdoor Air Method = "by People and by Area" (IFCIDENTIFIER)
    Outdoor Air per Area = 0.3047999999999999 (IFCREAL)
    Outdoor Air per Person = 2.3597372159999996 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Plenum = FALSE (IFCBOOLEAN)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.267767543055555 (IFCPOWERMEASURE) [WATT]
    Space Type = "Office - Enclosed" (IFCLABEL)
    Specified Lighting Load = 42.801177483588766 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 11.840301458380695 (IFCREAL)
    Specified Power Load = 58.365242023075581 (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 16.145865625064584 (IFCREAL)
    Total Heat Gain per person = 131.88198157749997 (IFCPOWERMEASURE) [WATT]
    Zone = "Default" (IFCTEXT)
  Energy Analysis: 191 more contents on 191 objects not shown
  Phasing | properties | on 6560 objects (2882 IFCMEMBER, 2026 IFCPLATE, 809 IFCWALLSTANDARDCASE, 243 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 451 objects (451 IFCSPACE)
    Phase = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCZONE)
    Phase = "Existing" (IFCLABEL)
  Dimensions | properties | on 416 objects (416 IFCMEMBER)
    Area = 0.42259999999999664 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2.9899999999999758 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.011959999999999903 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 387 objects (387 IFCPLATE)
    Area = 0.27507999999999466 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2.9899999999999758 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.0068769999999999569 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 0.091999999999998944 (IFCLENGTHMEASURE) [METRE]
  Dimensions | properties | on 349 objects (349 IFCMEMBER)
    Area = 0.1449 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2.4000000000000004 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.0021599999999999996 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 295 objects (295 IFCMEMBER)
    Area = 0.46599920764915898 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3.299994340351136 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.013199977361404547 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 276 objects (276 IFCPLATE)
    Area = 0.3035994793123114 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 3.299994340351136 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.0075899869828077119 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 0.092000000000002094 (IFCLENGTHMEASURE) [METRE]
  Dimensions | properties | on 270 objects (270 IFCMEMBER)
    Area = 0.14400000000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1. (IFCLENGTHMEASURE) [METRE]
    Volume = 0.004000000000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 210 objects (210 IFCPLATE)
    Area = 0.091999999999999665 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1. (IFCLENGTHMEASURE) [METRE]
    Volume = 0.0022999999999999319 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 0.091999999999999665 (IFCLENGTHMEASURE) [METRE]
  Dimensions | properties | on 194 objects (194 IFCPLATE)
    Area = 2.4000000007315205 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2.4000000000000004 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.0600000000182878 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1.0000000003048002 (IFCLENGTHMEASURE) [METRE]
  Dimensions: 1881 more contents on 4610 objects not shown
  Constraints | properties | on 2141 objects (1191 IFCMEMBER, 946 IFCPLATE, 4 IFCDOOR)
    Level = "RDC -ANDOY000-AR-AB-100" (IFCLABEL)
  Constraints | properties | on 1547 objects (847 IFCMEMBER, 688 IFCPLATE, 12 IFCDOOR)
    Level = "Etage 1 -ANDOY000-AR-AB-110" (IFCLABEL)
  Constraints | properties | on 1082 objects (760 IFCMEMBER, 321 IFCPLATE, 1 IFCDOOR)
    Level = "Sous sol -1 -ANDOY000-AR-AB-90" (IFCLABEL)
  Constraints | properties | on 183 objects (94 IFCWINDOW, 69 IFCDOOR, 20 IFCOPENINGELEMENT)
    Level = "Etage 1 -ANDOY000-AR-AB-110" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [METRE]
  Constraints | properties | on 173 objects (97 IFCWINDOW, 68 IFCDOOR, 8 IFCOPENINGELEMENT)
    Level = "RDC -ANDOY000-AR-AB-100" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [METRE]
  Constraints | properties | on 140 objects (71 IFCPLATE, 69 IFCMEMBER)
    Level = "Etage 2" (IFCLABEL)
  Constraints | properties | on 129 objects (65 IFCOPENINGELEMENT, 34 IFCWINDOW, 30 IFCDOOR)
    Level = "Etage 2" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [METRE]
  Constraints | properties | on 124 objects (122 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Base Constraint = "RDC -ANDOY000-AR-AB-100" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Up to level: Etage 1 -ANDOY000-AR-AB-110" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 3.3799999999999768 (IFCLENGTHMEASURE) [METRE]
  Constraints: 157 more contents on 1508 objects not shown
  Structural | properties | on 995 objects (809 IFCWALLSTANDARDCASE, 160 IFCCURTAINWALL, 23 IFCWALL, 3 IFCOPENINGELEMENT)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 27 objects (27 IFCCOLUMN)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover 1 <25 mm>" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover 1 <25 mm>" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover 1 <25 mm>" (IFCLABEL)
  Structural | properties | on 11 objects (11 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 1 object (1 IFCCOLUMN)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover 1 <25 mm>" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover 1 <25 mm>" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover 1 <25 mm>" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
  Structural | properties | on 17 type objects
    Section Shape = 0 (IFCINTEGER)
  Structural | properties | on 1 type object
    Section Shape = 8 (IFCINTEGER)
  Cross-Section Definition | properties | on 989 objects (804 IFCWALLSTANDARDCASE, 160 IFCCURTAINWALL, 22 IFCWALL, 3 IFCOPENINGELEMENT)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
  Cross-Section Definition | properties | on 6 objects (5 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Angle From Vertical = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Cross-Section = "Slanted" (IFCIDENTIFIER)
  Text | properties | on 90 objects (52 IFCWINDOW, 26 IFCOPENINGELEMENT, 8 IFCDOOR, 4 IFCWALLSTANDARDCASE)
    Orientation- Element = "SO" (IFCTEXT)
  Text | properties | on 74 objects (55 IFCWINDOW, 15 IFCCURTAINWALL, 2 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT)
    Orientation- Element = "N" (IFCTEXT)
  Text | properties | on 69 objects (55 IFCWINDOW, 10 IFCWALLSTANDARDCASE, 3 IFCWALL, 1 IFCDOOR)
    Orientation- Element = "NE" (IFCTEXT)
  Text | properties | on 43 objects (31 IFCWINDOW, 11 IFCWALLSTANDARDCASE, 1 IFCCURTAINWALL)
    Orientation- Element = "S" (IFCTEXT)
  Text | properties | on 23 objects (19 IFCWINDOW, 2 IFCOPENINGELEMENT, 1 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Orientation- Element = "O" (IFCTEXT)
  Text | properties | on 23 objects (16 IFCWINDOW, 4 IFCCURTAINWALL, 1 IFCOPENINGELEMENT, 1 IFCWALL)
    Orientation- Element = "E" (IFCTEXT)
  Construction | properties | on 7 objects (7 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
    Extend Below Riser Base = 0. (IFCLENGTHMEASURE) [METRE]
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [METRE]
    Maximum Ridge Height = 10.551997471673735 (IFCLENGTHMEASURE) [METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [METRE]
    Maximum Ridge Height = 7.2869918120248443 (IFCLENGTHMEASURE) [METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [METRE]
    Maximum Ridge Height = 7.0669918120248507 (IFCLENGTHMEASURE) [METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [METRE]
    Maximum Ridge Height = 0.40699747167373579 (IFCLENGTHMEASURE) [METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 21 type objects
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 3 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 3 type objects
    Wall Closure = "By host" (IFCIDENTIFIER)
    Wrap Layers (Ext) from Ext = 0.10249999999999999 (IFCLENGTHMEASURE) [METRE]
    Wrap Layers (Int) from Ext = 0.17750000000000002 (IFCLENGTHMEASURE) [METRE]
  Construction: 22 more contents on 0 objects not shown
  Horizontal Grid | properties | on 91 objects (90 IFCCURTAINWALL, 1 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Horizontal Grid | properties | on 68 objects (66 IFCCURTAINWALL, 2 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 1 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 3 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Horizontal Grid | properties | on 2 type objects
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 1. (IFCLENGTHMEASURE) [METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 2.4000000000000004 (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 28 objects (27 IFCCURTAINWALL, 1 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 1 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 18 objects (17 IFCCURTAINWALL, 1 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 12 objects (12 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 3 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 12 objects (12 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 11 objects (11 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 20 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 11 objects (11 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 15 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 11 objects (11 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 18 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid | properties | on 10 objects (10 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 19 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [METRE]
  Vertical Grid: 17 more contents on 50 objects not shown
  Materials and Finishes | properties | on 27 objects (27 IFCCOLUMN)
    Structural Material = "Concrete - Cast-in-Place Concrete" (IFCLABEL)
  Materials and Finishes | properties | on 17 objects (16 IFCWINDOW, 1 IFCOPENINGELEMENT)
    U fenêtre = "J-Glass λU=0.91" (IFCLABEL)
  Materials and Finishes | properties | on 1 object (1 IFCCOLUMN)
    Structural Material = "Metal - Steel 43-275" (IFCLABEL)
  Materials and Finishes | properties | on 16 type objects
    Material Architrave = "Door - Architrave" (IFCLABEL)
    Material Door = "Door - Panel" (IFCLABEL)
    Material Frame = "Door - Frame/Mullion (1)" (IFCLABEL)
    Material Ironmongery = "Door - Handle" (IFCLABEL)
  Materials and Finishes | properties | on 8 type objects
    Structural Material = "Concrete Masonry Units _High Density" (IFCLABEL)
  Materials and Finishes | properties | on 3 type objects
    Material Frame = "Window Frame" (IFCLABEL)
    Material Glass = "J-Glass λU=0.91" (IFCLABEL)
    Material Trim = "Window Frame" (IFCLABEL)
  Materials and Finishes | properties | on 3 type objects
    Structural Material = "J-Béton lourd normal armé (Eléments de construction pierreux sans joints)- Plancher" (IFCLABEL)
  Materials and Finishes | properties | on 2 type objects
    Structural Material = "Air Infiltration Barrier" (IFCLABEL)
  Materials and Finishes: 5 more contents on 0 objects not shown
  Electrical - Loads | properties | on 205 objects (205 IFCSPACE)
    Design HVAC Load per area = 0. (IFCREAL)
    Design Other Load per area = 0. (IFCREAL)
  Electrical - Loads | properties | on 6 objects (3 IFCBUILDINGELEMENTPROXY, 3 IFCOPENINGELEMENT)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCRAMP)
    Down label = TRUE (IFCBOOLEAN)
    Down text = "DN" (IFCTEXT)
    Show Up arrow in all views = FALSE (IFCBOOLEAN)
    Up label = TRUE (IFCBOOLEAN)
    Up text = "UP" (IFCTEXT)
  Graphics | properties | on 16 type objects
    Vis - Ironmongery = TRUE (IFCBOOLEAN)
  Graphics | properties | on 15 type objects
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "<Solid fill>" (IFCLABEL)
  Graphics | properties | on 6 type objects
    Coarse Scale Fill Color = 11447982 (IFCINTEGER)
    Coarse Scale Fill Pattern = "<Solid fill>" (IFCLABEL)
  Graphics | properties | on 3 type objects
    Vis - Cavity Closers = TRUE (IFCBOOLEAN)
  Graphics | properties | on 2 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Mechanical - Flow | properties | on 15 objects (15 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 3 objects (3 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 1.7555375578355974 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 2 objects (2 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 3.5405801603029117 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 2 objects (2 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 1.2324071559601808 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 2 objects (2 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 2.5264226381982304 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 2 objects (2 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 1.528320501841762 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 35.862728101044262 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Actual Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Outdoor Airflow = 31.527562302460215 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Airflow = "Specified" (IFCIDENTIFIER)
    Specified Exhaust Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Return Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Specified Supply Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow: 177 more contents on 177 objects not shown
  Electrical - Lighting | properties | on 205 objects (205 IFCSPACE)
    Average Estimated Illumination = 0. (IFCILLUMINANCEMEASURE) [LUX]
    Ceiling Reflectance = 75. (IFCREAL)
    Floor Reflectance = 20. (IFCREAL)
    Lighting Calculation Workplane = 0.76200000000000001 (IFCLENGTHMEASURE) [METRE]
    Room Cavity Ratio = 0. (IFCREAL)
    Wall Reflectance = 50. (IFCREAL)
  Supports(Type) | properties | on 7 objects (7 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Left Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Left Support Type = "Stringer-50mm_Width" (IFCLABEL)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Right Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Right Support Type = "Stringer-50mm_Width" (IFCLABEL)
  Calculation Rules(Type) | properties | on 7 objects (7 IFCSTAIR)
    Maximum Riser Height = 0.17000000000000001 (IFCLENGTHMEASURE) [METRE]
    Minimum Run Width = 0.99999999999999989 (IFCLENGTHMEASURE) [METRE]
    Minimum Tread Depth = 0.25 (IFCLENGTHMEASURE) [METRE]
  Graphics(Type) | properties | on 16 objects (16 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle : Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 7 objects (7 IFCSTAIR)
    Cut Mark Type = "Sgl Zigzag" (IFCLABEL)
  Graphics(Type) | properties | on 3 objects (3 IFCRAMP)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 2.5 (IFCREAL)
  Graphics(Type) | properties | on 1 object (1 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics(Type) | properties | on 16 type objects
    Vis - Ironmongery = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 4 type objects
    Vis - Cavity Closers = TRUE (IFCBOOLEAN)
  Construction(Type) | properties | on 13 objects (13 IFCRAILING)
    Angled Joins = "Add Vertical/Horizontal Segments" (IFCIDENTIFIER)
    Baluster Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Landing Height Adjustment = 0. (IFCLENGTHMEASURE) [METRE]
    Rail Connections = "Trim" (IFCIDENTIFIER)
    Railing Height = 1.1000000000000001 (IFCLENGTHMEASURE) [METRE]
    Tangent Joins = "Extend Rails to Meet" (IFCIDENTIFIER)
    Use Landing Height Adjustment = FALSE (IFCBOOLEAN)
  Construction(Type) | properties | on 7 objects (7 IFCSTAIR)
    Function = "Interior" (IFCIDENTIFIER)
    Landing Type = "Non-Monolitic_Landing" (IFCLABEL)
    Run Type = "Wood_Steps_w-50mm_Tread-10mm_Nosing-13mm_Riser" (IFCLABEL)
  Construction(Type) | properties | on 3 objects (3 IFCRAMP)
    Function = "Interior" (IFCIDENTIFIER)
    Shape = "Solid" (IFCIDENTIFIER)
    Thickness = 0.14999999999999997 (IFCLENGTHMEASURE) [METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 0.56500000000000006 (IFCLENGTHMEASURE) [METRE]
  Construction(Type) | properties | on 19 type objects
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction(Type) | properties | on 4 type objects
    Wall Closure = "By host" (IFCIDENTIFIER)
    Wrap Layers (Ext) from Ext = 0.10249999999999999 (IFCLENGTHMEASURE) [METRE]
    Wrap Layers (Int) from Ext = 0.17750000000000002 (IFCLENGTHMEASURE) [METRE]
  Identity Data(Type) | properties | on 16 objects (16 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data(Type) | properties | on 15 objects (15 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Stringer-50mm_Width" (IFCTEXT)
  Identity Data(Type) | properties | on 13 objects (13 IFCRAILING)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "1100mm" (IFCTEXT)
  Identity Data(Type) | properties | on 7 objects (7 IFCSTAIR)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Private" (IFCTEXT)
  Identity Data(Type) | properties | on 3 objects (3 IFCRAMP)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Standard" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "EXT_Toiture atrium_T-ext-02" (IFCTEXT)
  Identity Data(Type) | properties | on 16 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Internal Single Door" (IFCTEXT)
    Keynote = "L20" (IFCTEXT)
    Manufacturer = "Revit" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "Internal Single" (IFCTEXT)
    Type Mark = "46" (IFCTEXT)
    Type Name = "J-1000x2110mm 2" (IFCTEXT)
  Identity Data(Type) | properties | on 2 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Mark = "64" (IFCTEXT)
    Type Name = "1200 x 2100 mm" (IFCTEXT)
  Identity Data(Type): 4 more contents on 0 objects not shown
  Other(Type) | properties | on 16 objects (16 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 15 objects (15 IFCMEMBER)
    Category = "Stairs: Supports" (IFCLABEL)
    Family Name = "Stringer" (IFCTEXT)
  Other(Type) | properties | on 13 objects (13 IFCRAILING)
    Category = "Railings" (IFCLABEL)
    Family Name = "Railing" (IFCTEXT)
  Other(Type) | properties | on 7 objects (7 IFCSTAIR)
    Category = "Stairs" (IFCLABEL)
    Family Name = "Assembled Stair" (IFCTEXT)
  Other(Type) | properties | on 3 objects (3 IFCRAMP)
    Category = "Ramps" (IFCLABEL)
    Family Name = "Ramp" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family Name = "Basic Roof" (IFCTEXT)
  Other(Type) | properties | on 16 type objects
    Category = "Doors" (IFCLABEL)
    Family Name = "Doors_IntSgl" (IFCTEXT)
    Frame Thickness = 0.032000000000000001 (IFCLENGTHMEASURE) [METRE]
  Other(Type) | properties | on 4 type objects
    Category = "Windows" (IFCLABEL)
    Default Head Height = 2.1099999999999999 (IFCLENGTHMEASURE) [METRE]
    Family Name = "Windows_Sgl_Plain" (IFCTEXT)
  Other(Type): 3 more contents on 0 objects not shown
  Dimensions(Type) | properties | on 15 objects (15 IFCMEMBER)
    Flip Section Profile = FALSE (IFCBOOLEAN)
    Structural Depth On Landing = 0.30756349186104037 (IFCLENGTHMEASURE) [METRE]
    Structural Depth On Run = 0.15199999999999997 (IFCLENGTHMEASURE) [METRE]
    Total Depth = 0.40000000000000002 (IFCLENGTHMEASURE) [METRE]
    Width = 0.050000000000000003 (IFCLENGTHMEASURE) [METRE]
  Dimensions(Type) | properties | on 3 objects (3 IFCRAMP)
    Maximum Incline Length = 11.999999999999998 (IFCLENGTHMEASURE) [METRE]
    Ramp Max Slope (1/x) = 12. (IFCREAL)
  Dimensions(Type) | properties | on 16 type objects
    Architrave Setback = 0.0050000000000000001 (IFCLENGTHMEASURE) [METRE]
    Door Panel Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Door Panel Thickness = 0.037999999999999999 (IFCLENGTHMEASURE) [METRE]
    Handle X Distance = 0.075000000000000011 (IFCLENGTHMEASURE) [METRE]
    Handle Z Distance = 1. (IFCLENGTHMEASURE) [METRE]
    Height = 2.1099999999999999 (IFCLENGTHMEASURE) [METRE]
    Height to Top Lock Rail = 1. (IFCLENGTHMEASURE) [METRE]
    Rough Height = 2.1099999999999999 (IFCLENGTHMEASURE) [METRE]
    Rough Width = 1. (IFCLENGTHMEASURE) [METRE]
    Stop Thickness = 0.019 (IFCLENGTHMEASURE) [METRE]
    StopDepth = 0.032000000000000001 (IFCLENGTHMEASURE) [METRE]
    Structural Tolerance = 0.0080000000000000002 (IFCLENGTHMEASURE) [METRE]
    Thickness = 0.037999999999999999 (IFCLENGTHMEASURE) [METRE]
    Tolerance = 0.002 (IFCLENGTHMEASURE) [METRE]
    UnderCut = 0.0080000000000000002 (IFCLENGTHMEASURE) [METRE]
    Width = 1. (IFCLENGTHMEASURE) [METRE]
  Dimensions(Type) | properties | on 2 type objects
    Height = 2.1000000000000001 (IFCLENGTHMEASURE) [METRE]
    Width = 1.1999999999999997 (IFCLENGTHMEASURE) [METRE]
  Dimensions(Type) | properties | on 2 type objects
    Cavity Closer Depth = 0.085000000000000006 (IFCLENGTHMEASURE) [METRE]
    Cavity Closer Offset from Ext = 0.10249999999999999 (IFCLENGTHMEASURE) [METRE]
    Cavity Closer Width = 0.050000000000000003 (IFCLENGTHMEASURE) [METRE]
    Cill Depth = 0.087500000000000008 (IFCLENGTHMEASURE) [METRE]
    Frame Depth = 0.065000000000000002 (IFCLENGTHMEASURE) [METRE]
    FrameOffset - External = 0.050000000000000003 (IFCLENGTHMEASURE) [METRE]
    Glazing Thickness = 0.024 (IFCLENGTHMEASURE) [METRE]
    Height = 2.8050000000000002 (IFCLENGTHMEASURE) [METRE]
    Rough Height = 2.8050000000000002 (IFCLENGTHMEASURE) [METRE]
    Rough Width = 1.2699999999999998 (IFCLENGTHMEASURE) [METRE]
    Width = 1.2699999999999998 (IFCLENGTHMEASURE) [METRE]
    Window Board Extension = 0.025000000000000001 (IFCLENGTHMEASURE) [METRE]
    Window Board Projection = 0.025000000000000001 (IFCLENGTHMEASURE) [METRE]
  Dimensions(Type) | properties | on 2 type objects
    Cavity Closer Depth = 0.085000000000000006 (IFCLENGTHMEASURE) [METRE]
    Cavity Closer Offset from Ext = 0.10249999999999999 (IFCLENGTHMEASURE) [METRE]
    Cavity Closer Width = 0.050000000000000003 (IFCLENGTHMEASURE) [METRE]
    Cill Depth = 0.087500000000000008 (IFCLENGTHMEASURE) [METRE]
    Frame Depth = 0.065000000000000002 (IFCLENGTHMEASURE) [METRE]
    FrameOffset - External = 0.050000000000000003 (IFCLENGTHMEASURE) [METRE]
    Glazing Thickness = 0.024 (IFCLENGTHMEASURE) [METRE]
    Height = 2.8050000000000002 (IFCLENGTHMEASURE) [METRE]
    Rough Height = 2.8050000000000002 (IFCLENGTHMEASURE) [METRE]
    Rough Width = 0.81999999999999984 (IFCLENGTHMEASURE) [METRE]
    Width = 0.81999999999999984 (IFCLENGTHMEASURE) [METRE]
    Window Board Extension = 0.025000000000000001 (IFCLENGTHMEASURE) [METRE]
    Window Board Projection = 0.025000000000000001 (IFCLENGTHMEASURE) [METRE]
  Dimensions(Type) | properties | on 1 type object
    Height = 2. (IFCLENGTHMEASURE) [METRE]
    Width = 0.90000000000000002 (IFCLENGTHMEASURE) [METRE]
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.1118113527127946 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 561.41399999999999 (IFCREAL)
    Thermal Resistance (R) = 8.9436356482392299 (IFCREAL)
  Analytical Properties(Type) | properties | on 19 type objects
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Analytical Properties(Type) | properties | on 4 type objects
    Analytic Construction = "Large single-glazed windows" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 0.91000000000000003 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Solar Heat Gain Coefficient = 0.85999999999999999 (IFCREAL)
    Thermal Resistance (R) = 1.0989010989010988 (IFCREAL)
    Visual Light Transmittance = 0.90000000000000002 (IFCREAL)
  Handrail 2(Type) | properties | on 13 objects (13 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Handrail 1(Type) | properties | on 13 objects (13 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Top Rail(Type) | properties | on 13 objects (13 IFCRAILING)
    Height = 1.1000000000000001 (IFCLENGTHMEASURE) [METRE]
    Type = "50x50mm_Rectangular" (IFCLABEL)
    Use Top Rail = TRUE (IFCBOOLEAN)
  Constraints(Type) | properties | on 16 objects (16 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 16 type objects
    Door Panel Height = 2.0599999999999996 (IFCLENGTHMEASURE) [METRE]
    Door Panel Width = 0.91599999999999993 (IFCLENGTHMEASURE) [METRE]
  Constraints(Type) | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [METRE]
  Analytical Properties | properties | on 22 type objects
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Analytical Properties | properties | on 3 type objects
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "User Defined" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 1. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Thermal Resistance (R) = 1. (IFCREAL)
  Analytical Properties | properties | on 3 type objects
    Analytic Construction = "Large single-glazed windows" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 0.91000000000000003 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Solar Heat Gain Coefficient = 0.85999999999999999 (IFCREAL)
    Thermal Resistance (R) = 1.0989010989010988 (IFCREAL)
    Visual Light Transmittance = 0.90000000000000002 (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.14303543632819618 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 271.49219999999997 (IFCREAL)
    Thermal Resistance (R) = 6.9912745098039224 (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 3.2745591939546603 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 534.17999999999995 (IFCREAL)
    Thermal Resistance (R) = 0.30538461538461537 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.244934714092751 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 457.55624999999981 (IFCREAL)
    Thermal Resistance (R) = 4.0827205882352944 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.11639854744370419 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 589.72099999999989 (IFCREAL)
    Thermal Resistance (R) = 8.5911725013892202 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.69999999999999996 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.78947368421052622 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 108.63000000000001 (IFCREAL)
    Thermal Resistance (R) = 1.2666666666666668 (IFCREAL)
  Analytical Properties: 16 more contents on 0 objects not shown
  Pset_ElementShading | properties | on 23 type objects
    Roughness = 0.9144000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Sliding Door - 4 Panel (AUS):Type 1:839914 | predefined | on 1 type object
  Sliding Door - 4 Panel (AUS):Type 1:839914:1 | predefined | on 1 type object
  Structural Section Geometry | properties | on 1 type object
    Centroid Horizontal = 0.15265000000000001 (IFCLENGTHMEASURE) [METRE]
    Centroid Vertical = 0.15395 (IFCLENGTHMEASURE) [METRE]
    Flange Thickness = 0.015400000000000002 (IFCLENGTHMEASURE) [METRE]
    Height = 0.30790000000000001 (IFCLENGTHMEASURE) [METRE]
    Web Fillet = 0.0152 (IFCLENGTHMEASURE) [METRE]
    Web Thickness = 0.0098999999999999991 (IFCLENGTHMEASURE) [METRE]
    Width = 0.30530000000000002 (IFCLENGTHMEASURE) [METRE]
  Structural Analysis | properties | on 1 type object
    Elastic Modulus strong axis = 0.0014450000000000003 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Elastic Modulus weak axis = 0.0004790000000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Moment of Inertia strong axis = 0.00022249000000000005 (IFCMOMENTOFINERTIAMEASURE) [derived]
    Moment of Inertia weak axis = 7.3080000000000012E-05 (IFCMOMENTOFINERTIAMEASURE) [derived]
    Nominal Weight = 96.899640329776233 (IFCREAL)
    Plastic Modulus strong axis = 0.0015920000000000003 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Plastic Modulus weak axis = 0.00072600000000000019 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Section Area = 0.0123 (IFCAREAMEASURE) [SQUARE_METRE]
    Torsional Moment of Inertia = 9.1200000000000023E-07 (IFCMOMENTOFINERTIAMEASURE) [derived]
    Warping Constant = 1560000. (IFCREAL)
  Materials and Finishes(Type) | properties | on 16 type objects
    Material Architrave = "Door - Architrave" (IFCLABEL)
    Material Door = "Door - Panel" (IFCLABEL)
    Material Frame = "Door - Frame/Mullion (1)" (IFCLABEL)
    Material Ironmongery = "Door - Handle" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 4 type objects
    Material Frame = "Window Frame" (IFCLABEL)
    Material Glass = "J-Glass λU=0.91" (IFCLABEL)
    Material Trim = "Window Frame" (IFCLABEL)
  Doors_IntSgl:J-1000x2110mm 2:360136 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:360136:1 | predefined | on 1 type object
  Pset_ManufacturerTypeInformation | properties | on 39 type objects
    Manufacturer = "Revit" (IFCLABEL)
  Doors_IntSgl:J-900x2110mm 3:705272 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:705272:1 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:361908 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:361908:1 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:362165 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:362165:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:408853 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:408853:1 | predefined | on 1 type object
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
    Interior Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
  Vertical Mullions | properties | on 2 type objects
    Interior Type = "Rectangular Mullion : 64 x 128 rectangular" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
    Interior Type = "Rectangular Mullion : 30mm_Square" (IFCLABEL)
  Doors_IntSgl:J-900x2110mm 3:361187 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:361187:1 | predefined | on 1 type object
  Siliding:1200 x 2100 mm:538230 | predefined | on 1 type object
  Siliding:1200 x 2100 mm:538230:1 | predefined | on 1 type object
  Siliding:1200 x 2100 mm:538311 | predefined | on 1 type object
  Siliding:1200 x 2100 mm:538311:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:706919 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:706919:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605512 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605512:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:707010 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:707010:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605566 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605566:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:657147 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:657147:1 | predefined | on 1 type object
  Double-Standard Frame w Glass:1770 x 2500:671404 | predefined | on 1 type object
  Double-Standard Frame w Glass:1770 x 2500:671404:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:601789 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:601789:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:747142 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:747142:1 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:747468 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:747468:1 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:605561 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:605561:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605563 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605563:1 | predefined | on 1 type object
  Doors_IntSgl:J-1400x2110mm:750830 | predefined | on 1 type object
  Doors_IntSgl:J-1400x2110mm:750830:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:753189 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:753189:1 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 2000x910mm 3:755806 | predefined | on 1 type object
  Double-Standard Frame-Variable:J-1800 x 2000:756339 | predefined | on 1 type object
  Double-Standard Frame-Variable:J-1800 x 2000:756339:1 | predefined | on 1 type object
  Double-Standard Frame w Glass:2060 x 2500:767743 | predefined | on 1 type object
  Double-Standard Frame w Glass:2060 x 2500:767743:1 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 900x910mm 2:362666 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:775181 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:775181:1 | predefined | on 1 type object
  Double-Standard Frame-Variable:J-1800 x 2000:775819 | predefined | on 1 type object
  Double-Standard Frame-Variable:J-1800 x 2000:775819:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:776307 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:776307:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:359217 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:359217:1 | predefined | on 1 type object
  Doors_IntSgl:J-920x2110mm 3:360002 | predefined | on 1 type object
  Doors_IntSgl:J-920x2110mm 3:360002:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:360536 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:360536:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:360730 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:360730:1 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 900x910mm 2:367281 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:361531 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:361531:1 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 1270x910mm 2:544925 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 820x910mm:543183 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605511 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:605511:1 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:605558 | predefined | on 1 type object
  Doors_IntSgl:J-640x2000mm 4:605558:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:361128 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:361128:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:661137 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:661137:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:661338 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:661338:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:664350 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:664350:1 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 1270x910mm 2:665502 | predefined | on 1 type object
  Windows_Sgl_Plain:J- 820x910mm:670554 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:670720 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:670720:1 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:671480 | predefined | on 1 type object
  Siliding:1800 x 2100 mm:671480:1 | predefined | on 1 type object
  Double-Standard Frame w Glass:1770 x 2500:671481 | predefined | on 1 type object
  Double-Standard Frame w Glass:1770 x 2500:671481:1 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:361081 | predefined | on 1 type object
  Doors_IntSgl:J-900x2110mm 3:361081:1 | predefined | on 1 type object
  Single-Narrow Frame w Glass:900 x 2000:413108 | predefined | on 1 type object
  Single-Narrow Frame w Glass:900 x 2000:413108:1 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:434419 | predefined | on 1 type object
  Doors_IntSgl:J-1000x2110mm 2:434419:1 | predefined | on 1 type object